......DE....FRGB..IT..............................
B
0098626
EUROPEAN PATENT APPLICATION
A1
19840118
EP
83200781.9
19830602
nl
en
en
8202285
19820607
NL
19840118
198403
19840118
198403
3
3H 05K 1/03 A
3H 05K 1/18 B
de
Gedruckte Leiterplatte enthaltende elektrische Schaltungsanordnung
en
Electric circuit assembly comprising a printed wiring board
fr
Agencement de circuit électrique comportant un circuit imprimé
Philips Electronics N.V.
00200769
PHN 10. 373 EP
Groenewoudseweg 1
5621 BA Eindhoven
NL
van der Wijst, Hendricus Martinus
c/o INT. OCTROOIBUREAU B.V. Prof. Holstlaan 6
NL-5656 AA Eindhoven
NL
Koppen, Jan
et al
00020421
INTERNATIONAAL OCTROOIBUREAU B.V., Prof. Holstlaan 6
5656 AA Eindhoven
NL
DE
FR
GB
IT
A supporting plate (1) having a network of conductors (5), on which supporting plate a number of circuit components (7-9) are placed which are interconnected in the network of conductors in an electric circuit comprises, in a place of the circuit which is sensitive to moisture, an interruption (2) in which a member (3) of a minimum moisture- absorbing material is provided. The connections of the surrounding circuit components extend in an aperture of the member (3) and are electrically interconnected there. The stability of the circuit is considerably improved thereby in particular in the case in which the circuit is an oscillator circuit.
The invention relates to an electric circuit assembly comprising a network of printed circuit conductors on a printed wiring board and a number of circuit components which are interconnected through the conductors.
It is known to provide printed circuits or conductors on printed circuit boards, to insert circuit components into holes in the boards, and to connect the various parts of the circuit at the connection places, for example by soldering, in particular by immersing in a solder bath. The material of the printed circuit boards is usually a glass fibre-reinforced polyester resin which satisfies the imposed requirements as regards thickness and rigidity.
It has been found that the properties of the electric circuits built up in the above-described manner can vary when the moisture content of the ambient air varies. This relates in particular to variations in the oscillator frequency of oscillator circuits, for example, those present in, for example, U.H.F. tuners. The most critical point proves to be the top of the oscillator resonant circuit. It has been found that the stray capacitance of the printed circuit board at this point varies under the influence of moisture and causes variations in the oscillator frequency.
The invention provides a particularly simple and effective solution to reduce this problem.
For that purpose, an electric circuit assembly of the type described in the opening paragraph is characterized in that the printed wiring board has an opening in which an apertured member of an electrically insulating moisture impermeable material is fitted, and that a number of circuit components are electrically interconnected by connections disposed in the aperture of the member.
Providing an apertured member (for example a small ring) of a moisture impermeable material (synthetic resins, for example polytetrafluoroethylene, are very suitable for this purpose) in printed wiring boards and inserting into the aperture and soldering together the connections of certain circuit components has for its result that the stray capacitance in that place in the circuit varies considerably less under the influence of varying moisture contents of the ambience. In the case of an oscillator circuit the oscillation frequency thus varies much less, in a given case 70% less.
An embodiment of the device according to the invention will be described in greater detail with reference to the drawing, in which :
- Figure 1 is a plan view of a printed circuit assembly comprising a printed wiring board;
- Figure 2 is a cross-sectional view through the printed wiring board of Figure 1 taken on the line II-II, and
- Figure 3 shows a circuit diagram of an oscillator circuit.
A supporting plate 1 (printed wiring board) of electrically insulating material has an opening 2. A body 3 of a moisture impermeable material which can withstand the soldering temperature, for example polytetrafluoroethylene, is pressed into said opening 2. Member 3, the shape of which is not critical - it may, for example, be square - but which for practical reasons is shown as a ring in the drawing, has an aperture 4. Supporting plate 1 has a network of conductors 5, for example, of (etched out) copper. A number of circuit components, inter alia a transistor 6, a varicap diode 7 and two inductors 8, 9, are interconnected through network of conductors 5. The components 6, 7, 8, 9 have connections extending in the aperture 4 of the member 3 and are electrically interconnected there. The variations of the oscillation frequency of the oscillator circuit of which these components form part (see Figure 3) prove to be-considerably less in a test, in a given case 70% less, than the variations of the oscillator frequency of the same circuit but provided on a supporting plate without an opening, in which at the location of the member 3 a portion of the network of conductors was present to which the connections of the components 6, 7, 8, 9 were soldered.
Providing a moisture impermeable member into a printed wiring board presents advantages not only in oscillator circuits but also in non-oscillator circuits which have a moisture-sensitive place. An advantage not yet mentioned is that by providing such a member in a critical place in the printed wiring board the supporting plate may without any objections b'e manufactured from a material which does not satisfy the requirement of moisture impermeability, for example, a paper-based laminate. Without the invention it would be necessary to manufacture the complete supporting plate from a moisture impermeable material in order to obtain a comparable effect, which has a cost price-increasing effect.
1. An electric circuit assembly comprising a network of printed circuit conductors on a printed wiring board and a number of circuit components which are interconnected through the conductors, characterized in that the printed wiring board has an opening in which an apertured member of an electrically insulating moisture impermeable material is fitted, and that a number of circuit components are electrically interconnected by connections disposed in the aperture of the member.
2. An assembly as claimed in Claim 1, characterized in that the member is formed from a minimum moisture- absorbing, solder-resistant synthetic resin.
3. An assembly as claimed in Claim 2, characterized in that the synthetic resin is polytetrafluoroethylene.
4. An assembly as claimed in Claim 1, 2 or 3, characterized in that the electric circuit is an oscillator circuit.
5. An assembly as claimed in Claim 4, characterized in that the oscillator circuit comprises a transistor, a varicap diode and two inductors, the collector connection of the transistor and the connections of the varicap diode and the inductors extending in the aperture of the member and being electrically interconnected.
6. A printed wiring board having an opening in which an apertured moisture impermeable member is fitted for an assembly as claimed in any of the Claims 1 to 5.