......DE....FRGB........NL........................
J
The file contains technical information submitted after the application was filed and not included in this specification
0201038
NEW EUROPEAN PATENT SPECIFICATION
B2
19960124
EP
86105951.7
19860430
19870422
19890330
19960124
en
en
en
92437/85
19850430
JP
92438/85
19850430
JP
19960124
199604
19861112
198646
19900718
199029
19891108
19960124
199604
6
6H 01M 10/40 A
de
Sekundärbatterie mit nichtwässrigem Lösungsmittel
en
Secondary battery using non-aqueous solvent
fr
Batterie secondaire à solvant non aqueux
EP-A- 149 497
EP-A- 175 373
EP-A- 0 092 713
EP-A- 0 165 047
DE-A- 3 231 243
JP-A- 5 835 881
JP-A- 5 893 176
JP-A- 5 946 760
JP-A- 6 054 181
JP-A-59 154 763
Journal of the Electrochemical Society, vol.131, no. 12, 1984, S. 2744-2750
Plastics & Polymers Conference Supplement No. 5, pp. 18-22
Bulletin of the Government Industrial Research Institute, Osaka, vol. 12, no. 2, 1961, pp. 110-118
"Lithium Batteries" edited by J.-P. Gabano (1983), pp. 169-406
Report of the Government Industrial Research Institute, Osaka, No. 317, 1961
Synthetic Metals, 18 (1987), pp. 537-542
Kiki Bunseki Jikken Ho, Japan, 1974
Bulletin of the Chemical Society of Japan, Vol. 46, No. 8, 1973, pp. 2575-78
Webster's Third New International Dictionary, pp. 88, 353
Handbook of Batteries and Fuel Cells, 1984, Definitions A3-A5
Carbon, Vol. 19, No. 6, pp. 457-465, 1981
Journal of Materials Science, 21 (1986), pp. 4443-4450
Journal of Materials Science, 25 (1990), pp. 4873-4879
Journal of the Electrochemical Society, Vol. 127, No. 11 (1980), pp. 2315-2319
Advanced Carbon Series 1, "Tanso Seni no Tenkai to Hyoka Hoho" by Jun-ichi Matsui, edited by the Society of Carbon Materials, Japan 1989
Extended Abstracts of the 40th ISE Meeting, Kyoto, Japan, Vol. 1, 1989
Proceedings of "Advanced Composite Materials and Structures", May 19-23, 1986, VNU Science Press, 1987, pp 196-210
SEN-I GAKKAISHI, Vol. 23, No. 7 (1967), pp. 342-347
Journal of Material Science 22 (1987), pp. 218-300
Chemistry and Physics of Carbon, Vol. 11 (1973), pp. 9-16
Journal of the Elextrochemical Society, vol. 131, no. 4 (1984), pp. 959-960
Tanso Zairyo Nyumon, Japan 1972, pp. 155-157
19860915
Hiratsuka, Kazuya
102, Hikari-Corpo 72-7, Yayoidai
Totsuka-ku Yokohama-shi Kanagawa-ken
JP
Sato, Yuichi
4-18-13, Tobio Atsugi-shi
Kanagawa-ken
JP
Aoki, Yoshiyasu
705, Neo-Corpo-Oojima 7-30-26, Oojima
Koto-ku Tokyo
JP
Yui, Hiroshi Plastic Laboratory
Mitsubishi Petrochemical Co. Ltd. 1, Touhou-cho
Yokkaichi-shi Mie-ken
JP
Miyabayashi, Mitsutaka Plastic Laboratory
Mitsubishi Petrochemical Co. Ltd. 1, Touhou-cho
Yokkaichi-shi Mie-ken
JP
Itsubo, Akira Plastic Laboratory
Mitsubishi Petrochemical Co. Ltd. 1, Touhou-cho
Yokkaichi-shi Mie-ken
JP
TOSHIBA BATTERY CO., LTD.
00585540
4-10, Minamishinagawa 3-chome Shinagawa-ku
Tokyo, 104
JP
MITSUBISHI PETROCHEMICAL CO., LTD.
00471870
PETROCHEMICAL CO., LTD., MITSUBISHI
5-2, 2-chome, Marunouchi
Chiyoda-ku Tokyo 100
JP
Hoffmann, Klaus, Dr. rer. nat.
et al
00005582
Hoffmann, Eitle & Partner Patentanwälte Postfach 81 04 20
D-81904 München
DE
01
19910618
1
Asahi Chemical Industry Co., Ltd.
00009040
2-6, Dojima-hama, 1-chome, Kita-ku
Osaka
JP
Strehl, Peter, Dipl.-Ing.
00011662
Patentanwälte Strehl Schübel-Hopf Groening u. Partner Postfach 22 14 55
D-80504 München
DE
02
19910618
1
Karl Lebling Ingenieurbüro
00045970
Seybothstr. 20
8000 München 90
DE
Spott, Gottfried, Dr.
00011331
Sendlinger-Tor-Platz 11
D-80336 München
DE
DE
FR
GB
NL
19861112
198646

BACKGROUND OF THE INVENTION
The present invention relates to a secondary battery using a non-aqueous solvent, more particularly to a secondary battery using a non-aqueous solvent which is less in self-discharge, has good charge/discharge cycle characteristics and is excellent in storability.
In recent years, as secondary batteries which are compact and lightweight and have high energy densities, those which use a kind of a conductive polymer as a negative electrode material and the negative electrode is combined with an electrolyte having dissolved an alkali metal ion such as lithium ion, sodium ion and the like have been attracted attention. This kind of secondary battery is doping/undoping or intercalating/deintercalating the aforesaid metal ion electrochemically to the negative electrode and this doping/undoping phenomenon, etc. are utilized as a charge/discharge step. Thus, it has an advantage that, as caused in the secondary battery which is employed a conventional alkaline metal itself as the negative electrode, internal short due to precipitation of the alkaline metal dendritely during the discharge or remarkable deterioration of charge/discharge efficiency can be eliminated.
As this kind of secondary battery, there has been known one, for example, in which a negative electrode comprising a polyacetylene and a lithium ion are combined as disclosed in Japanese Provisional Patent Publication No. 136469/1981. Further, as a conductive polymer which is usable for a negative electrode material, there may be mentioned, in addition to the above polyacetylene, a linear high molecular compound having a conjugated double bond such as a poly(p-phenylene), a polypyrrol, a polythienylene, a polyaniline, a poly(p-phenylenesulfide), a poly(p-phenyleneoxide) and the like.
Since these conductive polymers are lightweight and a potential for doping/undoping an alkali metal ion such as lithium ion, etc. to said polymer is substantially similar as a charge/discharge potential in case that the alkali metal is employed as a negative electrode, it has an advantage that an energy density per unit weight is high when it has been used in a secondary battery. However, the aforesaid conductive polymer is unstable at a state of doping the alkali metal ion, that is, a charged state, and since it reacts with a solvent or decomposes itself, there are problems that a self-discharge becomes remarkably great at well as a cycle characteristic will be deteriorated.
On the other hand, there has been reported a secondary battery in which a graphite having a structure of spreading conjugated double bonds quadratically is used as a carbonaceous material and a graphite interlayer compound which is intercalated by electrochemically reducing an alkali metal ion is employed as a negative electrode active substance. However, in such a secondary battery, since an alkali metal-graphite interlayer compound formed by charging is chemically unstable and it reacts with solvent in accordance with destruction of a graphite structure, there are disadvantages that its storability is bad and deterioration of charge/discharge efficiency as well as lowering of cycle characteristics will be occurred.
Further, there has been reported a secondary battery in which as the carbonaceous material for constituting a negative electrode, those obtained by carbonizing an organic high molecular compound such as a phenol resin, a polyacrylonitrile, a cellulose and the like have been used. For example, in Japanese Provisional Patent Publication No. 209864/1983, a secondary battery using as a negative electrode a carbonaceous material obtained by heat treating an aromatic condensed polymer, which has an atomic ratio of hydrogen/carbon being in the range of 0.15 to 0.33 has been disclosed.
Such a secondary battery has high output power as compared with a secondary battery using the conventional conductive polymer or a graphite as a negative electrode. However, it is the actual circumstances that there is not yet improved at all in the point that the negative electrode reacts with an electrolytic solvent of self-discharge and a deterioration of cycle characteristics will be caused.
As stated above, there remains a problem that a negative electrode material which utilizes a dope/undope or an intercalate/deintercalate phenomenon of an alkali metal ion is used in a battery, in all cases, a self-discharge increases and a cycle lifetime is short.

SUMMARY OF THE INVENTION
An object of the present invention is to eliminate such conventional problems and to provide a secondary battery using a non-aqueous solvent which is less in self-discharge, good in charge/discharge cycle characteristics and excellent in storability.
The present inventors have carried out earnest investigations in order to establish the above object by focusing the development of a negative electrode material for the secondary battery using a non-aqueous solvent. As results, they have found that by constituting a negative electrode with a carbonaceous material which satisfies various conditions mentioned below simultaneously, a secondary battery using a non-aqueous solvent having excellent characterstics can be obtained and accomplished the present invention.
The present invention provides a secondary battery according to the present claim 1.

BRIEF DESCRIPTION OF THE DRAWINGS
Fig. 1 is a longitudinal sectional view showing one example of the non-aqueous solvent secondary battery of the present invention; and
Figs. 2 to 4 are drawings showing charge/discharge curve of the batteries.

DESCRIPTION OF THE PREFERRED EMBODIMENTS
In the secondary battery using a non-aqueous solvent of the present invention, as a starting material for obtaining a carbonaceous material which constitutes a negative electrode, it can be used at least one compound selected from the group consisting of a high molecular weight linear novolac resin, a condensed polycyclic hydrocarbon compound and polycyclic heterocyclic compound.
Condensed polycyclic hydrocarbon compounds are such that at least two monocyclic hydrocarbon compounds consisting of a three-or more membered ring are condensed together or derivatives of such condensed products. Specific examples of the condensed polycyclic hydrocarbon compounds may be mentioned, for example, naphthalene, phenanthrene, anthracene, triphenylene, pyrene, chresene, naphthacene, picene, perylene, pentaphene, pentacene and the like, and the derivatives thereof may include carboxylic acid, carbocyclic acid anhydride or carboxylic acid amide of the above compunds. Further, various kinds of pitches mainly comprising mixtures of the above respective compunds.
Polycyclic heterocyclic compounds are such that at least two monocyclic heterocyclic compounds consisting of a three- or more membered ring are condensed together or at least one such monocyclic heterocyclic compound is condensed with at least one monocyclic hydrocarbon compound consisting of a three- or more membered ring and derivatives of such condensed products. Specific examples of the polycyclic heterocyclic compounds may be mentioned, for example, indole, isoindole, quinoline, isoquinoline, quinoxaline, phthalazine, carbazole, acridine, phenazine, phenanthridine and the like, and the derivatives thereof may include carboxylic acid, carbocyclic acid anhydride or carboxylic acid amide of the above compounds. Further, 1,2,4,5-tetracarboxylic acid of benzene, its dianhydride or its diimide may also be used.
The carbonaceous materials of the present invention are those obtained by carbonizing the above mentioned respective compound and have a pseudographite structure satisfying the following conditions simultaneously.
That is, in the first place, an atomic ratio of hydrogen/carbon measured by an elemental analysis is not more than 0.10, more preferably not more than 0.07.
In the second place, a spacing (d₀₀₂) of (002) plane measured by X-ray wide angle diffraction is 3.37 Å or more, preferably 3.39 Å to 3.68 Å, more preferably 3.41 Å to 3.68 Å.
In the third place, a crystallite size in the direction of c axis, Lc, measured by the same X-ray wide angle diffraction is 12 Å to 150 Å, preferably 12 Å to 100 Å, more preferably 12 Å to 70 Å.
While the carbonaceous material of the present invention can be obtained by carbonizing the above-mentioned respective compounds, the procedures of the carbonization are considered as described below in the case of the condensed polycyclic hydrocarbon compound as the starting material. That is, when a thermal energy greater than the dissociation energy necessary to break the bond between the skeletal carbon and an adjacent hydrogen atom or a substituent is provided by heating, carbon radicals are formed predominantly by homolytic cleavage. A chain of carbon radicals is cyclized to provide a higher molecular weight and the polycyclic aromatic planes are developed so that the process of carbonization successively occurs. In the initial stage of carbonization, for example, benzene rings are bound together one-dimensionally to form a one-dimensional graphite structure. Subsequently, the benzene rings start to bind with one another two-dimensionally, and gradually expanding polycyclic aromatic planes begin to stack in layers to form a two-dimensional graphite structure.
With further progress of carbonization, more benzene rings are bound two-dimensionally and adequately expanded polycyclic aromatic planes stack one on another in an orderly manner to form the ordinary graphite. In accordance with the present invention, all structures that lead to the final graphite are collectively referred to as the pseudographite structure.
The pseudographite structure in accordance with the present invention can be determined quantitatively by using an X-ray wide angle diffraction. The ordinary graphite shows a sharp diffraction peak corresponding to a (002) plane at about 2θ = 26°.
A one-dimensional graphite formed in the initial stage of carbonization of the present invention shows no diffraction peak corresponding to the (002) plane or shows a very broad and its intensity is low.
Then, the polycyclic aromatic planes is developed two-dimensionally to some extent and begin to stack one after another, the diffraction peak corresponding to the (002) plane gradually becomes sharp and its intensity increases.
The pseudographite structure which characterizes the carbonaceous material of the present invention is such that the spacing of (002) planes, d₀₀₂, is at least 3.37 Å and the crystallite size in the direction of c axis, Lc, is not more than 150 Å. Preferably, d₀₀₂ is at least 3.40 Å and not more than 3.68 Å, whereas Lc is at least 12 Å and not more than 150 Å. The case where no diffraction peak corresponding to the (002) plane is observed at all is also included in the present invention.
When the carbonaceous material to be used is not satisfied any one of the above three inevitable requirements, that is, the atomic ratio of hydrogen/carbon is 0.10 or more, the spacing d₀₀₂ of the (002) plane measured by the X-ray wide angle diffraction is not more than 3.37 Å or the crystallite size in the direction of c axis, Lc, mesured by the same exceeds 150 Å, in the secondary battery using the carbonaceous material as the negative electrode, disadvantages that over voltage of charge/discharge at the negative electrode side becomes large, a gas is generated from the electrode at the charging, storability of the battery at the charged state is bad and charge/discharge cycle characteristics are deteriorated are caused.
In the carbonaceous material to be used in the present invention, the following conditions are also satisfied in addition to the above three conditions. That is, in the pseudographite structure determined quantitatively by using the X-ray wide angle diffraction, a crystallite size in the direction of a axis La is 10 Å or more, more preferably 15 Å or more and 70 Å or less, particularly preferably 19 Å or more. Further, a distance a₀ (= 2d₁₁₀) twice the spacing d₁₁₀ of the (110) planes measured by the X-ray wide angle diffraction is 2.38 Å or more and less than 2.46 Å, more preferably 2.39 Å or more. Moreover, at least one of the signals have an inter-peak line width (ΔHpp) obtained by first differential absorption curve of the electron spin resonance spectrum (measured at 23°C) of preferably 20 gauss or more, or no signals have an inter-peak line width (ΔHpp) of not more than 20 gauss (20 × 10⁻⁴ Tesla). More preferably, at least one of the signals have an inter-peak line width (ΔHpp) obtained by first differential absorption curve of the electron spin resonance spectrum (measured at 23°C) of preferably 50 gauss (50 × 10⁻⁴ Tesla) or more, or no signals have an inter-peak line width (ΔHpp) of not more than 50 gauss (50 × 10⁻⁴ Tesla).
The above carbonaceous material is specified by the atomic ratio of hydrogen/carbon obtained by the elemental analysis, but a small proportion of other atoms such as a nitrogen, oxygen, halogen may be present.
In the present invention, the carbonaceous material constituting the negative electrode can be obtained by carbonating the aforesaid compounds, more specifically by sintering under vacuum or through an inert gas (N₂, Ar, etc.). Since the carbonating temperature is closely related to the above atomic ratio of hydrogen/carbon, it is required to set the atomic ratio to not more than 0.10. The carbonating temperature is different depending on the kinds of the compounds to be used as a starting material but usually 500 to 3,000°C is preferred.
Further, after completion of the carbonization step, the obtained carbonaceous material may be activated by heating the carbonaceous material under oxidative gaseous atmosphere such as vapor, carbon dioxide, etc. whereby a specific surface area thereof can be increased.
The positive electrode material of the non-aqueous solvent secondary battery in accordance with the present invention is a metallic chalcogen compound which release or capture an alkali metal cation such as lithium ion, etc. accompanying charge/discharge reaction.
First, specific examples of the metallic chalcogen compounds to be used as the constituting material of the positive electrode of the present invention may include oxides such as Cr₃O₈, V₂O₅, V₆O₁₃, LiCoO₂, MoO₃, WO₃, etc.; sulfides such as TiS₂, V₂S₅, MoS₂, MoS₃, CuS, Fe_{0.25}V_{0.75}S₂, Cr_{0.25}V_{0.75}S₂, Cr_{0.5}V_{0.5}S₂, Na_{0.1}CrS₂, etc.; phosphine · sulfur compounds such as NiPS₃, FePS₃, etc.; and selenium compounds such as VSe₂, NbSe₃, etc., among them, TiS₂, M,oS₂ and V₂O₅ are particularly preferred.
To use such metallic chalcogen compounds as the positive electrode is preferred in the point of obtaining a secondary battery having large capacity and high reliability.
Further, in the non-aqueous secondary battery of the present invention, as the electrolyte, those dissolved an electrolytic salt in a non-aqueous solvent can be used. As the non-aqueous solvent, there may be used propylene carbonate, ethylene carbonate, dimethoxyethane, γ-butyrolactone, tetrahydrofuran, 2-methyltetrahydrofuran, sulforane, 1,3-dioxorane and the like, and they may be used alone or in combination of 2 or more. On the other hand, as the electrolytic salts, those obtained by optionally combining an anion such as CIO_4 -, PF_6 -, BF_4 -, CF₃SO_3 -, AsF_6 -, etc. and an alkali metal cation such as Li⁺, Na⁺, K⁺, etc. can be used. As the cation, in addition to the above alkali metal cation, cation species of quaternary amines such as N(CH₃)_4 +, N(C₂H₅)_4 +, N(n-C₃H₇)_4 +, etc. may be used.
When the metallic chalcogen compound is used as the active substance in the positive electrode and carbonaceous materials as the negative electrode of the secondary battery, either one of the positive electrode and the negative electrode or both of the positive and negative electrodes may preferably be doped an alkali metal cation such as Li⁺ and the like.
In case where doping is previously carried out with respect to the positive electrode, a battery in the discharged state can be realized while doping in the negative electrode provides a battery in the charged state. When the doping is carried but in both of the positive and negative electrodes, a battery in any state between discharged and charged by changing the ratio of doping amounts to the respective electrodes can be manufactured.
The capacity of the battery is determined by the total amounts of an alkali metal to be doped in the positive and/or negative electrodes.
When the carbonaceous material of the present invention is used in the negative electrode, the alkali metal is doped in a film-like or a strip-like carbonaceous material or is doped in moldings prepared by mixing a powder of the carbonaceous material and a powder state adhesive such as polytetrafluoroethylene, polyethylene, etc. and kneading, and then by molding under heating.
As the method for doping the alkali metal cation in the electrodes previously, there may be mentioned, for example, the electrochemical method, the chemical method and the physical method.
More specifically, as the electrochemical method, there may include a method in which the carbonaceous material of the present invention is used as the positive electrode, an alkali metal M is used as the negative electrode and an electrolyte obtained by dissolving an alkali metal salt such as MCIO₄, MPF₆, MBF₄, MAsF₆, MAICI₄, MCI, MBr, Ml and the like (where M is anyone of Li, Na, K, Rb and Cs) in an organic solvent such as propylene carbonate, 1,2-dimethoxyethane, γ-butyrolactone, dioxolan, ethylene carbonate, 2-methyltetrahydrofuran and the like is interposed between the electrodes to continue therebetween or a current is passed therethrough. As the chemical method, there may be mentioned the method in which the carbonaceous material according to the present invention is dipped in an organic solvent solution such as ether, aliphatic hydrocarbon, etc., dissolved an alkylated alkali metal therein. Further, as the physical method, there may be mentioned the method in which the carbonaceous material according to the present invention is exposed to vapor of an alkali metal. Of these methods, preferred are the electrochemical method and the chemical method and more preferred is the electrochemical method.
When the alkali metal is doped in the positive electrode, i.e., in the metallic chalcogen compound which is the discharged state of the battery, the same method as in the above carbonaceous material can also be applied.
In this case, when the metallic chalcogen compound electrode is used as the positive electrode, a negative potential is applied to the electrode and a positive potential is applied to the opposite electrode.
As the opposite electrode material, there may be mentioned, for example, an inert metal such as platinum, etc., and an alkali metal such as lithium, etc., but the use of lithium is particularly desired.
When the non-aqueous solvent secondary battery is constituted by the above material, the positive electrode and the negative electrode are laminated opposite to each other lying a separator between them and/or interposed a separator between them and a non-aqueous solvent containing an electrolyte. Each electrode has a plate-like structure in general, but the structure where one electrode is made a cylindrical shape and the other electrode is inserted therein may be employed. Further, the structure where the positive electrode and the negative electrode are made opposite to each other through a separator and spirally wound to form a spiral structure may also be employed.
Further, it is a desirable embodiment that the electrolytic solution is impregnated in a separator such as a non woven, a woven, an open cell cellular foaming material and a porous plastic sheet and the separator is interposed between both of the electrodes.
In the non-aqueous secondary battery constituted by the negative electrolyt, the positive electrode and the electrode comprising the aforesaid each materials, it is confirmed that an electrochemically oxidation/ reducton reaction in accordance with the dope/undope of the alkali metal ion is occurred at the charge/discharge and the battery has been less self-discharge and has good cycle characteristics.
In the secondary battery using a non-aqueous solvent of the present invention, a discharging capacity of the positive electrode should preferably be set 1.1-fold or more to that of the negative electrode, more preferably 1.1-fold to 3-fold, and most preferably 1.5-fold to 2-fold.
That is, for example, in case of using V₂O₅ as the positive electrode active substance, by repeating dope/undope of lithium to the V₂O₅, reversibility of dope/undope of lithium to the V₂O₅ will be gradually impaired when the doping is carried out in an amount of 2/3 or more to the maximum amount capable of being doped the lithium to the V₂O₅ so that deterioration of the battery capacity accompanied by proceeding of cycles will be remarkable.
By the reason as stated above, when the battery constitution using the metallic chalcogen compound as the positive electrode and the carbonaceous material in accordance with the present invention as the negative electrode is employed, it is preferred that the capacity of the positive electrode is set 1.1-fold or more to that of the negative electrode to enlarge a space (residual capacity) capable of accepting a lithium ion at discharging.
When the capacity of the positive electrode is set 1.1-fold or more to that of the negative electrode, the capacity of the battery is regulated by the capacity of the negative electrode. Therefore, it is not preferred to remarkably enlarge the capacity of the positive electrode to that of the negative electrode since high capacity characteristics which are possessed of the battery of the present constitution will be lost, and thus, the discharging capacity of the positive electrode is set within the above range.
In the present invention, each measurements of the elemental analysis, X-ray wide angle diffraction and electron spin resonance spectrum are carried out following the methods as described below.

[Elemental analysis]
A sample is dried in vacuum at 120°C for about 15 hours. Then, the sample is transferred onto a hot plate in a dry box and dried in vacuum at 100°C for 1 hour. A portion of the dried sample is put into an aluminum cup in an argon atmosphere, and the carbon content is determined from the weight of CO₂ gas evolved as a result of combustion whereas the hydrogen content is determined from the weight of H₂O also evolved by combustion. In the Examples of the present invention that follow, an elemental analyzer of Perkin-Elmer Model 240 C was used.

[X-ray wide angle diffraction]

(1) d₀₀₂, the spacing of (002) planes, and d₁₁₀, the spacing of (110) planes:
A powder of carbonaceous material (flaky carbonaceous material is reduced to a powder in an agate mortar) is packed into a sample cell together with about 15 wt% of the powder of an internal standard substance, a high-purity silicon powder of the standard grade for X-ray analysis. A wide-angle X-ray reflection diffractometer scan is obtained with monochromatic CuKα radiation from a graphite monochrometer. Instead of making corrections associated with the Lorentz factor, polarization factor, absorption factor and atomic scattering factor, the following simple and convenient method is used. Draw a baseline for the scan curves corresponding to diffractions at (002) and (110) Planes. Plot the substantial intensities as calculated from the baseline, obtaining corrected curves for (002) and (110) planes. Draw an angular axis at a height which is two-thirds of the.height of the peak in each curve and obtain the midpoint of the line defined by the two points where a line parallel to that angular axis intersects the scan curve. Correct the angle of the midpoint by the internal standard to obtain a value twice the angle of diffraction. Substitute this value and the wavelength of CuKα radiation, λ, into the following two equations of Bragg's law to obtain d₀₀₂ and d₁₁₀:
d
002
=
λ
2sinθ
[Å];
d
110
=
λ
2sinθ'
[Å]
wherein
- λ: 1.5418 Å
- θ, θ': the angle of diffraction corresponding to d₀₀₂ or d₁₁₀.

(2) Crystallite size in c and a axes, Lc and La:
Obtain the half-width β at a point half the height of the peak in each of the corrected scan curves prepared in (1), and substitute this value into the following equations:
Lc=
K·λ
β·cosθ
[Å];
La=
K·λ
β·cosθ'
[Å]
Various values may be taken for the shape factor K, but in the present invention, K = 0.90 is used. For the meanings of λ, θ and θ', the same as the previous paragraph.

[Line width between peaks in the first differential of the absorption spectrum of electron spin resonance: ΔHpp]
The first differential of the absorption spectrum of electron spin resonance was measured with JEOL JES-FE 1X ESR spectrometer in the X-band. A powder of carbonaceous material (flaky carbonaceous material is reduced to a powder in an agate mortar) is put into a capillary tube (ID: 1 mm) which is placed in an ESR tube (OD: 5 mm). The radiofrequency magnetic field is modulated by an amount of 6.3 gauss. All the procedures above are followed within air at 23°C. The value of the line width between peaks in the first differential of the absorption spectrum (ΔHpp) is determined by comparison to a standard sample Mn⁺/MgO.

EXAMPLES

Examples 1 to 4

(1) Preparation of the carbonaceous material
In a reactor were put 108 g of ortho-cresol, 32 g of paraformaldehyde and 240 g of ethylcwllosolve with 10 g of sulfuric acid, and the mixture was reacted at 115°C for 4 hours under stirring. After completion of the reaction, the mixture was neutralized by adding 17 g of NaHCO₃ and 30 g of water. Then, under stirring with high speed, the reaction mixture was poured into 2 liters of water and precipitated products were collected by filtration to obtain 115 g of linear high molecular weight novolac resin. The number average molecular weight of the resin was measured by applying the vapor pressure method (in methylethyl ketone, at 40°C) to obtain 2600.
After dissolving 2.25 g of this novolac resin and 0.25 g of hexamine in ethanol, the ethanol was evaporated and removed to obtain a mixture of the novolac resin and hexamine. Then, the mixture was put in a glass vessel under nitrogen gas stream, and heat treated at 250°C for 2 hours under nitrogen gas stream.
The thus obtained heat-treated mixture was not dissolved in ethanol but swelled. The swelled heat-treated mixture was carried out the press forming at a temperature of 190°C under a pressure of 200 Kg/cm to obtain a strip having a width of 2 cm, a length of 5 cm and a thickness of 1 mm.
Then, the press forming product was set in an electric furnace and under nitrogen stream carbonization was carried out by elevating the temperature to 2100°C per elevating speed of 20°C/min and maintaining the temperature, i.e., at 2100°C for one hour under nitrogen stream. As a result, 80 mg of a strip-like carbonaceous material a having black color was obtained.
Further, in the above steps, by the same conditions as in the above except for changing the carbonization temperature to 1600°C, 1400°C, 1000°C and 800°C, each 80 mg of strip-like carbonaceous materials b, c, d and e was obtained, respectively.
Each value of the carbonizatidn temperature [°C] during synthesis, the atomic ratio of hydrogen/carbon measured by elemental analysis, the plane spacing d₀₀₂ [Å] of (002) plane and the plane spacing d₁₁₀ [Å] of (110) plane each measured by the X-ray wide angle diffraction, the crystallite size Lc [Å] in the direction of c axis and the crystallite size La [Å] in the direction of a axis, and the line width between peaks of the electron spin resonance spectrum ΔHpp [gauss] of the carbonaceous materials a to e was summarized in Table 1. In the table, each of the above values with respect to graphite was also shown.
As clearly seen from the table, among the above carbonaceous materials a to e; a and b are materials for the negative electrode.

TABLE 1
Carbonaceous material | Carbonization temperature [°C] | Hydrogen/carbon atomic ratio | d₀₀₂ [Å] | a₀ (2d₁₁₀) [Å] | La [Å] | Lc [Å] | ΔHpp [gauss]
a | 2100 | 0.04 | 3.58 | 2.42 | 23 | 15 | 200
b | 1600 | 0.05 | 3.68 | 2.39 | 19 | 12 | 90
c | 1400 | 0.12 | 3.72 | 2.39 | 17 | 11 | 60
d | 1000 | 0.16 | 3.90 | 2.38 | 14 | 11 | -
e | 800 | 0.23 | unclear the diffraction peak | 18
graphite | - | 0.01 | 3.36 | 2.46 | 327 | 308 | 5

(2) Evaluating tests of the secondary battery performances
By using each of the carbonaceous materials ordained by the above, the secondary batteries using a non-aqueous solvent as shown in Fig. 1 were prepared. In Fig. 1, reference numeral 1 represents a negative electrode and it is prepared by press forming 50 mg of each powder of the carbonaceous material as mentioned above to form a pellet having a diameter of 20 mm. 2 is a collector for the negative electrode comprising nickel. A negative electrode terminal 4 is electrically connected to the collector 2 for the negative electrode through a spring 3. 5 is positive electrode which'is prepared by press forming 50 mg of each powder of the carbonaceous material as mentioned above to form a pellet having a diameter of 20 mm, is prepared by mixing and kneading 450 mg of titanium disulfide (TiS₂) with 25 mg of polytetrafluoroethylene and 25 mg of acetylene black and then press forming it to a pellet having a diameter of 20 mm or is prepared by mixing and kneading 450 mg of vanadium pentoxide (V₂O₅) with 25 mg of polytetrafluoroethylene and 25 mg of acetylene black and then press forming it to a pellet having a diameter of 20 mm. The positive electrode 5 is one in which is carried out a preliminary discharging at 2 mA for 10 hours in a propylene carbonate solution containing 1.5 mole/liter of LiCO₄. Further, the positive electrode 5 is compressedly adhered to a collector 6 for the positive electrode comprising titanium which serves as a positive terminal. Betwen the negative electrode 1 and the positive electrode 5, a separator 7 comprising non woven fabric of propylene carbonate is provided therethrough and they are all compressedly adhered with each other by the spring 3. Reference numerals 8 and 9 are vessels made of Teflon (trade name, produced by du Pont de Nemours), and inner materials are sealed by an O ring 10. Moreover, 2 ml of a propylene carbonate solution containing 1.5 mole/liter of LiCIO₄ as an electrolyte is filled in the separator 7, and the vessels 8 and 9.
Here, by combinedly using the carbonaceous materials a, b, c, d and e shown in Table 1, and TiS₂ and V₂O₅ as the above positive electrode 5 and the negative electrode 1, batteries F, G, H, I, J and K were prepared and they were evaluated with respect to the following evaluating tests of respective performances.

Comparative examples 1 to 8
In the same manner as in Examples 1 to 4, by combinedly using the carbonaceous materials d and e shown in Table 1, graphite and TiS₂ and V₂O₅ as the above positive electrode 5 and the negative electrode 1, batteries H, K, N, O, P, Q, R and S for comparative purposes were prepared and they were also evaluated with respect to the following evaluating tests of respective performances.

(a) Evaluating test of charge/discharge cycle characteristics
(i) As to the above respective batteries F to K and N to S, charge/discharge test was carried out under argon gas atmosphere at 25°C up to each 100 cycles. A charging current and a discharging current were all 500 µA and discharge was started immediately after completion of charging. Closed circuit terminal voltages for charging and discharging processes were set as follows, respectively.
- Batteries F to H and N to P:
  - charging voltage = 2.1 V,
  - discharging terminal voltage = 1.0 V
  - Batteries I to K and Q to S:
    - charging voltage = 3.0 V,
    - discharging terminal voltage = 2.0 V
Fig. 3 shows charge/discharge curves of the batteries F, H and O at the fifth cycle. In the Fig., curves F₁, H₁ and O₁ each represent charging curves of the batteries F, H and O, respectively, and curves F₂, H₂ and O₂ each represent discharging curves of the same. Moreover, in Fig. 4, charge/discharge curves of the batteries I, K and Q at the fifth cycle are shown, and curves I₁, K₁ and Q₁ each represent charging curves of the batteries I, K and Q, respectively, and curves I₂, K₂ and Q₂ each represent discharging curves of the same.
Furthermore, in Table 2, charging capacities, discharging capacities and charge/discharge efficiencies at the fifth cycle and the 100th cycle and a ratio (%) of discharging capacity at the 100th cycle to the fifth cycle of each of the batteries are shown. (ii) Charge/discharge test was carried out in the same manner as in the above (i) except for changing the charge/discharge cycle number to 50 cycles. In Table 3, charging capacities, discharging capacities and charge/discharge efficiencies at the tenth cycle and the 50th cycle and a ratio (%) of discharging capacity at the 50th cycle to the tenth cycle of each of the batteries are shown.

(b) Evaluating tests of self-discharge and preservability
(i) In the same manner as in the above (a), usual charge/discharge was carried out up to the ninth cycle and then self-discharge test was carried out at the tenth cycle. That is, at the tenth cycle, discharge after completion of charging was carried out after preservation at 25°C for 30 days.
In Table 4, charging capacities, discharging capacities and charge/discharge efficiencies at which discharging was immediately carried out at the ninth cycle and at which discharging was carried out at the tenth cycle after preservation for 30 days and a ratio (%) of discharging capacity at the tenth cycle to the ninth cycle of each of the batteries are shown.
(ii) In the same manner as in the above (i), usual charge/discharge was carried out up to the forth cycle and then self-discharge test was carried out at the fifth cycle. That is, at the tenth cycle, discharge after completion of charging was carried out after preservation at 25°C for 30 days.
In Table 5, charging capacities, discharging capacities and charge/discharge efficiencies at which discharging was immediately carried out at the forth cycle and at which discharging was carried out at the fifth cycle after preservation for 30 days and a ratio (%) of discharging capacity at the fifth cycle to the forth cycle of each of the batteries are shown.
As clearly seen from the description as mentioned above, the secondary battery using a non-aqueous solvent of the present invention using a carbonaceous material having the specific structure for the negative electrode has extremely excellent charge/discharge cycle characteristics as compared with those used a conventional graphite as the negative electrode material and those used a carbonaceous material deviated from the requirements of the present invention, and is less in self-discharge and excellent in preservability whereby its industrial value is extremely great.
1. A secondary battery using a non-aqueous solvent comprising a positive electrode capable of being re-charged and constituted by a metallic chalcogen compound, an electrolytic solution which comprises an electrolyte dissolved in the non-aqueous solvent, and a negative electrode capable of being re-charged which comprises a powder of a carbonaceous material obtained by the carbonization of at least one of a high molecular weight linear novolac resin, a condensed polycyclic hydrocarbon compound and a polycyclic heterocyclic compound, and having a pseudographite structure, which structure, if it were to be subjected to further progress of carbonisation, would be converted to graphite, an atomic ratio of hydrogen/carbon of not more than 0.10, a spacing of (002) planes as determined by X-ray wide-angle diffraction of 3.37-3.68 Å, a crystallite size in the direction of the c axis of 12 Å to 150 Å, a distance a₀ twice the spacing d₁₁₀ of the (110) planes measured by X-ray wide angle diffraction of 2.38 Å to less than 2.46 Å and a crystallite size in the direction of the a axis, La, of 10 Å to 70 Å.
2. A secondary battery using a non-aqueous solvent according to claim 1, wherein the battery has a laminated structure of said positive electrode and said negative electrode through a separator impregnated with an electrolyte.
3. A secondary battery using a non-aqueous solvent according to claim 1, wherein said electrolyte is a combination of an alkali metal cation and at least one anion selected from ClO_4 -, PF_6 -, BF_4 -, CF₃SO_3 - and AsF_6 -; or a quaternary ammonium salt.
4. A secondary battery using a non-aqueous solvent according to claim 1, wherein said negative electrode comprises a carbonaceous material having a spacing of (002) planes, d₀₀₂ as determined by X-ray wide angle diffraction of 3.39 Å - 3.68 Å and a crystallite size in the direction of the c axis, Lc, of 12 Å to 100 Å.
5. A secondary battery using a non-aqueous solvent according to claim 4, wherein said negative electrode comprises a carbonaceous material having an atomic ratio of hydrogen/carbon of not more than 0.07, a d₀₀₂ of 3.41 Å to 3.68 Å and an Lc of 12 Å to 70 Å.
6. A secondary battery using a non-aqueous solvent according to claim 5, wherein said negative electrode comprises a carbonaceous material having an La of 15 Å to 70 Å and an a₀ of 2.39 Å to less than 2.46 Å.
7. A secondary battery using a non-aqueous solvent according to claim 1, wherein said metallic chalcogen compound is selected from Cr₃O₈, V₂O₅, V₆O₁₃, LiCoO₂, MoO₃, WO₃, TiS₂, V₂S₅, MoS₂, MoS₃, CuS, Fe_{0.25}V_{0.75}S₂, Cr_{0.25}V_{0.75}S₂, Cr_{0.5}V_{0.5}S₂, Na_{0.1}CrS₂, NiPS₃, FePS₃, VSe₂ and NbSe₃.
8. A secondary battery using a non-aqueous solvent according to claim 1, wherein the discharging capacity of the positive electrode is set 1.1-fold or more to that of the negative electrode.
9. A secondary battery using a non-aqueous solvent according to claim 1, wherein said carbonaceous material is previously doped with an alkali metal cation.
10. A secondary battery using a non-aqueous solvent according to claim 1, wherein said chalcogen compound is previously doped with an alkali metal cation.
1. Sekundärbatterie, bei der ein nicht-wässriges Lösungsmittel verwendet wird, umfassend eine zur Wiederaufladung befähigte positive Elektrode aus einer metallischen Chalkogen-Verbindung, eine elektrolytische Lösung, die einen in dem nicht-wässrigen Lösungsmittel gelösten Elektrolyt enthält, sowie eine zur Wiederaufladung befähigte negative Elektrode, welche ein Pulver aus einem kohlenstoffhaltigen Material enthält, das durch Karbonisieren von mindestens einem hochmolekularen linearen Novolak-Harz, einer kondensierten polyzyklischen Kohlenwasserstoff-Verbindung und von mindestens einer polyzyklischen heterozyklischen Verbindung erhältlich ist und eine Pseudographit-Struktur aufweist, wobei die Struktur, falls sie weiter karbonisiert würde, in Graphit überführt würde, und welche ein Atomverhältnis von Wasserstoff/Kohlenstoff von nicht mehr als 0,10, einen Abstand der (002)-Gitterebenen, bestimmt durch Röntgenstrahl-Weitwinkelbeugung, von 3,37 bis 3,68 Å, eine Kristallit-Größe in Richtung der c-Achse von 12 bis 150 Å, eine Entfernung a₀ des doppelten Abstands d₁₁₀ der (110)-Gitterebenen, gemessen durch Röntgenstrahl-Weitwinkelbeugung, von 2,38 bis weniger als 2,46 Å sowie eine Kristallit-Größe in Richtung der a-Achse, La, von 10 bis 70 Å aufweist.
2. Sekundärbatterie gemäß Anspruch 1, bei der ein nicht-wässriges Lösungsmittel verwendet wird, worin die Batterie eine über einen mit einem Elektrolyt imprägnierten Separator laminierte Struktur der genannten positiven und negativen Elektroden aufweist.
3. Sekundärbatterie gemäß Anspruch 1, bei der ein nicht-wässriges Lösungsmittel verwendet wird, worin der genannte Elektrolyt eine Kombination eines Alkalimetallkations und mindestens eines Anions, ausgewählt aus C10_4 -, PF_6 -, BF_4 -, CF₃SO_3 - und aus AsF_6 -, oder ein quaternäres Ammoniumsalz ist.
4. Sekundärbatterie gemäß Anspruch 1, bei der ein nicht-wässriges Lösungsmittel verwendet wird, worin die genannte negative Elektrode ein kohlenstoffhaltiges Material umfaßt, das einen Abstand der (002)-Gitterebenen, d₀₀₂, bestimmt durch Röntgenstrahl-Weitwinkelbeugung, von 3,39 bis 3,68 Å sowie eine Kristallit-Größe in Richtung der c-Achse, Lc, von 12 bis 100 Å aufweist.
5. Sekundärbatterie gemäß Anspruch 4, bei der ein nicht-wässriges Lösungsmittel verwendet wird, worin die genannte negative Elektrode ein kohlenstoffhaltiges Material umfaßt, das ein Atomverhältnis von Wasserstoff/Kohlenstoff von nicht mehr als 0,07, einen d₀₀₂-Wert von 3,41 bis 3,68 Å und einen Lc-Wert von 12 bis 70 Å aufweist.
6. Sekundärbatterie gemäß Anspruch 5, bei der ein nicht-wässriges Lösungsmittel verwendet wird, worin die genannte negative Elektrode ein kohlenstoffhaltiges Material umfaßt, das einen La-Wert von 15 bis 70 Å und einen a₀-Wert von 2,39 bis weniger als 2,46 Å aufweist.
7. Sekundärbatterie gemäß Anspruch 1, bei der ein nicht-wässriges Lösungsmittel verwendet wird, worin die genannte metallische Chalkogen-Verbindung aus Cr₃O₈, V₂O₅, V₆O₁₃, LiCoO₂, MoO₃, WO₃, TiS₂, V₂S₅, MoS₂, MoS₃, CuS, Fe_{0,25}V_{0,75}S₂, Cr_{0,25}V_{0,75}S₂, Cr_{0,5}V_{0,5}S₂, Na_{0,1}CrS₂, NiPS₃, FePS₃, VSe₂ und aus NbSe₃ ausgewählt ist.
8. Sekundärbatterie gemäß Anspruch 1, bei der ein nicht-wässriges Lösungsmittel verwendet wird, worin die Entladungskapazität der positiven Elektrode auf das 1,1-fache oder mehr zu derjenigen der negativen Elektrode festgesetzt ist.
9. Sekundärbatterie gemäß Anspruch 1, bei der ein nicht-wässriges Lösungsmittel verwendet wird, worin das genannte kohlenstoffhaltige Material vorab mit einem Alkalimetallkation dotiert ist.
10. Sekundärbatterie gemäß Anspruch 1, bei der ein nicht-wässriges Lösungsmittel verwendet wird, worin die genannte Chalkogen-Verbindung vorab mit einem Alkalimetallkation dotiert ist.
1. Batterie secondaire utilisant un solvant non aqueux comprenant une électrode positive capable d'être rechargée et constituée par un composé métallique chalcogène, une solution électrolytique qui comprend un électrolyte dissous dans le solvant non aqueux, et une électrode négative capable d'être rechargée qui comprend une poudre d'un matériau carbonisé obtenu par la carbonisation d'au moins une résine novolaque linéaire à masse moléculaire élevée, un composé polycyclique hydrocarboné condensé et un composé polycyclique hétérocyclique, et ayant une structure pseudographite, laquelle structure, si elle était sujette à l'avancement ultérieur de la carbonisation, pourrait être convertie en graphite, un ratio atomique d'hydrogène/carbone non supérieur à 0,10, un espacement des plans (002) comme déterminé par diffraction des rayons X à grand angle de 3,37 à 3,68 Å, une dimension de cristallite dans la direction de l'axe c de 12 Å à 150 Å, une distance a_o double de l'espacement d₁₁₀ des plans (110) mesurée par la diffraction des rayons X à grand angle de 2,38 Å à moins de 2,46 Å et une dimension de cristallite dans la direction de l'axe a, La, de 10 A à 70 Å.
2. Batterie secondaire utilisant un solvant non aqueux selon la revendication 1, dans laquelle la batterie présente une structure laminée de ladite électrode positive et de ladite électrode négative avec entre elles un séparateur imprégné d'un électrolyte.
3. Batterie secondaire utilisant un solvant non aqueux selon la revendication 1, dans laquelle ledit électrolyte est une combinaison de cation d'un métal alcalin et d'au moins un anion choisi parmi ClO_4 -, PF_6 -, BF_4 -, CF₃SO_3 - et AsF_6 - ; ou un sel d'ammonium quaternaire.
4. Batterie secondaire utilisant un solvant non aqueux selon la revendication 1, dans laquelle ladite électrode négative comprend un matériau carbonisé ayant un espacement des plans (002), d₀₀₂, tel que déterminé par la diffraction des rayons X à grand angle de 3,39 Å à 3,68 Å et une dimension de cristallite dans la direction de l'axe c, Lc, de 12 Å à 100 Å.
5. Batterie secondaire utilisant un solvant non aqueux selon la revendication 4, dans laquelle ladite électrode négative comprend un matériau carbonisé ayant un ratio atomique d'hydrogène/carbone pas plus grand que 0,07, un d₀₀₂ de 3,41 Å à 3,68 Å et un Lc de 12 Å à 70 Å.
6. Batterie secondaire utilisant un solvant non aqueux selon la revendication 5, dans laquelle ladite électrode négative comprend un matériau carbonisé ayant une La de 15 Å à 70 Å et un a_o de 2,39 Å à moins de 2,46 A.
7. Batterie secondaire utilisant un solvant non aqueux selon la revendication 1, dans laquelle ledit composé chalcogène métallique est choisi parmi Cr₃O₈ , V₂O₅, V₆O₁₃, LiCoO₂, MoO₃, WO₃, TiS₂, V₂S₅, MoS₂, MoS₃, CuS, Fe_{0,25}V_{0,75}S₂, Cr_{0,25}V_{0,75}S₂, Cr_{0,5}V_{0,5}S₂, Na_{0,1}CrS₂, NiPS₃, FePS₃, VSe₂ et NbSe₃.
8. Batterie secondaire utilisant un solvant non aqueux selon la revendication 1, dans laquelle la capacité de décharge de l'électrode positive est fixée à 1,1 fois ou plus celle de l'électrode négative.
9. Batterie secondaire utilisant un solvant non aqueux selon la revendication 1, dans laquelle ledit matériau carbonisé est dopé préalablement avec un cation d'un métal alcalin.
10. Batterie secondaire utilisant un solvant non aqueux selon la revendication 1, dans laquelle ledit composé chalcogène est préalablement dopé avec un cation d'un métal alcalin.