......DE....FRGB..................................
R
DIM360 - Ver 2.5 (21 Aug 1997) 2100000/0
0216366
EUROPEAN PATENT SPECIFICATION
B1
19920506
EP
86113129.0
19860924
19891003
19910301
en
en
en
210815/85
19850924
JP
19920506
199219
19870401
198714
19920506
199219
19910726
5
5G 06K 19/06 A
de
Speicherkarte
en
Memory card
fr
Carte à mémoire
EP-A- 0 071 255
EP-A- 0 140 230
EP-A- 0 163 534
EP-A- 0 193 856
GB-A- 2 095 175
GB-A- 2 096 541
Hara, Kazuya Patent Dept Dev.Div Hamura R&D Center
Casio Computer Co. Ltd. 3-2-1 Sakae-cho
Hamura-machi Nishitama-gun Toky 190-11
JP
CASIO COMPUTER COMPANY LIMITED
00249360
19 060 EP
6-1, 2-chome, Nishi-Shinjuku
Shinjuku-ku Tokyo 160
JP
Strasse, Joachim, Dipl.-Ing.
et al
00011612
Strasse, Vonnemann & Partner Balanstrasse 55
81541 München
DE
DE
FR
GB
19890531
198922
The present invention relates to a memory card including an IC (Integrated Circuit) chip.
Conventionally known is a memory card with an IC chip therein, which starts to operate in response to an external input signal, compares the input signal with identification information previously stored in the chip, and delivers a comparison result.
From GB-A-2 095 175 an identification card is known with a symmetrical structure in which the IC module and the leads and contact surfaces necessary for the operation of the module are attached to a separate carrier and embedded in the identification card with the IC module located in an area of the card having the maximum permitted thickness, whereas the contact surfaces are arranged outside this area.
Disclosed in US-A-4,483,067 is a method for manufacturing an identification card of a type which is so constructed that a secondary carrier, on which an IC chip is mounted, is provided in a primary carrier, which is formed of a number of sheets of an electrically insulating thermoplastic material.
US-A-4,222,516 also discloses an identification card which is formed of only a single sheet.
Using the above prior art identification cards, it was revealed that the cards are prone to warp.
The object of the present invention is to provide a memory card, which is manufactured by laminating a plurality of sheets, and cannot warp so much that its performance is affected substantially.
The object of the present invention is achieved by a memory card comprising:
an IC module including said IC chip and a plurality of external connecting terminals;
a first laminated structure formed of a plurality of sheets laminated to each other and having a plurality of holes for exposing said external connecting terminals of said IC module to the outside; and
a second laminated structure formed of a plurality of sheets laminated to each other;
wherein the first and second laminated structures are, apart from the holes in the first structure, vertically symmetrical with respect to each other concerning the number of sheets and adhesive-agent layers and the respective material of the sheets;
characterized in that
said IC module comprises a circuit board on which said IC chip and said external connecting terminals are mounted;
a center sheet having a cavity for accomodating said circuit board is provided;
said first laminated structure is bonded to one side surface of said center sheet, and said second laminated structure is bonded to the other side surface of said center sheet; and each of the sheets has substantially the same plane size as that of said center sheet.
According to the invention the first and second laminated structures as well as the center sheet are formed so that the card of uniform thickness in spite the provision of the IC module within the card.
Further advantages embodiments are defined in the subclaims 2 to 6.
This invention can be more fully understood from the following detailed description when taken in conjunction with the accompanying drawings, in which:
- Fig. 1 is a perspective view showing a memory card according to an embodiment of the present invention;
- Fig. 2 is an exploded perspective view of the memory card of Fig. 1; and
- Fig. 3 is an enlarged sectional view of the memory card, as taken along line III-III in Fig. 1.
An embodiment of the present invention will now be described with reference to the accompanying drawings.
Fig. 1 shows memory card 10 according to an embodiment of the present invention.
Memory card 10 has a rectangular plane configuration, and its dimensions, including the length, width, and thickness, are prescribed by the ISO (International Standardization Organization). Magnetic stripe 12 is formed on the upper surface of card 10, so as to extend beside and along one longitudinal edge of the card. Corresponding to stripe 12, IC module 14 is contained in card 10. Module 14 includes L-shaped printed-circuit board 16 CPU (central processing unit) chip 18 and memory chip 20, mounted on longitudinal portion 24 of board 16 so as to avoid the central part of portion 24, and a plurality of external terminals 22 on bent portion 26 of board 16. Memory chip 20 is formed, for example, of a nonvolatile EP-ROM (erasable and programmable ROM) or EEP-ROM (electrically erasable and programmable ROM). CPU chip 18 serves to compare a personal identification number, inputted through terminals 22, with personal identification information stored in chip 20, and to deliver the result of the comparison. Here it is to be desired that the information in chip 20 should not be transmitted to terminals 22. Besides the identification information, personal past records, including credit and transaction data, are stored in chip 20.
Fig. 2 is an exploded perspective view of memory card 10, and Fig. 3 is an enlarged sectional view taken along line III-III in Fig. 1. As seen from these drawings, card 10 has a seven-layer construction.
L-shaped printed-circuit board 16 of IC module 14 is formed of a flexible, glass-epoxy resin sheet with a thickness of 200 microns. Longitudinal portion 24 of board 16 is a little shorter than the longitudinal edge of memory card 10. The width of portion 24 is greater than the respective transverse dimensions of CPU chip 18 and memory chip 20. Opening 28 for CPU chip 18 is formed in a cross region of board 16, where longitudinal portion 24 crosses bent portion 26, while opening 30 for memory chip 20 is formed near the free end of portion 24. Eight external terminals 22 are arranged, in two equal lines, near the free end of bent portion 26 of board 16. Formed on the upper surface of board 16, moreover, is predetermined lead pattern 32, which electrically connects chips 18 and 20 to terminals 22. Pattern 32 is formed by etching a copper foil which is laminated on insulating board 16. External terminals 22 are formed on pattern 32, by plating with copper, to a predetermined thickness. Joint portions 36 (Fig. 3), between lead pattern 32 and terminals 34 of each of chips 18 and 20, are plated with tin, on their back. In this embodiment, terminals 34 of each chip are each formed of a gold bump on the upper surface of the chip. CPU chip 18 and memory chip 20 are accommodated in openings 28 and 30, respectively, and joint portions 36 of pattern 32 are connected to the corresponding gold-bump terminals 34 of chip 18 and 20. These connections are made by welding gold and tin, by pulse-heating. Connecting portions between gold-bump terminals 34 of CPU chip 18 and joint portions 36 of pattern 32 and connecting portions between gold-bump terminals 34 of memory chip 20 and joint portions 36 of pattern 32 are covered with sealed-resin 38 by molding, so that chips 18 and 20 are fixed to board 16. After the connections are made, the lower portion of each chip projects slightly from the lower surface of board 16, through its corresponding opening 28 or 30, as shown in Fig. 3.
Center sheet 42, having L-shaped opening 40 for IC module 14, is formed of a rigid polyvinyl-chloride sheet with a thickness of approximately 200 microns. Longitudinal portion 44 of opening 40 corresponds to magnetic stripe 12 on the top surface of memory card 10.
First upper and lower sheets 46 and 48, each formed of a soft polyvinyl-chloride sheet with a thickness of 40 microns, are bonded to the upper and lower surfaces, respectively, of center sheet 42, by means of an adhesive agent. As shown in Fig. 3, the respective lower surfaces of CPU chip 18 and memory chip 20 are in contact with the upper surface of lower sheet 48. Between sheets 46 and 48, the inside spaces of openings 28 and 30 for chips 18 and 20 of board 16, are filled with epoxyresin-based filler 50, e.g., of a two-liquid type, to fix the chips. Eight small apertures 52 in two lines are formed on upper sheet 46, into which external terminals 22 on board 16 are fitted.
Second upper and lower sheets 54 and 56, each formed of a rigid polyvinyl-chloride sheet with a thickness of 100 microns, are bonded to the upper surface of first upper sheet 46 and the lower surface of first lower sheet 48, respectively. Square openings 58 and 60 are formed on sheets 54 and 56, respectively. Openings 58 and 60, which have an area corresponding to that of each chip of IC module 14, are located corresponding to chips 18 and 20, respectively. Square metal pieces 62 and 64 are fitted in their corresponding openings 58 and 60. They serve to protect the chips from external force. Pieces 62 and 64 are formed of stainless steel, and are thinner than second sheets 54 and 56. This difference in thickness, between pieces 62 and 64 and sheet 54 and 56, as shown in Fig. 3, allows the projection of CPU chip 18 and memory chip 20 in the thickness direction, from board 16, and the projection of first sheets 46 and 48, corresponding to the chips. At the same time, the difference prevents metal pieces 62 and 64 from projecting in the thickness direction, from second sheets 54 and 56. Eight small apertures 66 in two lines are also formed on second upper sheet 54, corresponding in position to external terminals 22 on board 16.
Upper and lower outermost films 68 and 70, each formed of a soft polyvinyl chloride film with a thickness of approximately 100 microns, are bonded to the upper surface of second upper sheet 54 and the lower surface of second lower sheet 56, respectively. Each small apertures 72 in two lines are formed on film 68, corresponding in positions to external terminals 22 on board 16. Magnetic stripe 12 is formed by coating fine powder of iron oxide, etc., on the upper surface of film 68, along the longitudinal edge of film 68. Stripe 12 does not extend on the central portion in the transverse direction.
A method of manufacturing memory card 10, according to the aforementioned embodiment of the present invention, will now be described.
- (1) Second lower sheet 56, first lower sheet 48, center sheet 42, first upper sheet 46, second upper sheet 54, and upper outermost film 68 are arranged successively over lower outermost film 70, so as to be spaced vertically. These films and sheets are continuous in their longitudinal directions, respectively, and are stored in the form of a roll, respectively. L-shaped opening 40, openings 60, small apertures 52, and openings 58 and small apertures 66 are previously formed on sheets 42, 56, 46 and 54, respectively.
- (2) Lower outermost film 70 is bonded to the lower surface of second lower sheet 56, while metal pieces 64, fitted in their corresponding openings 60 of second lower sheet 56, are bonded to the upper surface of film 70. Likewise, upper outermost film 68 is bonded to the upper surface of second upper sheet 54, while metal pieces 62, fitted in openings 58 of second upper sheet 54, are bonded to the lower surface of film 68.
- (3) First lower sheet 48 is bonded to the upper surface of second lower sheet 56, and then, center sheet 42 is bonded to the upper surface of sheet 48.
- (4) IC module 14, which is manufactured separately in advance, is fitted into L-shaped opening 40 of center sheet 42 so that the lower surface of module 14 is bonded to the upper surface of first lower sheet 48.
- (5) Filler 50 is filled into openings 28 and 30 for chips 18 and 20, in board 16, so as to surround the chips.
- (6) First upper sheet 46 is bonded to the upper surface of center sheet 42, which has IC module 14 in its L-shaped opening 40. Then, the lower surface of second upper sheet 54, to which upper outermost film 68 has been bonded, is bonded to the upper surface of sheet 46. Thereupon, the top face of each external terminal 22 of IC module 14 is flush with the upper surface of film 68, as shown in Fig. 3. At the same time, unification of films 68, sheets 54, 46, 42, 48 and 56, and film 70 is completed.
- (7) Memory card 10 is cut for the plane dimensions prescribed by the ISO.
- (8) Magnetic strip 12 is formed on the upper surface of upper outermost film 68.
The thickness of adhesive-agent layers, between the films and sheets, is approximately 20 microns. Thus, memory card 10 has an average thickness of about 800 microns, as provided by the ISO.
Memory card 10, according to the above described embodiment of the present invention, is characterized in that an upper laminated structure which includes first and second upper sheets 46 and 54 and upper outermost film 70 and locates on the upper surface side of center sheet 42 having IC module 14 in its L-shaped opening 40, and a lower laminated structure which includes first and second lower sheets 48 and 56 and lower outermost film 70 and locates on the lower surface side of sheet 42, are equivalent in the combined number of films and sheets, and in the number of adhesive-agent layers, and are vertically symmetrical.
Accordingly, the upper and lower laminated structures are equally subject to contraction of the adhesive agent, due to its drying after lamination, and extension or contraction of the films and sheets, attributable to changes of temperature and humidity. Thus, tensile and compressive forces, produced in memory card 10, are well-balanced, so that the card cannot be warped.
Metal pieces 62 and 64, used to protect CPU chip 18 and memory chip 20 contained in memory card 10 from external force, have a plane area much smaller than those of second upper and lower sheets 54 and 56. Therefore, card 10 can have flexibility. If card 10 is flexible, it can be deformed in accordance with the motion of the surface of a user's body, as it is put in a trousers back pocket, for example. Therefore, the pocketed card can reduce its sense of unfitness and the possibility of its injuring the body. As shown in Fig. 3, moreover, the top face of each external terminal 22 of IC module 14 is flush with the upper surface of upper outermost film 68. Accordingly, dust, which may cause a failure in electrical contact, between a probe (not shown) of a terminal apparatus and terminals 22, is prevented from collecting in small apertures 72 of film 68.
In the embodiment described above, CPU chip 18 and memory chip 20, mounted on board 16, are spaced. Alternatively, however, these chips may be formed into a single unit, which may be disposed in a single position on board 14. In this case, the unified IC chip is preferably located close to external terminals 22. Magnetic stripe 12 may be omitted, for the simplicity of manufacturing processes. Since memory card 10 is vertically symmetrical, with respect to center sheet 42, moreover, it may be manufactured in a manner reverse to the order of procedure described in connection with the above embodiment.
1. A memory card, provided with an IC chip and constructed with a plurality of sheets, comprising:
an IC module (14) including said IC chip (18; 20) and a plurality of external connecting terminals (22);
a first laminated structure formed of a plurality of sheets (68, 54, 46) laminated to each other and having a plurality of holes (72, 66, 52) for exposing said external connecting terminals (22) of said IC module (14) to the outside; and
a second laminated structure formed of a plurality of sheets (48, 56, 70) laminated to each other;
wherein the first and second laminated structures are, except for said holes (72, 66, 52) in the first structure, vertically symmetrical with respect to each other concerning the number of sheets and adhesive-agent layers and the respective materials of the sheets;
characterized in that
said IC module (14) comprises a circuit board (24) on which said IC chip (18; 20) and said external connecting terminals (22) are mounted;
a center sheet (42) having a cavity (40) for accomodating said circuit board (24) is provided;
said first laminated structure is bonded to one side surface of said center sheet (42), and said second laminated structure is bonded to the other side surface of said center sheet (42);
each of the sheets (68, 54, 46 and 48, 56 70) has substantially the same plane size as that of said center sheet (42); and
the first and second laminated structures as well as the center sheet are formed so that the card is of uniform thickness in spite of the provision of the IC module within the card.
2. The memory card according to claim 1,
characterized in that an opening (58, 60) is formed on at least one of said sheets (68, 54, 46 and 48, 56, 70) of both said first and second laminated structures so as to correspond to said IC chip (18; 20) of said IC module (14) accomodated in said cavity (40) of said center sheet (42), and a metal member (62, 64) is located in the opening (58, 60).
3. The memory card according to claim 2, wherein the number of said sheets (68, 54, 46 and 48, 56, 70) of both said first and second laminated structures is three.
4. The memory card according to claim 1, comprising:
a metal layer (62, 64) having a little larger area than that of said IC chip (18; 20) and mounted in said both first and second laminated structures at portions thereof only corresponding to said IC chip (18; 20) so as to cover one and the other side surfaces of said IC chip (18; 20) of said IC module (14) accomodated in said cavity (40) of said center sheet (42).
5. The memory card according to claim 4,
characterized in that another IC chip (18 or 20) is mounted on said circuit board (24).
6. The memory card according to claim 5,
characterized in that the two IC chips (18, 20) mounted on said circuit board (24) are located in portions near opposite side edges of said memory card, respectively.
1. Carte à mémoire munie d'une puce d'IC et construite avec une pluralité de feuilles, comprenant :
un module d'IC (14) incluant ladite puce d'IC (18 ; 20) et une pluralité de bornes de connexion externes (22) ;
une première structure laminée constituée par une pluralité de feuilles (68, 54, 46) laminées les unes sur les autres et comportant une pluralité de trous (72, 66, 52) pour exposer lesdites bornes de connexion externes (22) dudit module d'IC (14) à l'extérieur ; et
une seconde structure laminée constituée par une pluralité de feuilles (48, 56, 70) laminées les unes sur les autres ;
dans laquelle les première et seconde structures laminées sont verticalement symétriques l'une par rapport à l'autre à l'exception desdits trous (72, 66, 52) ménagés dans la première structure, en ce qui concerne le nombre de feuilles et de couches d'agent adhésif ainsi que les matériaux respectifs des feuilles ;
caractérisée en ce que :
ledit module d'IC (14) comprend une plaquette de circuit imprimé (24) sur laquelle ladite puce d'IC (18 ; 20) et lesdites bornes de connexion externes (22) sont montées ;
une feuille centrale (42) comportant une cavité (40) pour l'adaptation de ladite plaquette de circuit imprimé (24) est prévue ;
ladite première structure laminée est liée à une surface latérale de ladite feuille centrale (42) et ladite seconde structure laminée est liée à l'autre surface latérale de ladite feuille centrale (42) ;
chacune des feuilles (68, 54, 46 et 48, 56, 70) présente sensiblement la même taille en plan que celle de ladite feuille centrale (42) ; et
les première et seconde structures laminées ainsi que la feuille centrale sont formées de telle sorte que la carte présente une épaisseur uniforme en dépit du positionnement du module d'IC dans la carte.
2. Carte à mémoire selon la revendication 1, caractérisée en ce qu'une ouverture (58, 60) est formée sur au moins l'une desdites feuilles (68, 54, 46 et 48, 56, 70) à la fois desdites première et seconde structures laminées de manière à correspondre à ladite puce d'IC (18 ; 20) dudit module d'IC (14) adaptée dans ladite cavité (40) de ladite feuille centrale (42), et un élément métallique (62, 64) est positionné dans l'ouverture (58, 60).
3. Carte à mémoire selon la revendication 2, dans laquelle le nombre desdites feuilles (68, 54, 46 et 48, 56, 70) à la fois desdites première et seconde structures laminées est de trois.
4. Carte à mémoire selon la revendication 1, comprenant : une couche métallique (62, 64) qui présente une aire légèrement plus grande que celle de ladite puce d'IC (18 ; 20) et qui est montée à la fois dans lesdites première et seconde structures laminées en des parties de celles-ci qui correspondent seulement à ladite puce d'IC (18 ; 20) de manière à recouvrir l'une et l'autre des surfaces latérales de ladite puce d'IC (18 ; 20) dudit module d'IC (14) adapté dans ladite cavité (40) de ladite feuille centrale (42).
5. Carte à mémoire selon la revendication 4, caractérisée en ce qu'une autre puce d'IC (18 ou 20) est montée sur ladite plaquette de circuit imprimé (24).
6. Carte à mémoire selon la revendication 5, caractérisée en ce que les deux puces d'IC (18, 20) montées sur ladite plaquette de circuit imprimé (24) sont positionnées respectivement en des parties voisines de bords latéraux opposés de ladite carte à mémoire.
1. Speicherkarte, mit einem IC-Chip versehen und aus einer Vielzahl von Lagen aufgebaut, folgendes umfassend:
ein IC-Modul (14) mit dem IC-Chip (18; 20) und einer Vielzahl von äußeren Verbindungsanschlüssen (22);
einen ersten Schichtaufbau, der aus einer Vielzahl von Lagen (68, 54, 46) gebildet ist, welche aufeinander geschichtet sind und eine Vielzahl von Öffnungen (72, 66, 52) zum Freilegen der äußeren Verbindungsanschlüsse (22) des IC-Moduls (14) gegenüber der äußeren Umgebung aufweisen; und
einen zweiten Schichtaufbau, der aus einer Vielzahl von Lagen (48, 56, 70) gebildet ist, welche aufeinander geschichtet sind;
worin der erste und der zweite Schichtaufbau, mit Ausnahme der Öffnungen (72, 66, 52) in dem ersten Aufbau, bezüglich der Anzahl von Lagen und Klebstoffschichten und dem jeweiligen Material der Lagen, vertikal zueinander symmetrisch sind,
dadurch gekennzeichnet, daß das IC-Modul (14) eine Leiterplatte (24) umfaßt, auf der der IC-Chip (18; 20) und die äußeren Verbindungsanschlüsse (22) angeordnet sind;
daß eine Mittellage (42) mit einer Ausnehmung (40) zur Aufnahme der Leiterplatte (24) vorgesehen ist;
daß der erste Schichtaufbau an einer Seitenfläche der Mittellage (42) befestigt ist, und der zweite Schichtaufbau an der anderen Seitenfläche der Mittellage (42) befestigt ist;
daß jede der Lagen (68, 54, 46 und 48, 56, 70) im wesentlichen dieselbe Ebenengröße wie die der Mittellage (42) hat; und
daß der erste und der zweite Schichtaufbau sowie die Mittellage so ausgebildet sind, daß die Karte trotz der Tatsache, daß das IC-Modul innerhalb der Karte angeordnet ist, gleichförmig dick ist.
2. Speicherkarte gemäß Anspruch 1,
dadurch gekennzeichnet, daß eine Öffnung (58, 60) auf mindestens einer der Lagen (68, 54, 46 und 48, 56, 70) der beiden ersten und zweiten Schichtaufbauten ausgebildet ist, damit sie dem IC-Chip (18; 20) des in der Ausnehmung (40) der Mittellage (42) angeordneten IC-Moduls (14) entspricht, und ein Metallteil (62, 64) sich in der Öffnung (58, 60) befindet.
3. Speicherkarte gemäß Anspruch 2, worin die Anzahl dieser Lagen (68, 54, 46 und 48, 56, 70) der beiden ersten und zweiten Schichtaufbauten drei ist.
4. Speicherkarte gemäß Anspruch 1, folgendes umfassend:
eine Metallschicht (62, 64) mit einem geringfügig größeren Bereich als derjenige des IC-Chips (18; 20) und angeordnet in sowohl dem ersten als auch dem zweiten Schichtaufbau an Abschnitten davon, die nur dem IC-Chip (18; 20) entsprechen, damit sie die eine und die andere Seitenfläche des IC-Chips (18; 20) des in der Ausnehmung (40) der Mittellage (42) angeordneten IC-Moduls (14) abdecken.
5. Speicherkarte gemäß Anspruch 4, dadurch gekennzeichnet, daß ein weiterer IC-Chip (18 oder 20) auf der Leiterplatte (24) angeordnet ist.
6. Speicherkarte gemäß Anspruch 5, dadurch gekennzeichnet, daß die beiden auf der Leiterplatte (24) angeordneten IC-Chips (18, 20) jeweils in Abschnitten nahe den gegenüberliegenden Seitenkanten der Speicherkarte angeordnet sind.