ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORS......................
J
DIM360 Ver 2.15 (14 Jul 2008) - 1100000/0
2145729
EUROPEAN PATENT APPLICATION
A1
20100120
EP
08381024.2
20080717
es
en
en
20100120
201003
20100120
201003
B24B 9/00 20060101AFI20090130BHEP
B24B 9/06 20060101ALI20090130BHEP
B28B 11/18 20060101ALI20090130BHEP
B28D 7/04 20060101ALI20090130BHEP
B65G 47/244 20060101ALI20090130BHEP
de
Maschine zur Vereinheitlichung von Fliesenprofile
en
Machine for unifying tile profiles
fr
Machine pour unifier le profil de carrelages
none
Maincer, S.L.
08261330
20081440
C/ Asturias, 4 Pol. Ind. El Colador
12200 Onda
ES
Vigil Fernandez, Francisco
C/ Asturias, 4 Pol. Ind. El Colador
12200 Onda (Castellón)
ES
Esteban Perez-Serrano, Maria Isabel
00158882
UDAPI & ASOCIADOS Explanada, 8
28040 Madrid
ES
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MT
NL
NO
PL
PT
RO
SE
SI
SK
TR
AL
BA
MK
RS
A machine for unifying profiles which is situated following firing of the tiles and prior to their classification, and is provided with a dry calibration line which simultaneously calibrates the two parallel sides of the tiles, using diamond grinders.

OBJECT OF THE INVENTION
This invention refers to a machine for unifying tile profiles, which functions in dry conditions without water, following firing of the tiles and prior to their classification.

BACKGROUND TO THE INVENTION
The same applicant has also filed an application for patent no. 200700372 which describes a rectifying machine for tiles.
Tiles are rectified prior to placing them in the furnace so that problems of rectification of fired tiles are eliminated, as are the need for energy required due to the hardness of the tiles and the water required to clean up the clay which forms.
The present invention includes a stage following rectification, in which the profiles are unified following firing, which is materialised in a dry calibration line.

DESCRIPTION OF THE INVENTION
This invention resolves the problem of unifying profiles without the need to use large amounts of energy or water.
The profile unification machine which is the object of the invention functions in a dry state, and is situated following firing of the tiles and prior to their classification, and is provided with a dry calibration line which simultaneously calibrates the two parallel sides of the tiles, using diamond grinders.
In order to unify the four sides of a tile two machines are placed in line, between which a tile rotator is situated, and a squarer at the entry of the second machine, thus giving rise to a tile profile unification system.

DESCRIPTION OF THE DRAWINGS
The present descriptive report is complemented by a set of plans illustrating a preferred embodiment of the invention, but which is in no way restrictive.
Figure 1 shows an example of a rectifying system representing the machine of the invention.

PREFERRED EMBODIMENT OF THE INVENTION
In this example of an embodiment a continuous process unifying profiles for tiles is carried out.
In order for the unification of the tile profiles to be complete, two machines (1) of the invention are placed in line, and between these a rotator (2) is placed in order to vary the part's position by 90°, from the first machine to the second, and a squarer (3) at the entry of the second machine, in order to ensure that the entry of the tile in the second machine is made with a perfect square.
In this example of an embodiment, the rectifying machine (1) of the invention is made from a varnished steel chassis. Said chassis is provided with height regulation.
In order to place the tile on track through the machines, entry guides are shown with an opening and closing system on the central axis of the machine and lateral translation.
In maximum cutting it is 5 to 6 tenths of a millimetre on each side of the part.
The parts are transported by means of toothed belts with a linatex surface.
The machine is provided with four 6.5 CV - 3000RPM at 50Hz, two on each side, with cup type diamond grinders.
Transmission takes place through a geared motor with elastic connection, toothed pulleys and a grooved axis which permits opening and closure of the pulleys.
The machine (1) is also provided with a lateral translation arrangement of belts and motors which enables the belts to be opened and closed for the adjustment to be made in the gears.
The machines (1) in this invention are provided with aspiration openings for the dust created during rectification, and an electric control panel for safety management, according to European Community regulations.
The second machine (1) is similar to the first, with a squaring system (3) which enables parts to be introduced into the 90° rotating process of the side on which the part is pushed into the interior of the machine.
The essential nature of this invention is not altered by any variations in materials, form, size and arrangement of its component elements, which are described in a non-restrictive manner, with this being sufficient to proceed to its reproduction by an expert.
1. Machine (1) for unifying profiles which can be used dry, characterised in that it simultaneously calibrates the two parallel sides of the tile, using diamond grinders.
2. System for unifying tile profiles characterised in that in order to unify the four sides of a tile two machines (1) are placed according to claim 1 in line, between which a tile rotator (2) is situated , and a squarer (3) at the entry to the second machine.

REFERENCES CITED IN THE DESCRIPTION
This list of references cited by the applicant is for the reader's convenience only. It does not form part of the European patent document. Even though great care has been taken in compiling the references, errors or omissions cannot be excluded and the EPO disclaims all liability in this regard.

Patent documents cited in the description
- WO
200700372
A
[0002]