ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIRO..CY..TRBGCZEEHUPLSK..HRIS..MTNO........................
*
J
DIM360 Ver 2.15 (14 Jul 2008) - 2100000/0
2201633
EUROPEAN PATENT SPECIFICATION
B1
20121031
EP
08806410.0
20080925
20100423
en
en
en
0718761
20070926
GB
20121031
201244
20100630
201026
20121031
201244
20120522
H01M 8/04 20060101AFI20100428BHEP
F16K 11/10 20060101ALI20100428BHEP
de
BRENNSTOFFZELLENSYSTEM MIT KATHODENAUSRÄUMUNG BEIM HERUNTERFAHREN
en
FUEL CELL SYSTEM WITH CATHODE PURGE UPON SHUT-DOWN
fr
Système de pile à combustible avec une purge cathodique lors de l'arrêt
WO-A-00/65676
WO-A-97/48142
WO-A-2004/051779
DE-B3-102005 031 422
JP-A- 2003 317 754
US-A- 3 394 723
12185536.5
20120921
ADCOCK, Paul
27 West End Long Whatton
Loughborough, Leics LE12 5DW
GB
HOOD, Peter, David
1026 Melton Road
Syston, Leicester LE7 2NN
GB
BAIRD, Scott
55 Rufford Avenue
Bramcote, Nottingham NG9 3JG
GB
Intelligent Energy Limited
101298815
INTEJ/P41741EP
Charnwood Building Holywell Park Ashby Road Loughborough
Leicestershire LE11 3GB
GB
Charig, Raymond Julian
100038459
Potter Clarkson LLP Park View House 58 The Ropewalk
Nottingham NG1 5DD
GB
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MT
NL
NO
PL
PT
RO
SE
SI
SK
TR
GB2008003256
20080925
en
WO2009040535
20090402
200914

Field of the Invention
The invention relates to the operation of, and apparatus relating to, a fuel cell system, and in particular though not exclusively to a strategy for shutting down a fuel cell system.

Background
Water is integral to the operation of a fuel cell system, for example in the form of the system described herein comprising a fuel cell stack based around a proton exchange membrane (PEM). Reaction of protons (hydrogen ions) conducted through the PEM from an anode flow path, with oxygen present in a cathode flow path, produces water. Excess water needs to be removed from the fuel cell stack to avoid flooding and causing a consequent deterioration in performance. An amount of water, however, needs to be present in at least the cathode flow path to maintain hydration of the PEM, so as to achieve optimum performance of the fuel cell. Managing this water, by deliberate injection and removal, can also provide a useful mechanism for removing excess heat from the fuel cell stack.
To optimise performance, water can be employed deliberately in such fuel cell systems through injection into the cathode flow path of the stack. Such water injection fuel cell systems have potential advantages of reduced size and complexity, as compared with other types of fuel cell systems employing separate cooling channels. Water may be injected directly into the cathode flow path through water distribution manifolds, as for example described in GB2409763.
For water injection systems, it is important that any water fed back into the cathode flow path is of high purity, so as to avoid contamination of the PEM and consequent degradation of stack performance. This requirement for high purity, however, means that additives to lower the freezing point of water cannot be used. For automotive applications in particular, typical requirements include starting up from below freezing, typically as low as -20°C to replicate environments in which the fuel cell may be used in practice. Since high purity water has a freezing point of 0°C (at 1 bar pressure), any water left in the fuel cell system will, given sufficient time, freeze after shut-down of the fuel cell.
Ice in the fuel cell system, and in particular within the cathode flow path, can prevent the stack from operating properly, or even at all. If any part of the cathode flow path is blocked with ice, air cannot be passed through the cathode and the fuel cell may not be capable of self-heating to above freezing point. Other methods of heating the whole stack will then be necessary, which will require consumption of external power before the fuel cell can begin supplying electrical power and heat by itself.
A purging operation can be used on shut-down of a fuel cell stack, such as that described in US 6479177. This document discloses a fuel cell stack having water cooling passages separate from the cathode flow path. A pressurised dry nitrogen feed is used to purge water from the stack before allowing the temperature of the stack to fall below freezing. This method, however, requires a supply of pressurised nitrogen, which might not be available or even desirable in an automotive environment.
It is an object of the invention to address one or more of the above mentioned problems.

Summary
The present invention provides a reverse flow relief valve according to claim 1. Also described herein is a method of shutting down operation of a fuel cell system comprising a fuel cell stack, the method comprising the sequential steps of: i) ceasing a supply of fuel to the fuel cell stack; ii) closing a shut-off valve on an exhaust line in fluid communication with a cathode system of the fuel cell system, the cathode system comprising a cathode fluid flow path passing through the fuel cell stack; iii) pressurising the cathode system with an air compressor in fluid communication with a cathode air inlet port in the fuel cell stack; and iv) ejecting water from the cathode flow path.
Also described herein is a fuel cell system comprising:
- a fuel cell stack;
- a cathode system having a cathode fluid flow path comprising a cathode air inlet line, a cathode volume within the fuel cell stack and a cathode exit line connected in series and configured to allow passage of air through the fuel cell stack;
- an air compressor in fluid communication with the cathode air inlet line;
- a thermally insulated containment vessel configured to receive water through a water return line from the cathode flow path,
- wherein the fuel cell system is configured to eject water from the cathode flow path into the containment vessel through the water return line upon shutting down operation of the system.
Also described herein is a reverse flow relief valve comprising:
- a first feed port;
- a second feed port;
- a non-return valve within a main fluid passage extending between the first and second feed ports, the non-return valve configured to allow fluid to pass from the first to the second feed ports and to block passage of fluid in the reverse direction;
- a bypass fluid passage in fluid communication with the main fluid passage;
- a sealing valve biased against an end of the bypass passage between the bypass passage and a purge port,
- wherein the sealing valve is configured to maintain a seal against the bypass passage when fluid pressure in the first feed port exceeds fluid pressure at the second feed port to prevent fluid flow from the main fluid passage to the purge port through the bypass fluid passage, and to allow fluid flow from the second feed port to the purge port through the bypass fluid passage when fluid pressure at the second feed port exceeds fluid pressure at the first feed port.
Also described herein is a fuel cell system comprising:
- a fuel cell stack;
- a cathode system having a cathode fluid flow path comprising a cathode air inlet line, a cathode volume within the fuel cell stack and a cathode exit line connected in series and configured to allow passage of air through the fuel cell stack;
- a heat exchanger connected in series with a water separator to the cathode exit line of the cathode fluid flow path,
- wherein a water ejection outlet line of the water separator is connected to a water containment vessel by a first water return line.

Brief Description of the Drawings
The invention will now be described by way of example only, and with reference to the appended drawings in which:
- figure 1 illustrates a schematic diagram of the arrangement of various components within an overall fuel cell system;
- figure 2 illustrates a schematic diagram of an exemplary water containment vessel;
- figure 3 illustrates a cutaway perspective view of an exemplary reverse flow relief valve;
- figures 4a and 4b illustrate schematically the operation of the reverse flow relief valve of figure 3; and
- figures 5a and 5b illustrate schematically two alternative configurations for cathode exit stream liquid separation.

Detailed Description
Figure 1 shows a schematic diagram of an exemplary fuel cell system 100 comprising a fuel cell stack 110 and other associated components. The fuel cell stack 110 has a cathode flow path passing through it, the cathode flow path comprising an air inlet 124 leading to an air inlet line 123 and into the stack at the cathode air inlet 126. After passing through an internal cathode volume (not shown) within the fuel cell stack 110, the cathode flow path exits the fuel cell stack 110 into the cathode exit line 121, through the cathode exhaust line 122 and an exhaust shut-off valve 120. During normal operation, the exhaust shut-off valve 120 is partially or fully open. Various components such as a heat exchanger 130, with associated cooling fan 139, and a water separator 131 may be connected to or part of the cathode exit line 121 and exhaust line 122 in the cathode flow path. Temperature sensors TX1, TX2, TX3, TX5 and pressure sensors PX2, PX3 may also be present, connected at appropriate places to monitor the inlet line 123 and exit line 121 of the cathode flow path.
The expression 'cathode system' in the present context is intended to encompass those parts of the fuel cell system 100 that are associated with the cathode volume within the fuel cell stack. These include the various internal components of the fuel cell such as the inlets, outlets, the internal flow path and water distribution structures, as well as components in fluid communication with the cathode volume such as the various inlet, outlet, recirculation and exhaust lines for both liquids and gases. The term 'cathode flow path' is intended to encompass a subset of the cathode system that includes a fluid flow path from the air inlet 124 through an air compressor 133, the inlet line 123, the cathode volume of the fuel cell stack 110, and the cathode exit line 121. The terms 'anode system' and 'anode flow path' are to be interpreted similarly, with reference to the various components of the fuel cell system 100 associated with the anode volume.
The air compressor 133, connected to the cathode air inlet line 123, provides compressed air to the cathode flow path. Other components such as an air inlet heat exchanger 134, a flow meter 135, one or more air filters 136, 137 and an air heater 138 may be present in the cathode inlet line 123 between the air inlet 124 and the fuel cell stack 110. The air inlet heat exchanger 134 may be used in conjunction with a coolant line 141, a three-way valve 142 and a temperature sensor TX7 to pre-heat air from the air compressor 133 with coolant from the coolant line 141 during operation of the fuel cell system 100. The coolant line 141 passing through the air inlet heat exchanger 134 forms a separate cooling circuit configured to extract heat from the air stream after the compressor 133. This coolant line 141 is preferably operated after the fuel cell stack 110 reaches a normal operating temperature, in order to avoid extracting heat from the air inlet stream in the cathode air inlet line 123 during start-up of the system 100. Diversion of coolant in the line 141 may be achieved through use off the valve 142, allowing control over whether coolant is delivered to the heat exchanger 134. Since the coolant line 141 is separate from water fed into the cathode system, the requirement for high purity water is not the same. The coolant used in the coolant line 141 may therefore comprise additives such as glycol to lower the freezing point of the coolant used.
Fuel, typically in the form of gaseous hydrogen, enters the fuel cell system via a pressure-reducing valve 151 and an actuated valve 152, preferably in the form of a normally-closed solenoid-actuated valve. The fuel supply 150, when in the form of hydrogen gas, is typically located remotely from the fuel cell system, for example in the form of a pressurised tank towards the rear of a vehicle. A further solenoid-actuated valve 153- and a pressure-reducing valve 154 may be provided closer to the fuel cell stack 110 in the fuel inlet line 155 of the anode flow path between the fuel source 150 and the anode inlet 156 of the fuel cell stack 110. Two separate sets of valves are therefore provided leading to the anode inlet 156, one set 151, 152 near to the tank and the other set 153, 154 closer to the fuel cell stack 110, with an intermediate pressurised fuel line.119 in between. The pressure-reducing valve 154 regulates the pressure of the dry fuel gas to a level suitable for introduction to the fuel cell stack 110. The pressure-reducing valve 154 is preferably a passive device which has a preset pressure setting applied, although an actively controlled device may be used. A fuel heater 145 is optionally provided, for example in the pressurised fuel line 119 before the valve 153, as shown in figure 1, or alternatively in the fuel inlet line 155 either before or after the pressure-reducing valve 154.
A further actuated valve 161 is provided on the anode exit line 165. Each actuated valve 152, 153, 161 may be provided with a local heater element to defrost the valve as required, although activation of the valves 152, 153, 161 through passage of current through the solenoid will provide a certain degree of heating. Preferably each of the actuated valves 152, 153, 161 is configured to be fail-safe, i.e. will only open when actuated by current passing though the solenoid.
To monitor and to relieve pressure of fuel within the anode flow path, a pressure sensor PX1 and/or pressure relief valve 157 may be provided. The pressure relief valve 157 is preferably set to open and exhaust fluid from the anode flow path through a pressure relief exhaust line 158 when the pressure in the anode flow path exceeds a safe operating level.
A further manually operable valve 162 in the anode exit line 165 may be present, this valve 162 being for used for example during servicing to ensure depressurisation of the anode flow path. Water build-up in the anode flow path in the fuel cell stack 110 may occur, for example as a result of diffusion of water through the PEM from the cathode side. Consequently, an anode exhaust water separator 163 may be provided in the anode exhaust line 164 to separate any water present in the exhaust line 164. This water can be exhausted or optionally recirculated. During operation of the fuel cell stack 110, the valve 161 is typically held closed, and only opened intermittently to exhaust any built-up water from the anode fluid path.
A cathode water injection inlet 127 is provided in the fuel cell stack 110, the inlet 127 connected to a cathode water injection line 125. The cathode water injection line 125 may be heated along a part or the whole of its length, and extends between a water containment vessel 140 and the cathode water injection inlet 127. A heater 129 may be provided to apply heat to a specific region of the line 125 to heat water passing through the injection line 125 towards the cathode water injection inlet 127. A further pressure sensor PX4 may be provided on the cathode water injection line 125 in order to monitor the back-pressure on the line 125 during operation.
Water from the cathode exit line 121 is pumped with a water pump 132, optionally provided with a heater 143, through a water return line 128 towards the water containment vessel 140, further details of which are provided below with reference to figure 2. Excess water is ejected from the fuel cell system 100 out of the water containment vessel 140 through a water overflow line 144.
Shown in figure 2 is a schematic cross-sectional view of the water containment vessel 140 of figure 1. The vessel 140 comprises a thermally insulating wall 210 and a lid 211, which may also be thermally insulated. Preferably the wall 210 of the vessel 140 is of a double wall construction, having a vacuum or other thermally insulating layer such as air or expanded polystyrene between the two walls. The inner surface 215 of the vessel 210 is preferably made from a material having a resistance to corrosion, such as stainless steel, to prevent contamination of water 212 within the vessel.
The purpose of the lid 211 is to allow connections to the various elements housed within the vessel 140, whilst also maintaining a good degree of insulation. Typically the lid 211 is manufactured from glass-reinforced nylon with an additional layer of insulating foam. Ports in the lid to accommodate passage of the lines 125, 144, 128 are preferably configured such that when the system is shutdown, any residual water runs back into the vessel. This involves using pipe of a suitably large diameter such that beads of water do not form to span the internal bore of the pipe and hang up in the line. Preferably, no fittings are used in the lid so that pipes passing through the lid 211 contain no sharp bends. In a general aspect, therefore, the water injection line 125 extending between the water containment vessel 140 and the cathode water injection inlet 127, and an exhaust line 121, 128 extending between a cathode exit line 121 and the water containment vessel 140 both comprise piping having an internal bore such that beads of water do not span the bore after ejection of water from the cathode system.
A thermostatic heating element 236 within the vessel 140 is provided to maintain the temperature of water 212 within the vessel 140 above freezing point. A level sensor 233 provides a signal indicating the level of water 212 within the vessel. A heater 237 is provided in addition to the thermostatic heating element 236 in order to provide faster heating to defrost the water 212 if frozen. Due to the energy requirement of changing the phase of water from solid to liquid, this heater 237 is typically of a higher power rating than the thermostatic heating element 236, for example around 180W or higher. The thermostatic heater 236 is configured to ensure that the temperature of the water 212 in the vessel 140 remains above a set point. This set point is typically 5°C, in order to prevent the water from freezing. The thermostatic heater 236 may be powered by a 12V battery supply, and set to operate for a prescribed period. Hence, during this period, liquid water in the vessel can be guaranteed. For longer periods at sub-zero ambient temperature, the thermostatic heater 236 is disabled to save on battery power. The water 212 may then freeze, and will require defrosting with the higher power heater 237. The thermostatic heater is typically of a power rating such that a maximum heat output is slightly larger than the maximum rated losses from the vessel. A typical power rating is in the range of 2 to 4 W.
A temperature sensor TX4, preferably comprising a submerged thermistor, is installed in order to allow the temperature of the water 212 in the vessel 140 to be monitored.
An overflow line 144 is provided to eject excess water from the containment vessel if a level of water in the vessel exceeds a preset amount.
Water from the water return line 128 enters the vessel 140 through a filter 234. A pump 230, 231, 240 pumps the water 212 from the vessel 140 through a further filter 214, a reverse flow relief valve 213 and into the cathode water injection line 125. A flow meter 235 is configured to monitor the amount of water passing through the cathode water injection line 125.
The pump is preferably constructed such that a motor portion 231 is located outside the containment volume of the vessel 140 and therefore avoids being in contact directly with water 212 within the vessel. A shaft 240 between the motor 231 and a pump head 230 allows the motor 231 to drive the pump head 230. The pump head, comprising at least the inlet, outlet and impeller, is preferably of a construction such that, after being submerged in frozen water the pump is able to operate again once the water is defrosted. The motor 231 is preferably rated for operation at sub-zero temperatures.
The pump head 230 is located so as to be submerged by water 212 in the vessel 140. This has the advantage of there being no requirement for the pump head 230 to be purged during shutdown or heated during startup, particularly when water 212 is maintained within the flask after shutdown. The pump head 230 is preferably configured to have a small thermal mass. Thawing of any ice within the pump head 230 is achieved via heat transferred from the surrounding water as it defrosts. The pump head 230 is also preferably configured to accommodate expansion due to ice formation. On thawing, the pump head 230 then returns to its original shape without compromising its operation.
The reverse flow relief valve 213 is constructed such that water is allowed to pass from the pump head 230 through the cathode water injection line 125 towards the cathode water injection inlet 127 when the pump is operational, creating a pressure drop across the valve in the direction of flow. However, when the pump is stopped and pressure in the cathode water injection line 125 is increased, the valve 213 allows water to flow back into the vessel 140 through a purge port 238.
The purpose of the reverse flow relief valve 213 is to allow water to be back flushed into the vessel 140 from the fuel cell stack 110 and connecting lines during shutdown of the system 100. Closing the cathode exhaust valve 120 allows water in the fuel cell stack 110 to be forced under pressure from the air compressor 133 back through the cathode water injection inlet 127, out of the stack 110 and through the water injection line 125 towards the water containment vessel 140. However, if a gear pump is used in the containment vessel, without the reverse flow relief valve 213 no water would flow due to the pressure required to push water back through the pump head 230. Therefore, the reverse flow relief valve 213 is configured such that in normal operation it allows water to pass through it from the pump to the fuel cell stack 110. When subjected to a small back pressure (for example in the region of 300mBar.g) when the pump head 230 is not being operated, a diaphragm opens and allows water to flow back into the flask through the purge port 238.
An exemplary embodiment of the reverse flow relief valve 213 is shown in figure 3 in cutaway form. In normal operation, water flows from the containment vessel 140 through the reverse flow relief valve 213 in the directions indicated by arrows 301. Water flows through a first feed port 314, through a non-return valve 316 and out of the valve 213 through a second feed port 320 towards the cathode water injection line 125. The pressure of water in the first feed port 314 is transmitted via a connecting passage 313 and transfer passage 312 to a cavity 311 sealed by a sealing valve, for example in the form of a diaphragm 321, and enclosed by a cover face 323. The pressure maintains a sealing face 317 of the diaphragm 321 against a face of a bypass passage 318, and thus prevents fluid from passing between the second feed port 320 and a low pressure cavity 315 behind the diaphragm 321.
Once the water containment vessel pump 230 is disabled, a loss of pressure in the first feed port 314 and an increase in pressure in the second feed port 320 caused by an increased pressure in the cathode volume of the fuel cell stack 110 causes the non-return valve 316 to close. The increased pressure in the second feed port causes the diaphragm 321, which is preferably composed of a resilient material such as a rubber, to flex and open up a passage between the bypass passage 318 and the low pressure cavity 315. Water is then allowed to flow from the second feed port 320 through the bypass passage 318, into the low pressure cavity 315, through a purge passage 322 and out of the valve 213 through the purge port 238. The overall direction of flow in the reverse direction is indicated by arrows 302.
The configuration of the reverse flow relief valve allows water to be ejected from the cathode volume in the fuel cell stack and the cathode water injection line while allowing the pump head 230 in the containment vessel 140 to remain primed with water.
Provided the water 212 in the vessel is not frozen, the pump head 230 then remains in a state ready to immediately begin pumping water for injection into the cathode volume of the fuel cell stack 110.
Figures 4a and 4b show schematically the two different modes of operation possible with the reverse flow relief valve 213. In figure 4a, the purge operation is shown, in which low pressure air from the fuel cell stack enters the valve 213 through the second feed port 320, and there is no flow into the first feed port 314. This low pressure air causes the diaphragm 321 to deflect and allow flow through the bypass passage 318 and out of the valve through the purge port 238 for delivery to the water reservoir in the water containment vessel 140. The non-return valve 316 prevents flow through to the first feed port 314.
In figure 4b, the water delivery operation of the reverse flow relief valve 213 is shown, in which high pressure water pumped from the reservoir in the water containment vessel 140 enters the valve 213 through the first feed port 314. The pressure, transmitted via the connecting passage 313 to the high pressure cavity 311, maintains the diaphragm 321 in a closed position against the bypass passage 318. Flow of water passes through the non-return valve 316 and out of the reverse flow relief valve 213 via the second feed port 320. No flow occurs through the purge port 238.
Two alternative arrangements of the cathode exit, exhaust and water ejection lines are shown schematically in figures 5a and 5b. In figure 5a, the water separator 131 is connected first in line with the cathode exit line 121, in series with and before the heat exchanger 130, and two water ejection lines 128a, 128b are used to send water via pumps 132a, 132b to the containment vessel 140. In figure 5b, the water separator 131 is connected in series with, but after, the heat exchanger 130, and a single pump 132 is used to pump water through the water return line 128 to the containment vessel 140.
In the configuration of figure 5a, the cathode exit stream is passed through the cathode exit line 121 to a cyclonic water separator 131, which removes the liquid content before redirecting saturated air to a heat exchanger 130. The heat exchanger 130 cools the saturated air stream, which results in a proportion of the entrained water changing to liquid phase. Two pumps 132a, 132b are used to transfer recovered water to the containment vessel 140, one pump 132a connected via water return line 128a to the base of the separator 131 and the other 132b connected via water return line 128b to the heat exchanger 130 exit manifold box. During normal fuel cell operation the variable shut off valve 120 is held open. However, during fuel cell system shutdown, this valve is closed to back pressure the cathode flow path. In this case the compressor 133 (or other device which supplies air to the fuel cell according to a defined flow rate set point) works harder to maintain a fixed air flow rate. The separator 131 contains a pressure relief valve (not shown) which, during this back pressured shutdown phase, opens allowing ejection of water from the water separator 131 through a water purge line 510 (typically to atmosphere). Prior to back pressuring the cathode flow path at system shutdown, the pump 132a is typically allowed to run for a few seconds to clear most of the water from the separator 131.
In the configuration of figure 5b, operation is similar to that of figure 5a, except that the cyclonic separator 131 is positioned after the heat exchanger 130. As such, the liquid element of the cathode exit stream is passed through the heat exchanger 130. In addition, only one pump 132 is required to transfer the recovered water back to the containment vessel 140. One advantage of this configuration is that as the inlet to the heat exchanger 130 is part way from the bottom, any residual water that remains in the heat exchanger 130 after shutdown will fall to occupy the lower part of the heat exchanger 130. In the event of the heat exchanger 130 then being subjected to sub-zero temperature, this water will freeze. However, flow will still be possible through the cathode flow path through the rest of the heat exchanger, which will then heat up and defrost the frozen water in the lower part.
The purge port 510 in each case allows the cyclonic separator to be cleared dry, allowing subsequent storage at low temperatures.
Preferably, the thermal inertia of the cyclonic separator 131 is low such that when a small amount of liquid water enters the separator when the separator 131 is below 0°C, the liquid water does not freeze.
Optionally, a pressure relief valve may be used to increase the back pressure of the system to such an extent that the transfer pumps 132, 132a, 132b are not required.
However, in this instance the cyclonic relief valve and purge port 510 might not be fitted, to ensure that the internal pressure in the cathode water exit line 121 forces water through the water ejection line towards the water containment vessel 140. If no transfer pump 132 is fitted, the arrangement shown in figure 5b is more preferable, to ensure that water ejected from the cathode exit line passes through a single water ejection line 128.
During operation of the fuel cell system 100 (with reference to figures 1 and 2), water from the containment vessel 140 is pumped through the cathode flow path via the cathode water injection line 125 and the cathode water injection inlet 127. After passing through the cathode volume within the fuel cell stack 110, water passes out of the stack 110 via the cathode water exit line 121 and into the heat exchanger 130. A mixture of exhaust gas and condensed water passes through the water separator 131. Condensed water then passes through the water return line 128 and into the water containment vessel 140. Any excess water is ejected through the water overflow line 144. Exhaust gases are ejected through the exhaust shut-off valve 120, which is held at least partially open to control the pressure within the cathode flow path.
With reference to figure 1, fuel gas is fed into the anode inlet 156 and into the anode volume (not shown) within the fuel cell stack 110. Valves 153, 161 are operated to maintain a desired pressure within the anode volume. The manual valve 162 connected to the anode outlet 159 remains closed. Optionally, water ejected from the anode exhaust stream is separated into liquid and gas phases with a further water separator 163.
On shutdown of the fuel cell system 100, the fuel supply to the fuel cell stack 110 is first shut off by closing the solenoid actuated valve 153 on the fuel supply line 155. The shut-off valve 120 on the cathode exhaust line 122 is then closed, while the air compressor 133 continues operation. In practice a time may be required to flush through the cathode flow path with air before the shut-off valve 120 is closed. The pressure in the cathode flow path then rises. The water ejection line pump 132, if present, preferably continues operation for a time after the shut-off valve is closed, to allow water to continue passing through to the containment vessel 140. The containment vessel pump 230 ceases operation, and water consequently stops being fed into the cathode water injection line 125.
A short purging operation of the anode flow path may also be used during shutdown to eject water present in the anode flow path, with water being forced through opened anode exit valve 161, followed by depressurisation of the anode volume in the fuel cell stack 110.
Air being flushed through the cathode flow path forces residual water out of the cathode volume in the fuel cell stack 110 and through the cathode exit line 121, through the heat exchanger 130 to the water separator 131. The pump 132 pumps water from the separator 131 through the water return line 128 and into the water containment vessel 140. When the shut-off valve 120 closes the cathode air pressure will rise, forcing water out of the cathode volume in the fuel cell stack 110 through the cathode water injection inlet 127 and through the cathode water injection line 125 and the purge port 23 8 of the reverse flow relief valve 213 towards the water containment vessel 140.
The ability to purge water from the cathode flow path through to the water containment vessel 140 allows water, which may be trapped in internal features and water distribution galleries, to be removed. For a typical size of fuel cell stack for automotive applications, this may result in around 30ml of water being removed from the cathode flow path. The use of the air compressor 133 rather than a nitrogen purge feed reduces the number of components required and avoids excessive drying out of the fuel cell stack. The membranes in the stack can then be kept in a more suitable state for a subsequent start-up operation. Timed operation of the air compressor on shutdown can be optimised to provide a balance between removing sufficient water to prevent adverse effects from sub-zero conditions and dehydration of the membranes. For a typical fuel cell system, the air compressor may be operated around 1 to 2 minutes after closing the exhaust valve 120. Hydrogen gas may also be used to purge excess water from the anode flow path.
Other embodiments of the invention are intended to be within the scope of the invention, as defined by the appended claims.
1. A reverse flow relief valve (213) comprising:
a first feed port (314);
a second feed port (320);
a non-return valve (316) within a main fluid passage extending between the first and second feed ports, the non-return valve configured to allow fluid to pass from the first to the second feed ports and to block passage of fluid in the reverse direction;
a bypass fluid passage (318) in fluid communication with the main fluid passage;
a sealing valve (317, 321) biased against an end of the bypass passage (318) between the bypass passage and a purge port (238),
wherein the sealing valve (317, 321) is configured to maintain a seal against the bypass passage (318) when fluid pressure in the first feed port (314) exceeds fluid pressure at the second feed port (320) to prevent fluid flow from the main fluid passage to the purge port (238) through the bypass fluid passage (318), and to allow fluid flow from the second feed port to the purge port through the bypass fluid passage when fluid pressure at the second feed port exceeds fluid pressure at the first feed port.
2. The reverse flow relief valve of claim 1 wherein the sealing valve (317, 321) is configured to allow fluid flow from the second feed port (320) to the purge port (238) through the bypass fluid passage (318) when fluid pressure at the second feed port exceeds fluid pressure at the first feed port by a predetermined amount.
3. The reverse flow relief valve of claim 2 wherein the predetermined amount is no less than 300 mbar.
4. The reverse flow relief valve of any one of claims 1 to 3 wherein the sealing valve comprises a resilient diaphragm (321), one face of which is in fluid communication with the first feed port (314), an opposing second face (317) of the diaphragm being biased against the end of the bypass passage (318).
5. The reverse flow relief valve of any one of claims 1 to 4 comprising a connecting fluid passage (313) extending between the first feed port (314) and the sealing valve (321).
6. A fuel cell system comprising the reverse flow relief valve of any one of claims 1 to 5 wherein the second feed port (320) of the reverse flow relief valve is connected to a cathode water injection line (125), the first feed port (314) is connected to a pump (230) and the purge port (238) is in fluid communication with an interior volume of a water containment vessel (140).
7. The fuel cell system of claim 6 further comprising:
a fuel cell stack (110);
a cathode system having a cathode fluid flow path comprising a cathode air inlet line (123), a cathode volume within the fuel cell stack and a cathode exit line (121) connected in series and configured to allow passage of air through the fuel cell stack (110);
a heat exchanger (130) connected in series with a water separator (131) to the cathode exit line (121) of the cathode fluid flow path,
wherein a water ejection outlet line (128) of the water separator (131) is connected to the water containment vessel (140) by a first water return line (128a).
8. The fuel cell system of claim 7 wherein a water ejection outlet of the heat exchanger (130) is connected to the water containment vessel (140) by a second water return line (128b).
9. The fuel cell system of claim 8 comprising a water pump (132a, 132b) in each of the first and second water return lines.
10. The fuel cell system of claim 6 further comprising:
a fuel cell stack (110);
a cathode system having a cathode fluid flow path comprising a cathode air inlet line (123), a cathode volume within the fuel cell stack and a cathode exit line (121) connected in series and configured to allow passage of air through the fuel cell stack;
an air compressor (133) in fluid communication with the cathode air inlet line (123);
wherein said water containment vessel (140) is thermally insulated and configured to receive water through a water return line (128) from the cathode flow path,
wherein the fuel cell system is configured to eject water from the cathode flow path into the containment vessel (140) through the water return line (128) upon shutting down operation of the system.
11. The fuel cell system of claim 10 wherein the containment vessel (140) is fluidly connected to the cathode water injection line (125), the cathode water injection line further comprising a cathode water injection inlet (127) in the fuel cell stack (110), the water injection line (125) being configured to allow passage of water from the cathode volume of the fuel cell stack into the containment vessel (140) via the reverse flow relief valve (213) configured to allow passage of water from the cathode flow path into the containment vessel when a pressure difference across the valve is reversed from that during operation of the fuel cell system.
1. Ein Rückström-Entlastungsventil (213) mit:
einem ersten Einspeisungsanschluss (314),
einem zweiten Einspeisungsanschluss (320),
einem Rückschlagventil (316) in einem Fluid-Hauptdurchgang, der sich zwischen dem ersten und dem zweiten Einspeisungsanschluss erstreckt, wobei das Rückschlagventil so konfiguriert ist, dass es Fluid von dem ersten zu dem zweiten Einspeisungsanschluss passieren lässt und das Passieren von Fluid in umgekehrter Richtung blockiert,
einem Fluid-Bypassdurchgang (318), welcher mit dem Fluid-Hauptdurchgang in Fluidverbindung steht,
einem Abdichtungsventil (317,321), welches gegen ein Ende des Bypassdurchgangs (318) zwischen dem Bypassdurchgang und einem Spülanschluss (238) vorbelastet ist,
wobei das Abdichtungsventil (317,321) so konfiguriert ist, dass es eine Abdichtung gegenüber dem Bypassdurchgang (318) beibehält, wenn Fluiddruck in dem ersten Einspeisungsanschluss (314) den Fluiddruck an dem zweiten Einspeisungsanschluss (320) übersteigt, um Fluidströmung von dem Fluid-Hauptdurchgang zu dem Spülanschluss (238) durch den Fluid-Bypassdurchgang (318) zu verhindern und um Fluidströmung von dem zweiten Einspeisungsanschluss zu dem Spülanschluss durch den Fluid-Bypassdurchgang zuzulassen, wenn Fluiddruck an dem zweiten Einspeisungsanschluss Fluiddruck an dem ersten Einspeisungsanschluss übersteigt.
2. Das Rückström-Entlastungsventil gemäß Anspruch 1, wobei das Abdichtungsventil (317,321) so konfiguriert ist, dass es Fluidströmung von dem zweiten Einspeisungsanschluss (320) zu dem Spülanschluss (238) durch den Fluid-Bypassdurchgang (318) zulässt, wenn Fluiddruck an dem zweiten Einspeisungsanschluss Fluiddruck an dem ersten Einspeisungsanschluss um ein vorbestimmtes Maß übersteigt.
3. Das Rückström-Entlastungsventil gemäß Anspruch 2, wobei das vorbestimmte Maß nicht weniger als 300mbar beträgt.
4. Das Rückström-Entlastungsventil gemäß einem der Ansprüche 1 bis 3, wobei das Abdichtungsventil ein elastisches Diaphragma (321) umfasst, wobei eine Fläche davon mit dem ersten Einspeisungsanschluss (314) in Fluidverbindung steht, und eine entgegengesetzte zweite Fläche (317) des Diaphragmas gegen das Ende des Bypassdurchgangs (318) vorbelastet ist.
5. Das Rückström-Entlastungsventil gemäß einem der Ansprüche 1 bis 4, mit einem Fluid-Verbindungsdurchgang (313), der sich zwischen dem ersten Einspeisungsanschluss (314) und dem Abdichtungsventil (321) erstreckt.
6. Ein Brennstoffzellensystem mit dem Rückström-Entlastungsventil gemäß einem der Ansprüche 1 bis 5, wobei der zweite Einspeisungsanschluss (320) des Rückström-Entlastungsventils mit einer Kathodenwassereinspritzleitung (125) verbunden ist, der erste Einspeisungsanschluss (314) mit einer Pumpe (230) verbunden ist, und der Spülanschluss (238) mit einem Innenvolumen eines Wasseraufnahmegefäßes (140) in Fluidverbindung steht.
7. Das Brennstoffzellensystem gemäß Anspruch 6 ferner mit:
einem Brennstoffzellenstack (110),
einem Kathodensystem mit einem Kathodenfluidströmungsweg mit einer Kathodenlufteinlassleitung (123), einem Kathodenvolumen innerhalb des Brennstoffzellenstacks und einer Kathodenauslassleitung (121), welche seriell verbunden und derart konfiguriert sind, dass sie das Passieren von Luft durch den Brennstoffzellenstack (110) zulassen,
einem Wärmetauscher (130), der seriell mit einem Wasserseparator (131) mit der Kathodenauslassleitung (121) des Kathodenfluidströmungswegs verbunden ist,
wobei eine Wasserausspritzauslassleitung (128) des Wasserseparators (131) über eine erste Wasserrückführleitung (128a) mit dem Wasseraufnahmegefäß (140) verbunden ist.
8. Das Brennstoffzellensystem gemäß Anspruch 7, wobei ein Wasserausspritzauslass des Wärmetauschers (130) über eine zweite Wasserrückführleitung (128b) mit dem Wasseraufnahmegefäß (140) verbunden ist.
9. Das Brennstoffzellensystem gemäß Anspruch 8 mit einer Wasserpumpe (132a,132b) in jeder der ersten und zweiten Wasserrückführleitungen.
10. Das Brennstoffzellensystem gemäß Anspruch 6 ferner mit:
einem Brennstoffzellenstack (110),
einem Kathodensystem mit einem Kathodenfluidströmungsweg mit einer Kathodenlufteinlassleitung (123), einem Kathodenvolumen innerhalb des Brennstoffzellenstacks und einer Kathodenauslassleitung (121), welche seriell miteinander verbunden und derart konfiguriert sind, dass sie das Passieren von Luft durch den Brennstoffzellenstack zulassen,
einem Luftkompressor (133), welcher mit der Kathodenlufteinlassleitung (123) in Fluidverbindung steht,
wobei das Wasseraufnahmegefäß (140) thermisch isoliert und so konfiguriert ist, dass es Wasser durch eine Wasserrückführleitung (128) von dem Kathodenströmungsweg aufnimmt,
wobei das Brennstoffzellensystem so konfiguriert ist, dass es Wasser aus dem Kathodenströmungsweg in das Aufnahmegefäß (140) durch die Wasserrückführleitung (128) nach dem Herunterfahren des Systems ausspritzt.
11. Das Brennstoffzellensystem gemäß Anspruch 10, wobei das Aufnahmegefäß (140) mit der Kathodenwassereinspritzleitung (125) fluidmäßig verbunden ist, wobei die Kathodenwassereinspritzleitung ferner einen Kathodenwassereinspritzeinlass (127) in dem Brennstoffzellenstack (110) umfasst und die Wassereinspritzleitung (125) derart konfiguriert ist, dass sie das Passieren von Wasser von dem Kathodenvolumen des Brennstoffzellenstacks in das Aufnahmegefäß (140) über das Rückström-Entlastungsventil (213) zulässt, welches konfiguriert ist, um Wasser von dem Kathodenströmungsweg in das Aufnahmegefäß passieren zu lassen, wenn eine Druckdifferenz über das Ventil, ausgehend von der während des Betriebes des Brennstoffzellensystems, umgekehrt wird.
1. Soupape de décharge à écoulement inversé (213) comprenant :
un premier orifice d'alimentation (314) ;
un second orifice d'alimentation (320) ;
une soupape de non-retour (316) à l'intérieur d'un passage de fluide principal s'étendant entre les premier et second orifices d'alimentation, la soupape de non-retour étant configurée pour permettre au fluide de passer du premier au second orifice d'alimentation et pour bloquer le passage du fluide dans la direction inversée ;
un passage de fluide de dérivation (318) en communication fluidique avec le passage de fluide principal ;
une soupape d'étanchéité (317, 321) sollicitée contre une extrémité du passage de dérivation (318) entre le passage de dérivation et un orifice de purge (238),
dans laquelle la soupape d'étanchéité (317, 321) est configurée pour maintenir un joint contre le passage de dérivation (318), lorsque la pression du fluide dans le premier orifice d'alimentation (314) dépasse la pression du fluide au niveau du second orifice d'alimentation (320), afin d'empêcher l'écoulement de fluide à partir du passage de fluide principal vers l'orifice de purge (238) par l'intermédiaire du passage de fluide de dérivation (318), et pour permettre l'écoulement de fluide à partir du second orifice d'alimentation vers l'orifice de purge par l'intermédiaire du passage de fluide de dérivation, lorsque la pression du fluide au niveau du second orifice d'alimentation dépasse la pression du fluide au niveau du premier orifice d'alimentation.
2. Soupape de décharge à écoulement inversé selon la revendication 1, dans laquelle la soupape d'étanchéité (317, 321) est configurée pour permettre l'écoulement de fluide à partir du second orifice d'alimentation (320) vers l'orifice de purge (238) par l'intermédiaire du passage de fluide de dérivation (318), lorsque la pression du fluide au niveau du second orifice d'alimentation dépasse la pression du fluide au niveau du premier orifice d'alimentation d'une quantité prédéterminée.
3. Soupape de décharge à écoulement inversé selon la revendication 2, dans laquelle la quantité prédéterminée n'est pas inférieure à 300 mbar.
4. Soupape de décharge à écoulement inversé selon l'une quelconque des revendications 1 à 3, dans laquelle la soupape d'étanchéité comprend un diaphragme résilient (321), dont une face est en communication fluidique avec le premier orifice d'alimentation (314), une seconde face opposée (317) du diaphragme étant sollicitée contre l'extrémité du passage de dérivation (318).
5. Soupape de décharge à écoulement inversé selon l'une quelconque des revendications 1 à 4, comprenant un passage de fluide de raccordement (313) s'étendant entre le premier orifice d'alimentation (314) et la soupape d'étanchéité (321).
6. Système de pile à combustible comprenant la soupape de décharge à écoulement inversé de l'une quelconque des revendications 1 à 5, dans lequel le second orifice d'alimentation (320) de la soupape de décharge à écoulement inversé est raccordé à une conduite d'injection d'eau de cathode (125), le premier orifice d'alimentation (314) est raccordé à une pompe (230) et l'orifice de purge (238) est en communication fluidique avec un volume intérieur d'une cuve de confinement d'eau (140).
7. Système de pile à combustible selon la revendication 6, comprenant en outre :
un empilement de pile à combustible (110) ;
un système de cathode ayant un trajet d'écoulement de fluide de cathode comprenant une conduite d'entrée d'air de cathode (123), un volume de cathode à l'intérieur de l'empilement de pile à combustible et une conduite de sortie de cathode (121) raccordée en série et configurée pour permettre le passage de l'air à travers l'empilement de pile à combustible (110) ;
un échangeur de chaleur (130) raccordé en série avec un séparateur d'eau (131) sur la conduite de sortie de cathode (121) du trajet d'écoulement de fluide de cathode,
dans lequel une conduite de sortie d'éjection d'eau (128) du séparateur d'eau (131) est raccordée à la cuve de confinement d'eau (140) par une première conduite de retour d'eau (128a).
8. Système de pile à combustible selon la revendication 7, dans lequel une sortie d'éjection d'eau de l'échangeur de chaleur (130) est raccordée à la cuve de confinement d'eau (140) par une seconde conduite de retour d'eau (128b).
9. Système de pile à combustible selon la revendication 8, comprenant une pompe à eau (132a, 132b) dans chacune des première et seconde conduites de retour d'eau.
10. Système de pile à combustible selon la revendication 6, comprenant en outre :
un empilement de pile à combustible (110) ;
un système de cathode ayant un trajet d'écoulement de fluide de cathode comprenant une conduite d'entrée d'air de cathode (123), un volume de cathode à l'intérieur de l'empilement de pile à combustible et une conduite de sortie de cathode (121) raccordés en série et configurés pour permettre le passage de l'air à travers l'empilement de pile à combustible ;
un compresseur d'air (133) en communication fluidique avec la conduite d'entrée d'air de cathode (123) ;
dans lequel ladite cuve de confinement d'eau (140) est thermiquement isolée et configurée pour recevoir de l'eau par l'intermédiaire d'une conduite de retour d'eau (128) à partir du trajet d'écoulement de cathode,
dans lequel le système de pile à combustible est configuré pour éjecter de l'eau à partir du trajet d'écoulement de cathode dans la cuve de confinement (140) par l'intermédiaire de la conduite de retour d'eau (128) lors de l'arrêt du fonctionnement du système.
11. Système de pile à combustible selon la revendication 10, dans lequel la cuve de confinement (140) est raccordée fluidiquement à la conduite d'injection d'eau de cathode (125), la conduite d'injection d'eau de cathode comprenant en outre une entrée d'injection d'eau de cathode (127) dans l'empilement de pile à combustible (110), la conduite d'injection d'eau (125) étant configurée pour permettre le passage de l'eau à partir du volume de cathode de l'empilement de pile à combustible dans la cuve de confinement (140) par l'intermédiaire de la soupape de décharge à écoulement inversé (213) configurée pour permettre le passage de l'eau à partir du trajet d'écoulement de cathode dans la cuve de confinement, lorsqu'une différence de pression dans la soupape est inversée par rapport à celle pendant le fonctionnement du système de pile à combustible.

REFERENCES CITED IN THE DESCRIPTION
This list of references cited by the applicant is for the reader's convenience only. It does not form part of the European patent document. Even though great care has been taken in compiling the references, errors or omissions cannot be excluded and the EPO disclaims all liability in this regard.

Patent documents cited in the description
- GB
2409763
A
[0003]
- US
6479177
B
[0006]