ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORS..SM..................
J
DIM360 Ver 2.40 (30 Jan 2013) - 1620000/0
2215918
EUROPEAN PATENT APPLICATION
A3
20140122
EP
10152125.0
20100129
en
en
en
322624
20090204
US
657550
20100123
US
20140122
201404
20100811
201032
A43B 7/04 20060101AFI20131218BHEP
de
Elektrisch beheizte Einlegesohlen für Schuhe und Heizsystem mit Fernbedienung für elektrische Einlegesohlen für Schuhe
en
Electrically heated insoles for footware and remote control heating system for electrical insoles for footware
fr
Semelles de chaussures électriquement chauffées et système de chauffage télécommandé pour les semelles de chaussures électriques
1
P3 Limited
101160314
R 13623
Room 1603, Citicorp Centre 18 Whitfield Road
North Point Hong Kong
CN
Reinbacher International Limited
101160315
R 13623
Room 1603, Citicorp Centre 18 Whitfield Road
North Point Hong Kong
CN
Au, Albert
Room 209, Hoi Ching House, Hoi Lai Estate, Lai Ch
Kowloon
CN
Margotti, Herwig Franz
100044028
Schwarz & Partner Patentanwälte Wipplingerstrasse 30
1010 Wien
AT
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
SE
SI
SK
SM
TR
AL
BA
RS
20140122
201404
A wire-free, rechargeable electrically heated insole for footwear. The insole comprises an upper sole and a bottom sole separated by electrical components for controlling the continuous monitoring and heating of the insole. An insert and fiber plane are also provided as a cushion for the electrical components between the upper and bottom soles. The electrical components comprise a printed circuit board electrically coupled with a thermostat, an amplifier and transistor, resistors, and a light emitting diode to form the electrical system. An integrated battery is used to power the system. The insole is designed to be automatically activated to generate heat when the temperature of the foot inside the footwear cools to a certain temperature and automatically de-activated or discontinue generating heat when the temperature of the foot inside the footwear heats to a certain temperature. Alternatively, the electrical insole for footwear may be heated using a remote control heating system comprising a remote transmitter coupled with a receiver and other additional electrical components provided in the sole.
R 13623
EP
10152125.0
P3 Limited
1
DH
20140103
A43B
DE
20317143
U1
SCHMIDT UDO [DE]
20040408
X
1-17
* column 2; figures 1,2,4,6,7,9 *
WO
2005072548
A1
THERM IC PROD
20050811
X
1
* claim 1; figures *
DE
202006001494
U1
ATUFORMA GMBH [DE]
20060323
A
1
* claim 1; figures *
Claudel, Benoît
The Hague
20131213
DE
20317143
U1
20040408
DE
10352050
A1
20041209
DE
20317143
U1
20040408
WO
2005072548
A1
20050811
AT
383786
T
20080215
CA
2555344
A1
20050811
DE
102004006046
A1
20050908
EP
1711080
A1
20061018
US
2009013554
A1
20090115
WO
2005072548
A1
20050811
DE
202006001494
U1
20060323
NONE