ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESM..................
J
DIM360 Ver 2.40 (30 Jan 2013) - 1620000/0
2400212
EUROPEAN PATENT APPLICATION
A3
20130814
EP
10186399.1
20101004
en
en
en
201020251359 U
20100628
CN
20130814
201333
20111228
201152
F21S 8/08 20060101AFI20130710BHEP
F21V 29/00 20060101ALI20130710BHEP
F21V 13/04 20060101ALI20130710BHEP
F21V 7/00 20060101ALI20130710BHEP
F21W 131/103 20060101ALN20130710BHEP
F21Y 105/00 20060101ALN20130710BHEP
de
LED-Lampe zur Erzeugung eines Lichtverteilungsmodus einer in etwa parallelen optischen Annährungsanordnung durch die Verwendung von Linsen
en
LED lamp forming light distribution mode of approximate parallel optical array by using lenses
fr
Lampe à diodes formant un mode de distribution de lumière en réseau optique approximativement parallèle à l'aide de lentilles
2
Wang, Zhen
101206370
Z3-7548
Room 104, East Gate Building 3 No. 10 Hepingli East Street Dongcheng District
Beijing 100013
CN
Wang, Zhen
Room 104, East Gate Building 3 No. 10 Hepingli East Street Dongcheng District
Beijing 100013
CN
Petraz, Gilberto Luigi
et al
100019804
GLP S.r.l. Piazzale Cavedalis 6/2
33100 Udine
IT
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
20130814
201333
A light-emitting diode (LED) lamp forming a light distribution mode of an approximate parallel optical array by using lenses is provided. The LED lamp includes substrates (1) for mounting LEDs (10), reflectors (2), a power source (5), and a top cover (6). Each of the substrates has a condenser lens (11) at a front end of each of the LEDs (10), and the condenser lenses (11) are used for converging beam angles of the LEDs (10). The plurality of LEDs (10) is arranged in a matrix to form an approximate parallel optical array. The reflectors (2) each have a curved surface (21) for performing reflection and light controlling on light rays reflected and controlled by a curved wall. The LED lamp realizes uniform lighting in the whole lighting range through performing lens condensing once and reflection light controlling once, thereby achieving excellent directivity of illumination and uniform brightness, and eliminating the glare phenomenon.
Z3-7548
EP
10186399.1
Wang, Zhen
2
DH
20130716
F21W
F21V
F21Y
F21S
WO
2009077177
A1
OSRAM OPTO SEMICONDUCTORS GMBH [DE]; KUHN GERHARD [DE]; LEONG CHIN KHE
20090625
X
1-3,7
* page 26, line 18 - line 21 *
Y
4
* page 27, line 22 - page 30, line 14 *
* figures 6A, 6B *
* figures 7B,7C *
EP
1988329
A1
STANLEY ELECTRIC CO LTD [JP]
20081105
X
1-3,7
* paragraph [0035] - paragraph [0039] *
* figures 1,3 *
WO
2010032183
A1
KONINKL PHILIPS ELECTRONICS NV [NL]; KRIJN MARCELLINUS P C M [NL]; VAN
20100325
X
1
* page 11 *
* figure 4 *
CN
201269438
Y
YIBO YANG [CN]
20090708
X
1-3
* figure 4 *
US
2009243455
A1
BIEBEL ULRICH [DE] ET AL
20091001
Y
4
* paragraph [0028] *
* figures 1,2 *
Demirel, Mehmet
The Hague
20130704
WO
2009077177
A1
20090625
CN
101903703
A
20101201
DE
102008036020
A1
20090625
EP
2232133
A1
20100929
WO
2009077177
A1
20090625
EP
1988329
A1
20081105
EP
1988329
A1
20081105
ES
2373122
T3
20120131
US
2009027883
A1
20090129
WO
2007097262
A1
20070830
WO
2010032183
A1
20100325
CN
102159876
A
20110817
EP
2326868
A1
20110601
JP
2012503273
A
20120202
KR
20110053480
A
20110523
RU
2011115089
A
20121027
TW
201020467
A
20100601
US
2011163334
A1
20110707
WO
2010032183
A1
20100325
CN
201269438
Y
20090708
NONE
US
2009243455
A1
20091001
AT
514901
T
20110715
CN
101501394
A
20090805
DE
102006037376
A1
20080214
EP
2049835
A1
20090422
HK
1132787
A1
20111230
JP
4861478
B2
20120125
JP
2010500706
A
20100107
US
2009243455
A1
20091001
WO
2008017652
A1
20080214