ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESM..................
J
DIM360 Ver 2.41 (21 Oct 2013) - 1620000/0
2405042
EUROPEAN PATENT APPLICATION
A3
20141203
EP
11004934.3
20110616
20110616
en
en
en
2010154136
20100706
JP
20141203
201449
20120111
201202
D03J 1/22 20060101AFI20141030BHEP
D03D 49/12 20060101ALI20141030BHEP
de
Breithaltervorrichtung für Webmaschine mit automatischem Breithalterpositionsumschaltmechanismus und Verfahren zum Antreiben des Breithalters dafür
en
Temple device for loom including automatic temple position switching mechanism and method of driving temple thereof
fr
Dispositif de templet pour métier à tisser incluant un mécanisme de commutation automatique de position de templet et procédé de commande de templet associé
3
Tsudakoma Kogyo Kabushiki Kaisha
101031220
T1343148EPP00Sv
18-18, Nomachi 5-chome
Kanazawa-shi, Ishikawa 921-8650
JP
Kakutani, Kazuto
c/o Tsudakoma Kogyo Kabushiki Kaisha 18-18, Nomachin 5-chome
Kanazawa-shi Ishikawa-ken 921-8650
JP
Itou, Naoyuki
c/o Tsudakoma Kogyo Kabushiki Kaisha 18-18, Nomachin 5-chome
Kanazawa-shi Ishikawa-ken 921-8650
JP
Samson & Partner
100783861
Widenmayerstraße 5
80538 München
DE
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
20141203
201449
Provided is a method of driving a temple (41) of a temple device (40) including an automatic temple position switching mechanism (42), the temple device (40) being used for a loom that weaves a fabric (2a) having two or more weave sections with different weft densities, the automatic temple position switching mechanism (42) automatically switching a position of the temple (41) between two positions that are an operating position and a standby position, the method being performed when displacing the temple (41) from the standby position toward the operating position in accordance with switching between the weave sections, the method including storing an operation mode related to movement of the temple (41) beforehand, and controlling the movement of the temple (41) in accordance with the stored operation mode in accordance with switching between the weave sections.
T1343148EPP00Sv
EP
11004934.3
Tsudakoma Kogyo Kabushiki Kaisha
3
MN
20141105
D03J
D03D
US
5065796
A
ROACH ERNEST F [US] ET AL
19911119
X,D
1-5
* abstract *
* column 4, line 25 - column 6, line 46 *
* figures 1-6 *
DE
9006343
U1
GEBRÜDER SULZER AG
19900920
A
1-5
* page 4, lines 3-20 *
* page 7, paragraph 3 *
* figures 1-5 *
DD
261383
A1
FUERSTENWALDE REIFEN VEB K [DD]
19881026
A
1-5
* the whole document *
JP
H10298853
A
TSUDAKOMA IND CO LTD
19981110
A
1-5
* abstract; figures 1-8 *
Louter, Petrus
Munich
20141030
US
5065796
A
19911119
CS
9102959
A3
19920513
DE
4132696
A1
19920409
EP
0479499
A1
19920408
JP
H04281041
A
19921006
US
5065796
A
19911119
DE
9006343
U1
19900920
NONE
DD
261383
A1
19881026
NONE
JP
H10298853
A
19981110
NONE