ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESM..................
J
JDIM360 Ver 1.28 (29 Oct 2014) - 1620000/0
2447399
EUROPEAN PATENT APPLICATION
A3
20150114
EP
11008526.3
20111025
20111025
en
en
en
2010242436
20101028
JP
20150114
201503
20120502
201218
D04B 1/22 20060101AFI20141211BHEP
de
Strickverfahren auf einer Flachstrickmaschine mit mehreren Fadenführern und entsprechendes Gestrick
en
Knitting method on a flat knitting machine having a plurality of yarn feeders and a corresponding knitted fabric
fr
Procédé de tricotage en utilisant un métier à tricoter rectiligne avec plusieurs guide-fills et un tricot correspondent
1
Shima Seiki Manufacturing., Ltd.
100974161
SM-E-30472/030
85, Sakata Wakayama-shi
Wakayama 641-8511
JP
Minami, Masayuki
SHIMA SEIKI MFG., LTD. 85, Sakata
Wakayama-shi Wakayama 641-8511
JP
Terai, Koichi
SHIMA SEIKI MFG., LTD. 85, Sakata
Wakayama-shi Wakayama 641-8511
JP
Schmidbauer, Andreas Konrad
101222806
Wagner & Geyer Patent- und Rechtsanwälte Gewürzmühlstrasse 5
80538 München
DE
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
20150114
201503
To provide a knitting method of a knitted fabric enabling knitting while preventing a cross-over yarn portion, which connects two knitted fabric portions at positions spaced apart in the wale direction of the knitted fabric, from becoming a free state, and a knitted fabric knitted by applying such knitting method of the knitted fabric. A preceding stitch row (knitting needle G of FB) is knitted with a knitting yarn from a yarn feeder 9 on a far side with respect to a FB, which is a target needle bed, on which knitting is carried out (S2), and the yarn feeder 9 is once moved towards the preceding stitch row side of a stitch (knitting needle G of FB) at a termination of the preceding stitch row (S3). A yarn feeder 8 on a near side with respect to the FB is moved in the direction opposite to the direction of forming the preceding stitch row so that the knitting yarn extending from the yarn feeder 8 intersect at the upper side of the needle bed gap of the knitting yarn extending from the yarn feeder 9 (S3). A trailing stitch row, which is the rest of the preceding stitch row, is then knitted with the yarn feeder 9 (S4).
SM-E-30472/030
EP
11008526.3
Shima Seiki Manufacturing., Ltd.
1
MN
20141217
D04B
EP
1652980
A1
SHIMA SEIKI MFG [JP]
20060503
A,D
1,3,4
* paragraphs [0041] - [0051]; claims 2, 5; figures 1-5 *
EP
1219740
A1
SHIMA SEIKI MFG [JP]
20020703
A
4
* paragraphs [0004] - [0007], [0020]; figure 8 *
EP
2154280
A1
SHIMA SEIKI MFG [JP]
20100217
A
4
* paragraph [0035]; claim 1; figures 1, 2 *
Sterle, Dieter
Munich
20141204
EP
1652980
A1
20060503
CN
1833059
A
20060913
EP
1652980
A1
20060503
JP
4002870
B2
20071107
JP
2005060861
A
20050310
KR
20060061348
A
20060607
US
2008169041
A1
20080717
WO
2005014902
A1
20050217
EP
1219740
A1
20020703
DE
60034958
T2
20080228
EP
1219740
A1
20020703
JP
3541192
B2
20040707
TW
470795
B
20020101
US
6578389
B1
20030617
WO
0116416
A1
20010308
EP
2154280
A1
20100217
CN
101663427
A
20100303
EP
2154280
A1
20100217
JP
5307000
B2
20131002
WO
2008139709
A1
20081120