ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESM..................
J
DIM360 Ver 2.15 (14 Jul 2008) - 1100000/0
2487110
EUROPEAN PATENT APPLICATION
A2
20120815
EP
12154565.1
20120208
20120208
en
en
en
102011010913
20110210
DE
201161441514 P
20110210
US
20120815
201233
20120815
201233
B64D 11/02 20060101AFI20120515BHEP
de
Handtrocknungsvorrichtung und Waschstand für ein Luftfahrzeug
en
Hand drying device and washing stand for an aircraft
fr
Dispositif de séchage à la main et support de lavage pour aéronef
7
Airbus Operations GmbH
101121620
A 13124 / KK
Kreetslag 10
21129 Hamburg
DE
Dehn, Martin
Börnsener Str. 17
21521 Aumühle
DE
Muin, Andrew
Kohldistelstr. 4
21698 Harsefeld
DE
Reh, Jan
Fersenfeldtsweg 4
22303 Hamburg
DE
Kopf, Korbinian Paul
100054307
Maiwald Patentanwalts GmbH Elisenhof Elisenstrasse 3
80335 München
DE
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
The hand cleaning process in aircraft requires a plurality of different steps. The invention relates to a hand drying device for an aircraft, which can be integrated into a washing stand, so that the hand washing and hand drying process can be performed within the washbasin of the washing stand. Corresponding sensors can be provided to make this process contactless, thereby making it possible to reduce the spread of bacteria or viruses.

Reference to Related Applications
This application claims the benefit of the filing date of German Patent Application No. 10 2011 010 913.7 filed February 10, 2011 and of United States Provisional Patent Application No. 61/441,514 filed February 10, 2011, the disclosure of which applications is hereby incorporated herein by reference.

Field of the Invention
The invention relates to devices involving the interior fixtures of toilet modules or kitchens in passenger aircraft. In particular, the invention relates to a hand drying device for an aircraft, a washing stand with a hand drying device, an aircraft toilet module, an aircraft kitchen module, as well as an aircraft with a hand drying device or a washing stand.

Background of the Invention
Hand washing basins in which the passengers and flight personnel can wash their hands are installed in aircraft cabins, in particular in aircraft toilet modules or kitchen modules (galleys) installed therein. Provided for drying the hands are tissues, which can be taken from a dispenser located in the vicinity of the hand washing basin. The used tissues are then collected in a waste container.
Both the fresh tissues and used tissues must be stored. In addition, it should be ensured that enough fresh tissues are available at all times. A corresponding supply may have to be kept in stock for this purpose, and the dispensing devices for dispensing the tissues should be refilled regularly. This may be associated with the need for more space, a higher weight and additional costs.
DE 10 2009 018 690 A1 and WO 2010/121862 A4 describe aircraft toilet modules with a hand washing basin.
DE 10 2009 021 970 A1 describes an autonomous water module for aircraft, which also exhibits a hand washing basin.

Summary of the Invention
A hand drying device for an aircraft, a washing stand, an aircraft toilet module, an aircraft kitchen module and an aircraft are indicated according to the features of the independent claims. Further developments of the invention may be gleaned from the subclaims and following specification.
A first aspect of the invention indicates a hand drying device for an aircraft, which is designed for generating a stream of air to dry the hands of a user. The hand drying device is here designed for connection to an air supply line of the aircraft, through which at least a portion of the air needed for operating the hand drying device can be provided.
Therefore, the hand drying device exhibits a blower, for example, which generates and emits the essentially dry and, if necessary, heated stream of air, which can then be used to dry the hands of the user.
The hand drying device is connected to an air supply line of the aircraft, and taps at least a portion of the air to be blown out from this air supply line. For example, already heated and compressed air is delivered via this air supply line, so that the air inside the hand drying device need only be additionally compressed to a comparatively slight extent, if at all. It is also possible that the air inside the hand drying device will not have to be heated any further, since the air made available by the air supply line is already sufficiently heated.
For example, this air supply line may involve a line that carries bleed air from one or more aircraft engines. A line of the air conditioning system can also be involved here, which carries air provided by the air conditioner of the aircraft.
In an embodiment of the invention, the hand drying device exhibits a compressor for recompressing the air provided by the air supply line of the aircraft. For example, this compressor can be a volume compressor or pump. This compressor can have a very efficient design, so that the generated air stream is blown out of the hand drying device at a comparatively high speed measuring up to several hundred kilometers per hour, e.g., 300 or 400 kilometers per hour, allowing the hand drying process to conclude within a few seconds, for example, within ten seconds.
In a further embodiment of the invention, the hand drying device exhibits another air supply for providing additional air. This additional air may be mixed in with the air provided by the air supply line of the aircraft within the hand drying device.
Depending on the quantity and pressure of the air provided by the air supply line, a valve may be furnished and used to regulate the additional air supply accordingly. In so doing, it may be ensured that the optional quantity of incoming air is always made available to the hand drying device, and furthermore that more air than needed is not removed from the cabin.
Another aspect of the invention indicates a washing stand for an aircraft, comprising a hand washing basin and a hand drying device designed for generating an air stream to dry the hands of a user, wherein the hand drying device exhibits several air outlets, which are integrated into the hand washing basin, and through which the air stream for drying the hands of the user is blown out.
The washing stand may also comprise a hand drying device described above and below.
For example, this washing stand may be an autonomous water module as described in DE 10 2009 021 970 A1, or a washing stand permanently installed in the cabin or a corresponding monument.
For example, the washing stand is a module for an onboard kitchen or a module for an aircraft toilet.
This washing stand exhibits an interface, which is designed for connection to a corresponding interface of the air supply line in the aircraft. In the case of an autonomous water module, this interface may be designed as a manually detachable connection that is easy to operate, so that the washing stand can be shifted within the aircraft cabin without any great effort.
In another embodiment of the invention, the hand drying device exhibits several air outlets, which are integrated into the hand washing basin, and through which the air stream for drying the hands of the user is blown out.
In other words, the user can thus wash his or her hands in the hand washing basin, and immediately thereafter dry them in the air stream without having to remove his or her hands from the washing basin for this purpose.
As a consequence, the blown off water may collect in the washing basin, and then be routed to a gray water storage tank.
In another embodiment of the invention, at least two of the air outlets are situated across from each other, so that two or more streams of air flowing in opposite directions can be generated.
For example, these air streams are flat, high speed air streams, which are generated slightly vertically offset from each other, so as not to impede each other to any significant extent.
In another embodiment of the invention, the washing stand exhibits a first optical sensor and/or a second optical sensor.
The first optical sensor records when the hand of the user is located in a first position provided for this purpose (e.g., under a water tap of the washing stand). The first optical sensor thereupon activates the flow of water out of this water tap.
The second optical sensor records when the hand of the user is located in a second position provided for this purpose, e.g., in the vicinity of the air outlets. In this case, the second optical sensor activates the hand drying device.
It may also be possible to only provide the first optical sensor, and for the water to only run for a definite period of time, for example until the user removes his or her hand from the location provided for hand washing, after which the hand drying device is automatically activated.
In another embodiment of the invention, the washing stand is designed for completely contactless use. The user may not have to touch any fittings, buttons or adjusting levers to carry out the washing routine. In particular, an automated soap dispenser may also be provided, e.g., which also exhibits an optical sensor, so that soap is dispensed when the user holds his or her hand under this soap dispenser. In particular, the soap dispenser may be positioned in such a way as to dispense the soap over the washing basin, so that excess soap drips into the basin.
Furthermore, an automated dispenser for dispensing a sterilizing or sanitary agent onto the user's hands may be provided as part of the washing stand. The agent may be sprayed onto the user's hands. The dispenser may also comprise one or more sensors, so that the agent is dispensed when the user holds his or her hand under this agent dispenser. In particular, the agent dispenser may be positioned in such a way as to dispense the agent over the washing basin, so that excess agent drips into the basin.
The ability to use the hand washing basin completely without contact may make it possible to significantly improve hygiene. In addition to the sensors, corresponding adjusting levers and/or buttons can be furnished to ensure that the washing basin remains operable even if a sensor fails.
Another aspect of the invention indicates an aircraft toilet module, which exhibits a hand drying device described above and below and/or a washing stand described above and below.
For example, the hand drying device or washing stand may be connected with the toilet, thereby providing a combined toilet bowl-washing stand module.
Another aspect of the invention indicates an aircraft kitchen module, which exhibits a hand drying device described above and below and/or a washing stand described above and below.
Another aspect of the invention indicates an aircraft, which exhibits a hand drying device described above and below and/or a washing stand described above and below.
In another embodiment of the invention, at least a portion of the air provided by the air supply line to the hand drying device is bleed air from an engine of the aircraft and/or air from an aircraft air conditioning system.
In another embodiment of the invention, at least a portion of the air provided by the air supply line to the hand drying device is air having a higher pressure than the cabin air of the aircraft and/or a higher temperature than the cabin air of the aircraft.
Apart from the above, let it be noted that the hand drying device may also exhibit a heater in order to heat up the air to be blown out.
According to another exemplary embodiment of the present invention the aircraft may further comprise a lighting arrangement for emitting light of different colors, wherein the lighting arrangement is adapted for emitting light of a first color only when rinsing water is ejected from the washing stand and wherein the lighting arrangement is adapted for emitting light of a second color only when the hand drying device is activated. The lighting arrangement may furthermore be adapted for emitting light of a third color only when soap is ejected and light of a fourth color only when a sanitary/sterilizing agent is dispensed. Thus, the user may be guided such that it is clear to him/her step is to be performed at which time.
Exemplary embodiments of the invention will be described below drawing reference to the figures.

Brief Description of the Figures
- Fig. 1 shows a washing stand 100 according to an exemplary embodiment of the invention.
- Fig. 2 shows an aircraft toilet module according to another exemplary embodiment of the invention.
- Fig. 3 shows a kitchen module according to another exemplary embodiment of the invention.
- Fig. 4 shows a washing stand according to another exemplary embodiment of the invention.
- Fig. 5 shows the combination of washing stand and toilet according to another exemplary embodiment of the invention.
- Fig. 6 shows a washing stand with running water tap according to an exemplary embodiment of the invention.
- Fig. 7 shows a washing stand with activated hand drying device according to an exemplary embodiment of the invention.
- Fig. 8 shows a washing stand with running water tap according to an exemplary embodiment of the invention.
- Fig. 9 shows a washing stand with activated hand drying device according to an exemplary embodiment of the invention.
- Fig. 10 shows an aircraft with a toilet module and a kitchen module according to an exemplary embodiment of the invention.
- Fig. 11 shows a dispenser for dispensing an agent onto the user's hands.

Detailed Description of Exemplary Embodiments
The depictions on the figures are diagrammatic and not to scale.
If the same reference numbers are used on different figures in the following description of figures, they denote the same or similar elements. However, the same or similar elements may also be denoted by different reference numbers.
Fig. 1 shows a washing stand 100 according to a first exemplary embodiment of the invention. The washing stand 100 exhibits a hand washing basin 101, over which the water outlet of a water tap 105 is situated, so that a user can wash his or her hands over or in the hand washing basin 101.
Also provided is a hand drying device 102 hooked up to an air supply line 103 of the aircraft via the interface 104 arranged on the rear side of the washing stand 100. For example, hot bleed air or air of the air conditioning system is carried by this air supply line 103, and delivered to the hand drying device 102 as needed.
To this end, for example, the hand drying device exhibits a valve 109, e.g., one that is designed like a flap, and exhibits a stop 110, which prevents air from being carried from the hand drying device 102 back into the air supply line 103.
A compressor (not shown on Fig. 1) that additionally compresses the provided air can be furnished within the hand drying device 102. Furthermore, another air supply 111 can be furnished, which can provide the hand drying device with additional air from the environment of the washing stand 100. This air supply can also be controlled by way of a corresponding valve 112.
The two lines 106, 107 are furnished to deliver the compressed air, guiding the compressed and if necessary heated air from the compressor to air nozzles or air slits integrated into the hand washing basin 101 at opposing locations, through which the air is then blown out.
Fig. 2 shows an aircraft toilet module 200, which incorporates a toilet bowl 201 and a washing stand 100. Distinct, separate fixtures were previously installed in aircraft toilet modules and aircraft kitchen modules for washing and drying hands: A water tap with washbasin, a tissue dispenser and a waste container. The disadvantage to this configuration on the one hand is that more space is needed for the different fixtures, which is associated with extra weight. In addition, the tissues should be routinely refilled, for example after each flight.
The process of cleaning the hands requires numerous operations to be performed in sequence. The water tap must first be activated, and the soap dispenser operated. The washing process then takes place, after which drying material (tissue) is provided from the dispenser furnished for this purpose, and the used tissues are thrown into the waste container. Each of these actions takes a certain amount of time, and further requires that users orient themselves as to where and how to perform the hand movements needed. Under certain conditions, for example in the event of great fatigue or in cases of nausea, this may place an excessive burden on the passenger, rendering them unable to successfully operate the different fixtures.
In particular when combined with a washing stand, using a hand drying device described above and below in an aircraft yields a variety of advantages.
For example, this may make washing and drying the hands a more hygienic, faster, intuitive and hence simpler process for the passenger. It also enables a seamless hand cleaning process, even under more difficult circumstances.
An advantage to the airlines has to do with reduced costs, since tissues need no longer be taken along for drying hands. This may make it possible to save on procurement, inventory, transportation, refilling and disposal costs.
In addition, this may yield a reduced weight, since tissues no longer have to be carried. No extra tissue dispensers, waste containers and storage areas have to be provided either, so that space may be economized in addition to weight and costs.
Furthermore, a lighting arrangement 202 is provided which comprises one or more lights, for example LEDs, for emitting light of different colors. The lighting arrangement is adapted for emitting light of a first color only when rinsing water is ejected from the washing stand and for emitting light of a second color only when the hand drying device 102 (see Fig. 1) is activated.
As a consequence, the combined washing stand may make it possible to simplify and optimize the hand cleaning process by combining devices for dispensing water, dispensing soap and drying (air jet) with each other.
Naturally, the washing stand may also be integrated into an onboard kitchen module, as shown diagrammatically on Fig. 3. The washing stand 100 is here pushed into a corresponding recess in the aircraft kitchen module 300 from above, and on its rear side is hooked up to an air supply line of the aircraft. Above the washing stand a lighting arrangement 202 is arranged.
Fig. 4 shows a perspective view of a washing stand 100 according to an exemplary embodiment of the invention. The hand washing basin 101 is recessed in the washing stand 100, and the water tap 105 is situated over it. For example, an optical sensor 407 is provided in the base of the water tap, which records when a hand of the user is located under the water dispensing opening 412 of the water tap. In this case, the water is then automatically dispensed, for example for a specific interval of time. The fresh water is supplied from below via the right line 403, and the gray water accumulating in the hand washing basin 101 is downwardly discharged via the left line 402.
The hand drying device 102 is integrated into the washing stand. It exhibits an engine block (compressor) 401, which is used to compress the air to be blown out. For example, this engine block 401 is located under the hand washing basin 101. The compressed air generated by the compressor is relayed to the outlet nozzles 404, 405 and 406. The nozzles 404 and 405 are situated to the left and right of the water tap on the one side of the hand washing basin 101, and the third nozzle 406 is located on the opposite side of the hand washing basin 101.
The nozzles are designed like slits, so that three flat air flows can be generated, as symbolized by the corresponding arrows.
Situated under the nozzles is a respective optical sensor 408, 409, which records when the hand of the user is in the vicinity of the corresponding nozzle. In this case, the hand drying device is activated, and the air streams are blown out, so that the user can dry both of his or her hands in a matter of a few seconds.
The fixtures, buttons or levers do not have to be touched, since the hand washing basin is completely automated, contactless and sensor-controlled.
For example, the optical sensors can be infrared sensors.
The hand washing basin 101 can be adjoined by a lateral table area 411, for example which exhibits a trough, and can be used as a vanity.
The lateral table can also adjoin the other side of the hand washing basin, for example as depicted on Fig. 6.
Fig. 5 shows the combination of a hand washing stand 100 and an aircraft toilet bowl 501. The toilet bowl 501 is here integrated into the washing stand module 100.
Fig.6 shows a washing stand 100 with running water tap. The generated water jet 601 flows directly into the hand washing basin 101, and is then discharged via the conduit 402 (see Fig. 4).
Fig. 7 shows a hand washing basin 101 with an activated hand drying device, which in the case of Fig. 7 generates four air streams 701, 702, 703 and 704. The air streams consist of heated air, which flows out of four corresponding, slit-like air nozzles, of which two are located on one side of the hand washing basin, and two on the opposite side of the hand washing basin.
Fig. 8 shows a hand washing procedure, in which the user holds his or her hand 802 under the water tap, whereupon the water automatically begins to flow, collects in the lower region of the hand washing basin, and is then routed via the constriction 801 to the discharge line 402 (see Fig. 4).
Fig. 9 shows the hand washing basin of Fig. 8 with activated hand drying device. Visible in particular is how the opposite air streams inside the combined hand washing basin are carried upwardly from the compressor (not shown on Fig. 9), and then exit the opposing nozzles. The exiting, laminar, mutually opposite air flows are slightly vertically offset relative to each other, so as not to impede each other.
Furthermore, an automated dispenser 1100 (see Fig. 11) for dispensing a sterilizing or sanitary agent onto the user's hands may be integrated into the hand washing basin. Next to the air stream nozzles openings 901, 902 may be provided for ejecting the sterilizing or sanitary agent onto the user's hands.
The curved design of the hand washing basin 101 helps to assist the hand drying process, since the air streams coming from the side of the water tap on the opposite side of the hand washing basin are deflected downward, thereby describing a 360 degree turn, after which they can again be routed to the blown out air. By contrast, the air streams from the nozzles opposite the water tap are directed slightly upward, so that they cannot influence the other stream.
Fig. 10 shows an aircraft 1000 with one or more toilet modules 200 as well as one or more kitchen modules 300 according to an exemplary embodiment of the invention.
Mobile hand washing basins may also be provided.
Fig. 11 shows an automated dispenser 1100 for dispensing a sterilizing or sanitary agent onto the user's hands, which may be part of the washing stand. The agent may be sprayed onto the user's hands. The dispenser may also comprise one or more sensors 1101, so that the agent is dispensed when the user holds his or her hand under this agent dispenser. In particular, the agent dispenser may be positioned above the washing basing, so that excess agent drips into the basin.
The dispenser 1100 may be integrated in the washing stand, for example into the water tap 105 or beside the water tap 105 (see Fig. 1).
Thus, a four phase washing cycle may be performed in a fully or semi automated manner. In a first phase or step soap may be applied to the user's hands. In phase two, the hands are rinsed in the water ejected from water tap 105. Then, in phase three, the hands are dried by an airstream from the hand drying device and in phase four the agent is applied onto the user's hands.
Each of the four phases may be visualized by colored light emitted from a lighting arrangement, such as a LED or an LED array. For example, each phase may be correlated with a respective color, e.g. yellow for application of soap, blue for rinsing in water, red for drying, orange for disinfection/sterilization, green for successful completion of whole cleaning cycle. Of course, other colors may be used. Further, acoustic and/or other visual or haptic signals may be used for guiding the user through the washing cycle.
In addition, let it be noted that "comprising" and "exhibiting" do not preclude other elements or steps, and "an" or "a" do not rule out a plurality. Let it further be noted that features or steps described with reference to one of the above exemplary embodiments can also be used in combination with other features or steps from other exemplary embodiments described above. Reference numbers in the claims are not to be construed as a limitation.
1. A hand drying device (102) for an aircraft,
wherein the hand drying device (102) is designed for generating an air stream to dry the hands of a user; and
wherein the hand drying device (102) is designed for connection to an air supply line (103) of the aircraft, which provides at least a portion of the air necessary for operating the hand drying device (102).
2. The hand drying device (102) of claim 1, further comprising:
a compressor (401) for recompressing the air provided by the air supply line (103) of the aircraft.
3. The hand drying device (102) of one of the preceding claims, further comprising:
an other air supply for providing additional air, which is mixed in with the air provided by the air supply line (103) of the aircraft within the hand drying device (102).
4. A washing stand (100) for an aircraft, comprising:
a hand washing basin (101); and
a hand drying device (102) designed for generating an air stream to dry the hands of a user;
wherein the hand drying device (102) exhibits several air outlets (404, 405, 406), which are integrated into the hand washing basin (101), and through which the air stream for drying the hands of the user is blown out.
5. The washing stand (100) of claim 4,
wherein the hand drying device (102) is a hand drying device of one of preceding claims 1 to 3.
6. The washing stand (100) of claim 5,
wherein at least two of the air outlets (404, 406) are situated across from each other, so as to generate two or more streams of air flowing in opposite directions.
7. The washing stand (100) of one of claims 4 to 6, further comprising:
a first optical sensor (407), which is designed to activate the dispensing of water when it detects the hand of the user at a first location provided for this purpose;
a second optical sensor (408, 409), which is designed to activate the hand drying device (102) when it detects the hand of the user at a second location provided for this purpose.
8. The washing stand (100) of one of claims 4 to 7,
designed for contactless use.
9. The washing stand (100) of one of claims 4 to 8, further comprising:
an automated dispenser (1100) for dispensing a sterilizing or sanitary agent onto the user's hands.
10. An aircraft toilet module (200), comprising:
a hand drying device (102) of one of claims 1 to 3 or a washing stand of one of claims 4 to 9.
11. An aircraft kitchen module, comprising:
a hand drying device (102) of one of claims 1 to 3 or a washing stand of one of claims 4 to 9.
12. An aircraft, comprising:
a hand drying device (102) of one of claims 1 to 3 or a washing stand of one of claims 4 to 9.
13. The aircraft of claim 12,
wherein at least a portion of the air provided by the air supply line (103) to the hand drying device (102) is bleed air from an engine of the aircraft.
14. The aircraft (1000) of claim 12 or 13,
wherein at least a portion of the air provided by the air supply line (103) to the hand drying device (102) is air having a higher pressure than the cabin air of the aircraft.
15. The aircraft (1000) of one of claims 12 to 14,
further comprising a lighting arrangement (202) for emitting light of different colors;
wherein the lighting arrangement is adapted for emitting light of a first color only when rinsing water is ejected from the washing stand;
wherein the lighting arrangement is adapted for emitting light of a second color only when the hand drying device (102) is activated.

REFERENCES CITED IN THE DESCRIPTION
This list of references cited by the applicant is for the reader's convenience only. It does not form part of the European patent document. Even though great care has been taken in compiling the references, errors or omissions cannot be excluded and the EPO disclaims all liability in this regard.

Patent documents cited in the description
- DE
102011010913
20110210
[0001]
- US
61441514
B
20110210
[0001]
- DE
102009018690
A1
[0005]
- WO
2010121862
A4
[0005]
- DE
102009021970
A1
[0006]
[0017]