ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESM..................
J
JDIM360 Ver 1.28 (29 Oct 2014) - 1620000/0
2518200
EUROPEAN PATENT APPLICATION
A3
20150610
EP
12165469.3
20120425
20120425
en
en
en
2011099544
20110427
JP
20150610
201524
20121031
201244
D05B 29/12 20060101AFI20150504BHEP
D05C 7/02 20060101ALI20150504BHEP
de
Nähmaschinen-Stickdruckvorrichtung und Nähmaschine
en
Sewing machine embroidery presser and sewing machine
fr
Pied presseur de broderie pour machine à coudre et machine à coudre
3
AISIN SEIKI KABUSHIKI KAISHA
100073475
A003.381.00
1, Asahi-machi, 2-chome
Kariya-shi, Aichi 448-8650
JP
Kawai, Yasunori
Aisin Seiki Kabushiki Kaisha, c/o Intellectual Property Department 1, Asahi-machi 2-chome
Kariya-shi, Aichi 448-8650
JP
Serjeants LLP
100060021
Dock 75 Exploration Drive
Leicester, LE4 5NU
GB
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
20150610
201524
Disclosed is a sewing machine embroidery presser attached to a presser bar, in a sewing machine including a needle bar that has a needle holder for holding a needle and is vertically movable in the height direction, a presser bar vertically movable in the height direction, and a presser lifting lever for vertically moving the presser bar, the sewing machine embroidery presser including: a presser holder attached to a lower portion of the presser bar using a fixture; an operational arm that is attached to the presser holder and moved vertically by the needle bar or the needle holder to vertically move in the height direction; a presser foot that is vertically movably held by the presser holder to move in synchronization with the operational arm, faces a needle plate of the sewing machine, and presses a target workpiece; a presser spring that is provided in the presser holder and has a biasing force for biasing the presser foot toward the needle plate; and a subsidiary lever pivotably provided in the presser holder, the subsidiary lever including a cam surface having a cam profile for vertically moving the operational arm in response to pivoting, a fixing trench that engages with the operational arm to move the presser foot to the presser holder side and temporarily set the presser foot in a first height position raised from the needle plate, and an operating portion operated by the user's finger.
A003.381.00
EP
12165469.3
AISIN SEIKI KABUSHIKI KAISHA
3
MN
20150511
D05B
D05C
US
2009114133
A1
FUJIHARA SHINYA [JP]
20090507
A
1-7
* paragraph [0025] - paragraph [0055]; figures 1-11 *
EP
1705278
A1
BROTHER IND LTD [JP]
20060927
A,D
1-7
* paragraph [0009] - paragraph [0036]; figures 1-4 *
EP
2390396
A1
AISIN SEIKI [JP]
20111130
A,P
1-7
* paragraph [0045] - paragraph [0074]; figures 1-13 *
Herry-Martin, D
Munich
20150421
US
2009114133
A1
20090507
JP
2009112325
A
20090528
US
2009114133
A1
20090507
EP
1705278
A1
20060927
CN
1837442
A
20060927
EP
1705278
A1
20060927
JP
4623423
B2
20110202
JP
2006263170
A
20061005
US
2006213409
A1
20060928
EP
2390396
A1
20111130
CN
102260967
A
20111130
EP
2390396
A1
20111130
JP
5574163
B2
20140820
JP
2011245110
A
20111208
US
2011290168
A1
20111201