ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESM..................
J
JDIM360 Ver 1.28 (29 Oct 2014) - 1620000/0
2679921
EUROPEAN PATENT APPLICATION
A3
20160106
EP
13160066.0
20130319
en
en
en
2012143606
20120627
JP
20160106
201601
20140101
201401
F24F 1/06 20110101AFI20151127BHEP
F25B 9/00 20060101ALI20151127BHEP
F25B 13/00 20060101ALI20151127BHEP
F24F 1/46 20110101ALI20151127BHEP
F24F 3/14 20060101ALI20151127BHEP
F24F 11/00 20060101ALI20151127BHEP
F25B 49/00 20060101ALI20151127BHEP
de
Kältekreislaufvorrichtung
en
Refrigeration cycle apparatus
fr
Appareil de circuit de réfrigération
3
Mitsubishi Electric Corporation
100785331
139EP 0660 SS
7-3, Marunouchi 2-chome
Chiyoda-ku Tokyo 100-8310
JP
Suzuki, Yasuhiro
c/o Mitsubishi Electric Corporation 7-3, Marunouchi 2-chome, Chiyoda-ku
Tokyo, 100-8310
JP
Makino, Hiroaki
c/o Mitsubishi Electric Corporation 7-3, Marunouchi 2-chome, Chiyoda-ku
Tokyo, 100-8310
JP
Maeyama, Hideaki
c/o Mitsubishi Electric Corporation 7-3, Marunouchi 2-chome, Chiyoda-ku
Tokyo, 100-8310
JP
Ishii, Minoru
c/o Mitsubishi Electric Corporation 7-3, Marunouchi 2-chome, Chiyoda-ku
Japan, 100-8310
JP
Pfenning, Meinig & Partner GbR
100060642
Patent- und Rechtsanwälte Theresienhöhe 11a
80339 München
DE
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
20160106
201601
From recent study of combustion of an HFC refrigerant that has a low GWP but is flammable, it has been found that the combustion scale tends to increase as the absolute humidity increases. In a refrigeration cycle apparatus using such a refrigerant, it is necessary to increase safety against unexpected refrigerant leakage in consideration of this tendency.
This refrigeration cycle apparatus includes a compressor having a compression mechanism section in an enclosed container and configured to compress and discharge a refrigerant so as to circulate the refrigerant in a refrigerant circuit, and an outdoor unit installed outdoors and having a housing divided by a partition plate into a fan chamber and a machine chamber including the compressor. The refrigerant is a flammable HFC refrigerant. The refrigeration cycle apparatus further includes a desiccant attached in thermal contact with a surface of the enclosed container of the compressor whose temperature is increased by a gas refrigerant compressed by the compression mechanism section during operation of the compressor so that the temperature becomes a high temperature near a temperature of the compressed gas refrigerant, and adsorbs water from air in the machine chamber during non-operation of the outdoor unit.
139EP 0660 SS
EP
13160066.0
Mitsubishi Electric Corporation
3
MN
20151203
F25B
F24F
JP
2000105003
A
SANYO ELECTRIC CO
20000411
X,D
1-8
* paragraph [0001] - paragraph [0026]; figures 1-3 *
JP
H08944
A
DAIKIN IND LTD
19960109
A
1-8
* page 2 - page 3; figures 1-4 *
EP
1681518
A1
DAIKIN IND LTD [JP]
20060719
A
1-8
* page 5 - page 15; figures 1-26 *
Amous, Moez
Munich
20151127
JP
2000105003
A
20000411
NONE
JP
H08944
A
19960109
JP
H08944
A
19960109
JP
3505786
B2
20040315
EP
1681518
A1
20060719
AU
2004280427
A1
20050421
CN
1864034
A
20061115
EP
1681518
A1
20060719
JP
3649236
B2
20050518
JP
2005114294
A
20050428
KR
20060085648
A
20060727
US
2007125115
A1
20070607
WO
2005036062
A1
20050421