ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESM..................
J
BDM Ver 0.1.59 (03 Mar 2017) - 1620000/0
2727511
EUROPEAN PATENT APPLICATION
A3
20170726
EP
13190311.4
20131025
en
en
en
2012241563
20121101
JP
2013163015
20130806
JP
20170726
201730
20140507
201419
A47L 15/00 20060101AFI20170620BHEP
de
Geschirrspüler
en
Dishwasher
fr
Lave-vaisselle
3
Panasonic Corporation
101067135
59 569 M XX
1006, Oaza Kadoma
Kadoma-shi Osaka 571-8501
JP
Hiromatsu, Naoki
c/o Panasonic Corporation, Intellectual Property Center IP Development Group 7F OBP Panasonic Tower, 1-61, Shiromi 2-chome Chuo-ku, Osaka-shi
Osaka 540-6207
JP
Shinkai, Kiyoyasu
c/o Panasonic Corporation, Intellectual Property Center IP Development Group 7F OBP Panasonic Tower, 1-61, Shiromi 2-chome Chuo-ku, Osaka-shi
Osaka 540-6207
JP
Mishima, Takuhiro
c/o Panasonic Corporation, Intellectual Property Center IP Development Group 7F OBP Panasonic Tower, 1-61, Shiromi 2-chome Chuo-ku, Osaka-shi
Osaka 540-6207
JP
Schwabe - Sandmair - Marx
100060632
Patentanwälte Rechtsanwalt Partnerschaft mbB Joseph-Wild-Straße 20
81829 München
DE
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
20170726
201730
A dishwasher includes: a washing tub (3) that accommodates a washing object (7); a washing nozzle (6) that sprays washing water to the washing object (7); a heater (8) that heats the washing water; a water level detecting device (20) that detects a water level in the washing tub (3); a washing pump (5) that circulates the washing water in the washing tub (3); a water supply valve (15) that supplies water into the washing tub (3); and a control device (21) that controls respective steps of washing, rinsing and drying.
The control device (21) performs a control for opening the water supply valve (15) to start water supply, closing the water supply valve (15) to finish the water supply by receiving information indicating that the water level reaches a detection water level, detected by the water level detecting device (20), and heating the washing water by the heater (8) before the washing pump (5) is operated.
Accordingly, it is possible to realize a dishwasher that performs washing with high detergency from the start of a washing step using a liquid detergent with the same amount of detergent.
59 569 M XX
EP
13190311.4
Panasonic Corporation
3
MN
20170626
A47L
US
2008236630
A1
KENNICHI SHIMOTERA [KR] ET AL
20081002
X
1-6,9
Y
7,8
* paragraphs [0036] - [0072] *
* paragraphs [0089] - [0091] *
* figures 1-3C *
WO
2012014441
A1
MATSUSHITA DENKI SANGYO KK
20120202
X
1,3,5,9
* abstract; claims 1-5; figures 1-6 *
EP
2599425
A1
PANASONIC CORP [JP]
20130605
* paragraphs [0015] - [0045] *
* claims 1-5; figures 1-6 *
EP
2319384
A1
MIELE & CIE [DE]
20110511
Y
7
A
1-6
* paragraphs [0008] - [0011] *
* paragraphs [0017] - [0019] *
* figures 1-6 *
FR
2593697
A1
ELTEK SPA [IT]
19870807
Y
8
* page 3, line 17 - page 4, line 4 *
* figure 2 *
WO
2006072481
A1
BOSCH SIEMENS HAUSGERAETE GMBH
20060713
A
5-9
* abstract; claims 1-19; figures 1-4 *
Weinberg, Ekkehard
Munich
20170614
US
2008236630
A1
20081002
CN
101273871
A
20081001
KR
20080088122
A
20081002
US
2008236630
A1
20081002
WO
2012014441
A1
20120202
CN
103052348
A
20130417
EP
2599425
A1
20130605
JP
5170327
B2
20130327
KR
20130031371
A
20130328
TW
201208631
A
20120301
WO
2012014441
A1
20120202
EP
2599425
A1
20130605
CN
103052348
A
20130417
EP
2599425
A1
20130605
JP
5170327
B2
20130327
KR
20130031371
A
20130328
TW
201208631
A
20120301
WO
2012014441
A1
20120202
EP
2319384
A1
20110511
NONE
FR
2593697
A1
19870807
DE
3701404
A1
19870813
FR
2593697
A1
19870807
IT
1187895
B
19871223
WO
2006072481
A1
20060713
BR
PI0519637
A2
20090303
CN
201012080
Y
20080130
DE
102004063284
A1
20060713
EP
1833350
A1
20070919
ES
2410855
T3
20130703
JP
4833996
B2
20111207
JP
2008525138
A
20080717
KR
20070089716
A
20070831
RU
2372831
C2
20091120
US
2010012158
A1
20100121
WO
2006072481
A1
20060713