ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESM..................
J
JDIM360 Ver 1.28 (29 Oct 2014) - 1620000/0
2789777
EUROPEAN PATENT APPLICATION
A3
20151118
EP
14164101.9
20140409
en
en
en
201306433
20130409
GB
20151118
201547
20141015
201442
E05B 15/02 20060101AFI20151015BHEP
E05B 47/06 20060101ALI20151015BHEP
E05B 13/00 20060101ALI20151015BHEP
E05B 63/16 20060101ALI20151015BHEP
de
Elektromechanischer Verriegelungsmechanismus
en
An electromechanical locking mechanism
fr
Mécanisme de verrouillage électromécanique
13
Access Control Technology Limited
101448972
10174EP
Unit C1 South City Business Centre Tallaght
Dublin 24
IE
McNamara, Martin
137 Castletown Leixlip
Kildare
IE
Dolan, Brendan
27 Woodlawn Rise Santry
Dublin 9
IE
Maguire, Rob
Ardlough Curragha Ashbourne
County Meath
IE
Maguire, Kevin
Apartment 2 Hybreasal House South Circular Road Kilmainham
Dublin 8
IE
O'Connor, Michael Donal
101286139
O'Connor Intellectual Property Suite 207, Q House Furze Road
Sandyford, Dublin 18
IE
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
20151118
201547
This invention relates to an electromechanical locking mechanism (1) comprising an inner escutcheon (5), an outer escutcheon (3), an inner handle (9), an outer handle (7), an inner spindle (13), an outer spindle (11), an inner spindle interlock (17), an outer spindle interlock (15) coupled to the inner spindle interlock and an electronic key reader (35) housed in the outer escutcheon. A latch (71) is mounted in the inner escutcheon (5) and is operable to releasably engage a notch (91) in the outer spindle interlock (17) and prevent rotation of the outer spindle interlock (15) and the outer spindle (11) when the latch (71) is engaged in the notch (91). The latch (71) is pivotably mounted in the inner escutcheon and pivots to and from a locking configuration in which part of the latch is located in the notch, and a release configuration in which the latch is free of the notch. The pivoting latch (71) will require less power to operate than linearly displaceable latches.
10174EP
EP
14164101.9
Access Control Technology Limited
13
DH
20151021
E05B
WO
2012122697
A1
SCHLAGE LOCK CO LLC [US]; ZHENG XUEWEN [CN]; LIU BIAO [CN]
20120920
X
1-3,5-7,13-15
* paragraph [0098] - paragraph [0099] *
A
4
* figures 1-5,15-16,25,26 *
US
2004003633
A1
ALEXANDER ARNON [US] ET AL
20040108
X
1-3,5,8-15
* paragraph [0038] - paragraph [0039] *
A
4
* figures 2-6 *
US
2011079057
A1
FROLOV GEORGE [US] ET AL
20110407
A
1,6,7
* paragraphs [0017] - [0018] *
* figures 1a,1b,1c *
DE
374125
C
WILHELM HUETTEMANN
19230420
A
1
* the whole document *
Bitton, Alexandre
The Hague
20151015
WO
2012122697
A1
20120920
AU
2011362542
A1
20131024
CN
103502549
A
20140108
EP
2683894
A1
20140115
NZ
616556
A
20150731
US
2014047878
A1
20140220
WO
2012122697
A1
20120920
US
2004003633
A1
20040108
AU
2003237818
A1
20031111
US
2004003633
A1
20040108
WO
03096292
A2
20031120
US
2011079057
A1
20110407
NONE
DE
374125
C
19230420
NONE