ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSK..HRIS..MTNORS..SM..................
J
DIM360 Ver 2.41 (21 Oct 2013) - 1100000/0
2803669
EUROPEAN PATENT APPLICATION
published in accordance with Art. 153(4) EPC
A1
20141119
EP
13786903.8
20130510
20140812
ko
en
en
20120049712
20120510
KR
20130052703
20130509
KR
20141119
201447
20141119
201447
C07F 11/00 20060101AFI20131128BHEP
C07F 7/10 20060101ALI20131128BHEP
C07F 7/20 20060101ALI20131128BHEP
de
ETHYLENOLIGOMERISIERUNGSVERFAHREN
en
ETHYLENE OLIGOMERIZATION METHOD
fr
PROCÉDÉ D'OLIGOMÉRISATION DE L'ÉTHYLÈNE
1
LG CHEM, LTD.
101427607
L11069WOEP
128, Yeoui-daero Yeongdeungpo-gu,
Seoul 150-721
KR
KWON, Heon-Yong
LG Chemical Development Corp. 104-1 Munji-dong Yuseong-gu
Daejeon 305-738
KR
LEE, Yong-Ho
LG Chemical Development Corp. 104-1 Munji-dong Yuseong-gu
Daejeon 305-738
KR
LIM, Kyoung-Chan
LG Chemical Development Corp. 104-1 Munji-dong Yuseong-gu
Daejeon 305-738
KR
LEE, Ki-Soo
LG Chemical Development Corp. 104-1 Munji-dong Yuseong-gu
Daejeon 305-739
KR
CHO, Min-Seok
LG Chemical Development Corp. 104-1 Munji-dong Yuseong-gu
Daejeon 305-738
KR
Goddar, Heinz J.
100002032
Boehmert & Boehmert Anwaltspartnerschaft mbB Patentanwälte Rechtsanwälte Pettenkoferstrasse 20-22
80336 München
DE
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
KR2013004159
20130510
ko
WO2013169069
20131114
201346
The present invention relates to a method for ethylene oligomerization. According so the method of the present invention, highly active ethylene oligomerization reaction is possible by using a catalyst system including a novel chromium compound exhibiting high activity for ethylene oligomerization reaction, and therefore, polyethylene can be prepared using a small amount of comonomers or using only ethylene without comonomers.

[Technical Field]
The present invention relates to a method for ethylene oligomerization. More particularly, the present invention relates to a method for ethylene oligomerization using a catalyst system including a novel chromium compound that exhibits high activity for ethylene oligomerization reaction.
This application claims the benefit of Korean Patent Application No. 10-2012-0049712 on May 10,2012 and Korean Patent Application No. 10-2013-0052703 on May 9,2013 with the Korean Intellectual Property Office, the disclosure of which is herein incorporated by reference in its entirety.

[Background Art]
Linear alpha-olefin is widely used in important commercial substances such as comonomers, detergents, lubricants, plasticizers or the like, and in particular, 1-hexene and 1-octene are commonly used as comonomers for controlling density of polyethylene during preparation of linear low density polyethylene (LLDPE).
In the conventional preparation process of LLDPE (Linear Low-Density Polyethylene), copolymerization of ethylene with alpha-olefin, for example, a comonomer such as 1-hexene and 1-octene is carried out in order to control density by forming branches in the polymer backbone.
Therefore, there is a problem that the comonomer increases the production cost of LLDPE having a high content of comonomers. Many different methods have been tried to solve this problem.
Further, because the application field or market size depends on the type of alpha-olefin, a technique capable of selectively producing a particular olefin is commercially important. Recently, many studies have been conducted on a chromium catalyst for preparing 1-hexene or 1-octene with a high selectivity through selective ethylene oligomerization.
The conventional commercial method for 1-hexene or 1-octene preparation is the SHOP process of Shell Chemical, the Ziegler Process of Chevron Philips, or the like, which is used to produce alpha-olefins having a wide distribution range from C4 ∼ C20 carbons.
Further, many studies have been conducted to selectively prepare 1-hexene or 1-octene by ethylene trimerization or tetramerization using an organic metal catalyst (J.Am.Chem.Soc 2003, 125, 5272, Ind.Eng.Chem.Res. 2008, 47, 5369, WO03/053890), but there is a still need for the catalysts exhibiting a sufficiently high activity.

[Disclosure]

[Technical Problem]
In order to solve the above problems of the conventional technology, an object of the present invention is to provide a method for ethylene oligomerization capable of maintaining high activity.

[Technical Solution]
In order to achieve the above object, the present invention provides a method for ethylene oligomerization, including the step of polymerizing ethylenes in the presence of a catalyst system including i) a ligand compound represented by the following Chemical Formula 1 and a chromium source, or ii) a chromium compound represented by the following Chemical Formula 2; and a cocatalyst. wherein R_1, R_2, R_2' and R_3 are the same as or different from each other, and each independently a hydrogen atom, a hydrocarbyl group having 1 to 30 carbon atoms, or a heterohydrocarbyl group having 1 to 30 carbon atoms, and
X is a halogen atom or an alkyl group having 1 to 6 carbon atoms.

[Advantageous Effects]
According to the preparation method of the present invention, highly active ethylene oligomerization reaction is possible. Therefore, it is possible to polymerize a low-density polyethylene in one reactor using only ethylene without injection of additional comonomers.

[Description of Drawings]
FIG. 1 is a graph showing the result of GC-MS of the products resulting from ethylene oligomerization according to Example 1 of the present invention.

[Best Mode]
The terminology used herein is for the purpose of describing particular embodiments only and is not intended to be limiting of the invention. The singular forms are intended to include the plural forms as well, unless the context clearly indicates otherwise. It will be further understood that the terms "includes, "comprises," or "has" when used in this specification, specify the presence of stated features, integers, steps, components, or combinations thereof, but do not preclude the presence or addition of one or more other features, integers, steps, components, or combinations thereof.
While the present invention is susceptible to various modifications and alternative forms, specific embodiments thereof are shown by way of example and will herein be described in detail. It should be understood, however, that these are not intended to limit the invention to the particular form disclosed, but on the contrary, the intention is to cover all modifications, equivalents and alternatives falling within the spirit and scope of the present invention.
Hereinafter, a method for ethylene oligomerization of the present invention will be described in detail.
The method for ethylene oligomerization of the present invention includes the step of polymerizing ethylenes in the presence of a catalyst system including i) a ligand compound represented by the following Chemical Formula 1 and a chromium source, or ii) a chromium compound represented by the following Chemical Formula 2; and a cocatalyst. wherein R_1, R_2, R_2' and R_3 are the same as or different from each other, and each independently a hydrogen atom, a hydrocarbyl group having 1 to 30 carbon atoms, or a heterohydrocarbyl group having 1 to 30 carbon atoms, and
X is a halogen atom or an alkyl group having 1 to 6 carbon atoms.
In the preparation method of the present invention, the catalyst system includes i) the ligand compound represented by Chemical Formula 1 and the chromium source, or ii) the chromium compound represented by Chemical Formula 2; and the cocatalyst.
The catalyst system can be used in ethylene polymerization reaction including ethylene oligomerization reaction.
As used herein, the term "catalyst system" means an active catalytic composition that can be obtained by adding three components of the chromium source, the ligand compound and the cocatalyst or alternatively two components of the chromium compound and the cocatalyst at the same time, or sequentially in any order in the presence or absence of any proper solvent in the presence or absence of monomers. The three components or two components of the catalyst system can be used without being supported on a support, or if necessary, they can be supported on the support to be used. That is, the catalyst system according to the present invention includes the ligand compound represented by Chemical Formula 1 and the chromium source, or the chromium compound represented by Chemical Formula 2 and the cocatalyst.
According to one embodiment of the present invention, the catalyst system may include the ligand compound represented by Chemical Formula 1, the chromium source and the cocatalyst. In this regard, a molar ratio of ligand compound: chromium source: cocatalyst may be approximately 1:1:1 to approximately 10:1:10,000, and preferably, approximately 1:1:100 to approximately 5:1:3,000. When the amount of the cocatalyst is too small to be within the range, complete activation of the catalyst does not occur to reduce activity of the catalyst system. On the contrary, when an excessive amount of the cocatalyst is included, excessive activator is economically infeasible in terms of productivity or acts as impurities to reduce purity of the product.
The catalyst system including the ligand compound represented by Chemical Formula 1, the chromium source and the cocatalyst can be obtained as an active catalyst by adding three components of the catalyst system at the same time, or sequentially in any order in the presence or absence of monomers in any proper solvent. The proper solvent may include substituted or unsubstituted hydrocarbons having 4 to 12 carbon atoms, and examples thereof may include heptane, benzene, toluene, diethyl ether, tetrahydrofuran, acetonitrile, dichloromethane, chloroform, chlorobenzene or the like, but is not limited thereto.
In Chemical Formulae 1 and 2, the hydrocarbyl group means a monovalent hydrocarbon group, and the heterohydrocarbyl group means a monovalent heterohydrocarbon group containing carbon atom and one or more heteroatoms.
According to one embodiment of the present invention, in Chemical Formula 1, R_1, R_2, R_2' and R_3 are each independently a hydrogen atom, an alkyl group having 1 to 20 carbon atoms, an alkenyl group having 2 to 20 carbon atoms, an aryl group having 6 to 14 carbon atoms, an alkylaryl group having 7 to 12 carbon atoms, an arylalkyl group having 7 to 12 carbon atoms or an alkoxyaryl group having 7 to 12 carbon atoms, but are not limited thereto.
Preferably, R_1, R_2, R_2' and R_3 are each independently a hydrogen atom, a linear alkyl group having 1 to 20 carbon atoms, an isopropyl group, a tert-butyl group, an amyl group, a phenyl group, an alkylphenyl group having 7 to 12 carbon atoms or an alkoxyphenyl group having 7 to 12 carbon atoms, but are not limited thereto.
According to one embodiment of the present invention, the ligand compound represented by Chemical Formula 1 may be selected from the following chemical structures, but the present invention is not limited thereto.
The compound represented by Chemical Formula 1 can be synthesized by the following method, but is not limited thereto. The preparation method of the ligand compound represented by Chemical Formula 1 will be described in detail in the following Examples.
The ligand compound represented by Chemical Formula 1 may further include the chromium source and the cocatalyst to be used in ethylene oligomerization reaction.
According to one embodiment of the present invention, the chromium source may be chromium or a chromium precursor. Specific examples of the chromium or chromium precursor may include chromium(III)acetylacetonoate, tris(tetrahydrofuran)chromium trichloride or chromium(III)-2-ethylhexanoate, but the present invention is not limited thereto.
According to another embodiment of the present invention, the catalyst system may include the chromium compound represented by Chemical Formula 2 and the cocatalyst. In this regard, the chromium compound represented by Chemical Formula 2 and the cocatalyst may be blended in a ratio of approximately 1:10 to approximately 1:10,000, and preferably, approximately 1:100 to approximately 1:1,000, based on the molar ratio of chromium and metal. When the amount of the cocatalyst is too small to be within the range, complete activation of the chromium compound does not occur to reduce activity of the catalyst system. On the contrary, when an excessive amount of the cocatalyst is included, excessive activator is economically infeasible in terms of productivity or acts as impurities to reduce purity of the product.
In the chromium compound represented by Chemical Formula 2, detailed descriptions and preferred examples of R_1, R_2, R_2', and R_3 are the same as in the descriptions of the ligand compound of Chemical Formula 1.
In Chemical Formula 2, X is a halogen atom or an alkyl group having 1 to 6 carbon atoms, and specific examples thereof may include methyl, ethyl, propyl, isopropyl, t-butyl, isobutyl or the like, but are not limited thereto.
According to one embodiment of the present invention, in Chemical Formula 2, X is preferably Cl or a methyl group, and more preferably Cl.
According to one embodiment of the present invention, the chromium compound represented by Chemical Formula 2 may be selected from the following chemical structures, but the present invention is not limited thereto.
The chromium compound represented by Chemical Formula 2 can be synthesized by the following method, but is not limited thereto. The preparation method of the chromium compound represented by Chemical Formula 2 will be described in detail in the following Examples.
In ethylene oligomerization reaction, the chromium compound represented by Chemical Formula 2 may be used singly or as the catalyst system including the cocatalyst. In particular, because highly active ethylene oligomerization reaction is possible, low-density polyethylene can be prepared in one reactor using a small amount of comonomers or using only ethylene without comonomers.
In the method for ethylene oligomerization of the present invention, the catalyst system includes the cocatalyst. The cocatalyst may be an organic metal compound containing the Group 13 metal. The organic metal compound containing the Group 13 metal is not particularly limited, as long as it can be generally used in olefin polymerization in the presence of a catalyst of a transition metal compound.
Specifically, the cocatalyst may be one or more selected from the group consisting of the compounds represented by the following Chemical Formulae 3 to 5, but the present invention is not limited thereto.
[Chemical Formula 3] -[Al(R_4)-O]c-
wherein R_4 is the same as or different from each other, and each independently a halogen radical, a hydrocarbyl radical having 1 to 20 carbon atoms, a halogen-substituted hydrocarbyl radical having 1 to 20 carbon atoms, and c is an integer of 2 or more,
[Chemical Formula 4] D(R_5)_3
wherein D is aluminium or boron, R_5 is hydrocarbyl having 1 to 20 carbon atoms or halogen-substituted hydrocarbyl having 1 to 20 carbon atoms,
[Chemical Formula 5] [L-H]+[Q(E)_4]-
wherein L is a neutral Lewis base, [L-H]+ is a Bronsted acid, Q is boron or aluminium in the +3 oxidation state, E is each independently an aryl group having 6 to 20 carbon atoms or an alkyl group having 1 to 20 carbon atoms in which one or more hydrogen atoms are substituted or unsubstituted with halogen, hydrocarbyl having 1 to 20 carbon atoms, an alkoxy functional group or a phenoxy functional group.
Examples of the compound represented by Chemical Formula 3 may include methylaluminoxane (MAO), ethyl aluminoxane, isobutyl aluminoxane, butyl aluminoxane or the like.
Examples of the alkyl metal compound represented by Chemical Formula 4 may include trimethylaluminium, triethylaluminium, triisobutylaluminium, tripropylaluminium, tributylaluminium, dimethylchloroaluminium, dimethylisobutylaluminium, dimethylethylaluminium, diethylchloroaluminium, triisopropylaluminium, tri-s-butylaluminium, tricyclopentylaluminium, tripentylaluminium, triisopentylaluminium, trihexylaluminium, ethyldimethylaluminium, methyldiethylaluminium, triphenylaluminium, tri-p-tolylaluminium, dimethylaluminiummethoxide, dimethylaluminiumethoxide, trimethylboron, triethylboron, triisobutylboron, tripropylboron, tributylboron or the like.
Examples of the compound represented by Chemical Formula 5 may include triethylammoniumtetraphenylboron, tributylammoniumtetraphenylboron, trimethylammoniumtetraphenylboron, tripropylammoniumtetraphenylboron, trimethylammoniumtetra(p-tolyl)boron, tripropylammoniumtetra(p-tolyl)boron, triethylammoniumtetra(o,p-dimethylphenyl)boron, trimethylammoniumtetra(o,p-dimethylphenyl)boron, tributylammoniumtetra(p-trifluoromethylphenyl)boron, trimethylammoniumtetra(p-trifluoromethylphenyl)boron, tributylammoniumtetrapentafluorophenylboron, N,N-diethylaniliniumtetraphenyl boron, N,N-diethylaniliniumtetraphenylboron, N,N-diethylaniliniumtetrapentafluorophenylboron, diethylammoniumtetrapentafluorophenylboron, triphenylphosphoniumtetraphenylboron, trimethylphosphoniumtetraphenylboron, triethylammoniumtetraphenylaluminium, tributylammoniumtetraphenylaluminium, trimethylammoniumtetraphenylaluminium, tripropylammoniumtetraphenylaluminium, trimethylammoniumtetra(p-tolyl)aluminium, tripropylammoniumtetra(p-tolyl)aluminium, triethylammoniumtetra(o,p-dimethylphenyl)aluminium, tributylammoniumtetra(p-trifluoromethylphenyl)aluminium, trimethylammoniumtetra(p-trifluoromethylphenyl)aluminium, tributylammoniumtetrapentafluorophenylaluminium, N,N-diethylaniliniumtetraphenylaluminium, N,N-diethylaniliniumtetraphenylaluminium, N,N-diethylaniliniumtetrapentafluorophenylaluminium, diethylammoniumtetrapentafluorophenylaluminium, triphenylphosphoniumtetraphenylaluminium, trimethylphosphoniumtetraphenylaluminium, triphenylcarboniumtetraphenylboron, triphenylcarboniumtetraphenylaluminium, triphenylcarboniumtetra(p-trifluoromethylphenyl)boron, triphenylcarboniumtetrapentafluorophenylboron or the like.
According to one embodiment of the present invention, the cocatalyst may be alumoxane, and preferably, methyl alumoxane (MAO) as alumoxane.
When ethylene oligomerization reaction is carried out according to the present invention, highly active ethylene oligomerization reaction is possible, and it is possible to polymerize low-density polyethylene in one reactor using only ethylene without additional injection of comonomers.
According to one embodiment of the present invention, the ethylene oligomerization reaction may be carried out at a temperature of approximately 5 to approximately 200°C, and preferably, at a temperature of approximately 30 to approximately 150°C, and more preferably, at a temperature of approximately 50 to approximately 110°C. In addition, the reaction may be carried out at a pressure of approximately 1 to approximately 300 bar, preferably at a pressure of approximately 2 to approximately 150 bar, and more preferably at a pressure of approximately 50 to approximately 100 bar. In terms of polymerization activity of the catalyst system and productivity, it is preferable that the ethylene oligomerization reaction is carried out within the above ranges of temperature and pressure.
The products of the ethylene oligomerization reaction according to the present invention may be obtained in the form of mixture due to Schultz-Flory distribution.

[Mode for Invention]
Hereinafter, the present invention will be described in more detail with reference to the following Examples. However, these Examples are illustrative purposes only, and the technical scope of the present invention is not limited thereto.

<Example>

Synthesis of ligand compound and chromium compound

Preparation Example 1

Preparation of {CH_3CH_2-S-Si(Me)_2-NH-Si(Me)_2-S-CH_2CH_3}CrCl_3[S-1 complex]

Preparation Example 1-1

Preparation of 1,3-dichlorohexamethyldisilazane
15.2 g of Hexamethyldisilazane, 32.2 g of dichlorodimethylsilane, and 100 mg of AlCl_3 were added to a Schlenk flask, and 150 mL of dichloromethane was added as a solvent. The mixture was stirred at 50°C for 3 days, and then the solvent was removed under vacuum. The crude product thus obtained was subjected to fractional distillation to give a colorless product.
(Yield: 80%)
^1H-NMR(500MHz, d_δ-benzene): δ(ppm) 1.10(br, 1H), 0.28(s, 12H)

Preparation Example 1-2

Preparation of CH_3CH_2-S-Si(Me)_2-NH-Si(Me)_2-S-CH_2CH_3[S-1 ligand]
1.06 g of 1,3-dichlorohexamethyldisilazane prepared in Preparation Example 1-1, 0.72 g of ethanethiol and 30 mL of THF were added to a Schlenk flask, and the mixture was cooled to - 78°C. Next, 1.75 mL of triethylamine was slowly added, and the temperature was raised to room temperature. The mixture was stirred. After terminating the reaction, the solvent and volatile materials were removed under vacuum. 100 mL of hexane was added to a flask and then filtered through a filter frit, and hexane was removed under vacuum to give a light yellow liquid product. (Yield 95%)
^1H-NMR(500MHz, CDCl_3): 8(ppm) 2.56(q, 4H), 1.30(t, 6H), 0.39(s, 12H)

Preparation Example 1-3

Preparation of {CH_3CH_2-S-Si(Me)_2-NH-Si(Me)_2-S-CH_2CH_3}CrCl_3 [S-1 complex]
52 mg of CH_3CH_2-S-Si(Me)_2-NH-Si(Me)_2-S-CH_2CH_3 prepared in Preparation Example 1-2 and 77 mg of CrCl_3(THF)_3 were added to a Schlenk flask, and 50 mL of THF was added and stirred. The solvent was removed under vacuum to give the title compound as a light gray solid.
(Yield 95%)

Preparation Example 2

Preparation of {CH_2(CH_2)_{10}-S-Si(Me)_2-NH-Si(Me)_2-S-(CH_2)_{10}CH_3}CrCl [S-2 complex]

Preparation Example 2-1

Preparation of CH_3(CH_2)_{10}-S-Si(Me)_2-NH-Si(Me)_2-S-(CH_2)_{10}CH_3 [S-2 ligand]
1.06 g of 1,3-dichlorohexamethyldisilazane prepared in Preparation Example 1-1,2.12 g of 1-dodecanethiol and 30 mL of THF were added to a Schlenk flask, and cooled to -78°C. Next, 1.75 mL of triethylamine was slowly added, and the temperature was raised to room temperature. Then, the mixture was stirred. After terminating the reaction, the solvent and volatile materials were removed under vacuum. 100 mL of hexane was added to a flask and then filtered through a filter frit, and hexane was removed under vacuum to give a light yellow liquid product. (Yield 93%)
^1H-NMR(500MHz, CDCl_3): δ(ppm) 2.57(q, 4H), 1.56(q, 4H), 1.35-1.20(m, 32H), 0.86(t, 6H), 0.40(s, 12H)

Preparation Example 2-2

Preparation of {CH_3(CH_2)_{10}-S-Si(Me)_2-NH-Si(Me)_2-S-(CH_2)_{10}CH_3}CrCl_3 [S-2 complex]
101 mg of CH_3(CH_2)_{10}-S-Si(Me)_2-NH-Si(Me)_2-S-(CH_2)_{10}CH_3 prepared in Preparation Example 2-1 and 60.9 mg of CrCl_3(THF)_3 were added to a Schlenk flask, 50 mL of THF was added thereto and stirred. The solvent was removed under vacuum to give the title compound as a light gray solid. (Yield 90%)

Preparation Example 3

Preparation of {(2-MeO)C_6H_4-S-Si(Me)_2-NH-Si(Me)_2-S-C_6H_4-(2-OMe)}CrCl_3 [S-3 complex]

Preparation Example 3-1

Preparation of (2-MeO)C_6H_4-S-Si(Me)_2-NH-Si(Me)_2-S-C_6H_4(2-OMe) [S-3 ligand
The compound was prepared in the same manner as in Preparation Example 2-1, except using 2-methoxythiophenol instead of 1-dodecanethiol. (Yield 84%)
^1H-NMR(500MHz, CDCl_3): 8(ppm) 7.39(q, 2H), 7.22(q, 2H), 6.84(m, 4H), 3.83(s, 6H), 1.25(brs, 1H), 0.25(s, 12H)

Preparation Example 3-2

Preparation of {(2-MeO)C_6H_4-S-Si(Me)_2-NH-Si(Me)_2-S-C_6H_4(2-OMe)}CrCl_3[S-3 complex]
412 mg of (2-MeO)C_6H_4-S-Si(Me)_2-NH-Si(Me)_2-S-C_6H_4(2-OMe) prepared in Preparation Example 3-1 and 377 mg of CrCl_3(THF)_3 were added to a Schlenk flask, and 20 mL of THF were added and stirred. The solvent was removed under vacuum to give the title compound as a light purple solid. (Yield 85%)

<Ethylene oligomerization reaction>

Example 1

Ethylene oligomerization reaction of S-1 complex]
The pressure of 500 ml-high pressure reaction vessel was reduced to vacuum, and then the internal environment was made to inactive condition using argon gas. Then, 250 ml of pure toluene was added, and methylaluminoxane (MAO) was added 600-fold of the Al/Cr molar ratio. Subsequently, a toluene solution (5 ml, 25 µmol of S-1 complex) of 5 mM S-1 complex catalyst of Preparation Example 1 was added and the solution reaction was carried out at 60°C for 1 hour under a 50 psig pressure of ethylene. Then, the activity was calculated from the increased weight of the solution after reaction and the weight of the reactor. The temperature of the reactor was reduced to 0°C, and then an HCl aqueous solution was slowly added to remove residual MAO and the catalyst. The organic layer was taken and filtered, and the produced polymer was separated and dried. Further, the organic layer was dried over MgSO_4 to remove the residual moisture, and then the composition of the organic layer was identified by GC-MS. As a result, a mixture of alpha-olefin polymers with Schultz-Flory distribution was identified.
A graph measured by GC-MS is shown in FIG. 1.

Example 2

Ethylene oligomerization reaction of S-1 complex]
Oligomerization reaction was carried out in the same manner as in Example 1, except that the reaction was carried out at a reaction temperature of 90°C in Example 1.

Example 3

Ethylene oligomerization reaction of S-2 complex]
Oligomerization reaction was carried out in the same manner as in Example 1, except that S-2 complex of Preparation Example 2 was used instead of S-1 complex in Example 1.

Example 4

Ethylene oligomerization reaction of S-2 complex]
Oligomerization reaction was carried out in the same manner as in Example 1, except that S-2 complex of Preparation Example 2 was used instead of S-1 complex and the reaction was carried out at a reaction temperature of 90°C in Example 1.

Example 5

Ethylene oligomerization reaction of S-3 complex]
Oligomerization reaction was carried out in the same manner as in Example 1, except that S-3 complex of Preparation Example 3 was used instead of S-1 complex in Example 1.

Example 6

Ethylene oligomerization reaction of S-3 complex
Oligomerization reaction was carried out in the same manner as in Example 1, except that S-3 complex of Preparation Example 3 was used instead of S-1 complex and the reaction was carried out at a reaction temperature of 90°C in Example 1.

Example 7

Ethylene oligomerization reaction of S-1 ligand compound and chromium source
The pressure of 500 ml-high pressure reaction vessel was reduced to vacuum, and then the internal environment was made to inactive condition using argon gas. Then, 250 ml of pure toluene was added, and methylaluminoxane (MAO) was added 600-fold of the Al/Cr molar ratio. Subsequently, a toluene solution (5 mM, 5 ml) of S-1 ligand compound of Preparation Example 1-2 was added to a 50 mL Schlenk flask, and the solution reaction was carried out at 90°C for 1 hour under a 50 psig pressure of ethylene. Then, the activity was calculated from the increased weight of the solution and the weight of the reactor. The temperature of the reactor was reduced to 0°C, and then an HCl aqueous solution was slowly added to remove residual MAO and the catalyst. The organic layer was taken and filtered, and the produced polymer was separated and dried. Further, the organic layer was dried over MgSO4 to remove the residual moisture, and then the composition of the organic layer was identified by GC-MS. As a result, a mixture of alpha-olefin polymers with Schultz-Flory distribution was identified.

Example 8

Ethylene oligomerization reaction of S-2 ligand compound and chromium source
Oligomerization reaction was carried out in the same manner as in Example 7, except that S-2 ligand compound was used instead of S-1 ligand compound in Example 7.

Example 9

Ethylene oligomerization reaction of S-3 ligand compound and chromium source
Oligomerization reaction was carried out in the same manner as in Example 7, except that S-3 ligand compound was used instead of S-1 ligand compound in Example 7.

Comparative Preparation Example 1

Preparation of {CH_3CH_2-S-(CH_3)_2-NH-Si(CH_3)_2-S-CH_2CH_3}CrCl_3 [T complex]
The title compound was prepared with reference to the previously reported literature, J.AM.CHEM.SOC. 2003, 125, 5272-5273.

Comparative Example 1
Oligomerization reaction was carried out in the same manner as in Example 1, except that T complex of Comparative Preparation Example 1 was used instead of S-1 complex and the reaction was carried out at a reaction temperature of 90°C in Example 1.
The results of ethylene oligomerization reaction of Examples 1 to 9 and Comparative Example 1 are shown in Table 1.

[Table 1]
| Catalyst | Reaction temperature (unit: °C) | Activity (unit: g/g of Cr/hr)
Example 1 | S-1 complex | 60 | 13,850
Example 2 | S-1 complex | 90 | 9,540
Example 3 | S-2 complex | 60 | 29,160
Example 4 | S-2 complex | 90 | 19,341
Example 5 | S-3 complex | 60 | 7,615
Example 6 | S-3 complex | 90 | 1,923
Example 7 | S-1 ligand/chromium source | 90 | 9,120
Example 8 | S-2 ligand/chromium source | 90 | 20,301
Example 9 | S-3 ligand/chromium source | 90 | 1,510
Comparative Example 1 | T complex | 90 | 2,510
Referring to Table 1, when ethylene oligomerization reaction was carried out using the catalyst system including the compound of the present invention, highly active ethylene oligomerization reaction was possible.
Referring to FIG. 1, when ethylene oligomerization reaction according to one embodiment of the present invention was carried out, it was found that alpha-olefin polymer products were obtained in the form of mixture according to Schultz-Flory distribution.
1. A method for ethylene oligomerization, comprising the step of polymerizing ethylenes in the presence of a catalyst system including i) a ligand compound represented by the following Chemical Formula 1 and a chromium source, or ii) a chromium compound represented by the following Chemical Formula 2; and a cocatalyst: wherein R_1, R_2, R_2' and R_3 are the same as or different from each other, and each independently a hydrogen atom, a hydrocarbyl group having 1 to 30 carbon atoms, or a heterohydrocarbyl group having 1 to 30 carbon atoms, and
X is a halogen atom or an alkyl group having 1 to 6 carbon atoms.
2. The method according to claim 1, wherein R_1, R_2, R_2' and R_3 are each independently a hydrogen atom, an alkyl group having 1 to 20 carbon atoms, an alkenyl group having 2 to 20 carbon atoms, an aryl group having 6 to 14 carbon atoms, an alkylaryl group having 7 to 12 carbon atoms, an arylalkyl group having 7 to 12 carbon atoms or an alkoxyaryl group having 7 to 12 carbon atoms.
3. The method according to claim 1, wherein R_1, R_2, R_2' and R_3 are each independently a hydrogen atom, a linear alkyl group having 1 to 20 carbon atoms, an isopropyl group, a tert-butyl group, an amyl group, a phenyl group, an alkylphenyl group having 7 to 12 carbon atoms or an alkoxyphenyl group having 7 to 12 carbon atoms.
4. The method according to claim 1, wherein X is Cl or a methyl group.
5. The method according to claim 1, wherein the compound represented by Chemical Formula 1 is one of the following chemical structures:
6. The method according to claim 1, wherein the compound represented by Chemical Formula 2 is one of the following chemical structures:
7. The method according to claim 1, wherein chromium source is selected from the group consisting of chromium(III)acetylacetonoate, tris(tetrahydrofuran)chromium trichloride, and chromium(III)-2-ethylhexanoate.
8. The method according to claim 1, wherein the cocatalyst is one or more selected from the group consisting of the compounds represented by the following Chemical Formulae 3 to 5:
[Chemical Formula 3] -[Al(R_4)-O]c-
wherein R_4 is the same as or different from each other, and each independently a halogen radical, a hydrocarbyl radical having 1 to 20 carbon atoms, a halogen-substituted hydrocarbyl radical having 1 to 20 carbon atoms, and c is an integer of 2 or more,
[Chemical Formula 4] D(R_5)_3
wherein D is aluminium or boron, R_5 is hydrocarbyl having 1 to 20 carbon atoms or halogen-substituted hydrocarbyl having 1 to 20 carbon atoms,
[Chemical Formula 5] [L-H]+[Q(E)_4]-
wherein L is a neutral Lewis base, [L-H]+ is a Bronsted acid, Q is boron or aluminium in the +3 oxidation state, E is each independently an aryl group having 6 to 20 carbon atoms or an alkyl group having 1 to 20 carbon atoms in which one or more hydrogen atoms are substituted or unsubstituted with halogen, hydrocarbyl having 1 to 20 carbon atoms, an alkoxy functional group or a phenoxy functional group.
9. The method according to claim 1, wherein the method is carried out at a temperature of 5 to 200°C and a pressure of 1 to 300 bar.

REFERENCES CITED IN THE DESCRIPTION
This list of references cited by the applicant is for the reader's convenience only. It does not form part of the European patent document. Even though great care has been taken in compiling the references, errors or omissions cannot be excluded and the EPO disclaims all liability in this regard.

Patent documents cited in the description
- KR
1020120049712
20120510
[0002]
- KR
1020130052703
20130509
[0002]
- WO
03053890
A
[0008]

Non-patent literature cited in the description
- J.Am.Chem.Soc
20030000
125
5272
[0008]
- Ind.Eng.Chem.Res.
20080000
47
5369
[0008]
- J.AM.CHEM.SOC.
20030000
125
5272
5273
[0063]