ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSK..HRIS..MTNORS..SM..................
*
J
BDM Ver 0.1.63 (23 May 2017) - 2100000/0
2893292
EUROPEAN PATENT SPECIFICATION
B1
20180207
EP
13762968.9
20130905
20141210
en
en
en
201261697624 P
20120906
US
20180207
201806
20150715
201529
20180207
201806
20171006
G01B 5/30 20060101AFI20140326BHEP
de
FERN-ARMBETÄTIGUNG EINES DEHNUNGSMESSERS
en
EXTENSOMETER REMOTE ARM ACTUATION
fr
ACTIONNEMENT DE BRAS D'EXTENSOMÈTRE À DISTANCE
CN-U- 201 740 701
US-A- 2 085 687
CASTRO, Fernando L.
c/o Illinois Tool Works Inc. 3600 West Lake Avenue
Glenview, Illinois 60026
US
TSIOMPLIKAS, Peter
c/o Illinois Tool Works Inc. 3600 West Lake Avenue
Glenview, Illinois 60026
US
Illinois Tool Works Inc.
101433274
A/ITW-359-PC/EP
155 Harlem Avenue
Glenview, IL 60025
US
Trinks, Ole
101100295
Meissner Bolte Patentanwälte Rechtsanwälte Partnerschaft mbB Postfach 10 26 05
86016 Augsburg
DE
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
US2013058337
20130905
en
WO2014039728
20140313
201411
20150715
201529

BACKGROUND OF THE DISCLOSURE

Field of the Disclosure
The present disclosure relates to an extensometer wherein the actuation of the arms is performed by a separate rotating bar.

Description of the Prior Art
An extensometer is an instrument that very accurately measures the extension of a test specimen in order to better capture the material properties of the specimen. A common extensometer is of the contacting type, which physically tracks two points in the specimen as the test takes place. These contacting points are typically in the form of arms that reach from the main body of the extensometer to the specimen location.
For automatic contacting extensometers, it is necessary to have a means to make the contacting arms attach to and detach from the test specimen. Existing products make use of actuators, usually electric motors that are mounted to each of the two moving arms.
During a test, the load cell on a test frame measures the force that is applied to the specimen. Since the arms are contacting the specimen, the load cell output will include not just the force applied to the specimen but also the additional force required to move the contacting arms. The force required to move these arms is called the running force. The running force also causes the contacting arms to deflect, causing errors in the extensometer readings. For these reasons, minimizing the running force is crucial to load output accuracy and extension accuracy.
The idea of an external bar being used to remotely actuate the arms has been used before in an extensometer, notably the MFL by Mess & Feinwerktechnik (MF) shown on Figure 1. The device in Figure 1 does not use a linear encoder to measure the displacement of the arms.
The actuation method employed in Figure 1 is based on the use of two eccentrically-mounted shafts that operate in a cam-action as shown in Figure 2. Driven from a common actuator shown in Figure 3, the cam bars move synchronously until the high point rotates into contact with a tab on each arm of the arm pair, forcing the arms open as shown in Figure 4.
Another prior art approach is to have a system where sensitive strain gauges are attached to the ends of the arms. The device then lets the strain gauges track the displacement of the specimen until the end of the very limited travel of the strain gauges is about to be reached, at which point the instrument uses actuators to move the arms in the direction of specimen elongation to provide slack and allow more strain gauge travel. As a result, this architecture is immune to increased friction. The arm location is driven by motors even during testing, and not by the specimen itself.
A remote arm actuation for extensometer is known from CN 201 740 701 U.
A further example of extensometer is shown in US 2 085 687 A.

SUMMARY OF THE DISCLOSURE
The objective according to the invention is achieved by an extensometer comprising the features of claim 1. The dependent claims further develop the idea of the present invention.
The disclosure allows the actuation of the arms to be removed from the arms by use of a separate rotating bar so as to avoid or minimize placing active mechanics onto the arms. The disclosure overcomes many challenges and successfully packages the mechanism fully inside the instrument, resulting in many advantages. Many of the typical advantages are the result of implementing the rotating bar inside the unit, with a unique method of transferring the rotational motion of the bar located in the back of the extensometer, yet actuating the arms which are located in front and outside of the instrument.

BRIEF DESCRIPTION OF THE DRAWINGS
Further objects and advantages of the disclosure will become apparent from the following description and from the accompanying drawings, wherein:
- Figures 1-4 are illustrations of the prior art.
- Figure 5 is perspective view of the rotating bar mechanism on the lower arm of a first embodiment of the present disclosure.
- Figure 6 is a perspective view of the arm actuation mechanism of a first embodiment of the present disclosure.
- Figure 7 is a top cross-sectional view of the arm actuation mechanism of the first embodiment of the present disclosure.
- Figure 8 is a perspective view of a portion of the mechanism of the first embodiment of the present disclosure.
- Figures 9a and 9b are side perspective and top plan views of a mechanism of the first embodiment of the present disclosure, for limiting angular displacement.
- Figures 10a and 10b are side plan views of a mechanism the first embodiment of the present disclosure for eliminating bar contact during carriage travel.
- Figure 11 is a perspective view of the first embodiment of the present disclosure.
- Figures 12-14 are additional views of alternative mechanisms of the first embodiment of the present disclosure.
- Figures 15 and 16 are perspective views of a mechanism that holds the angular position of the rotating spool.
- Figure 17 is a perspective view of the opening bar system of a second embodiment of the present disclosure.
- Figures 18a and 18b are top and bottom views, respectively, of the rotating bar pivot points of a second embodiment of the present disclosure.
- Figure 19 is a perspective view of the arms in the closed position in the second embodiment of the present disclosure.
- Figure 20 is a perspective view of the arms in the open position in response to the rotation of the bar in the second embodiment of the present disclosure.
- Figure 21 is a perspective view of a sliding roller in the second embodiment of the present disclosure.
- Figures 22-27 are further perspective views of the further embodiments of the present disclosure.

DETAILED DESCRIPTION OF THE PREFERRED EMBODIMENTS
Referring now to the drawings in detail wherein like numerals indicate like elements throughout the several views, one sees that Figure 1, while prior art, illustrates the general structure of an extensometer 1000. The extensometer 1000 includes an upper arm assembly 1002 and a lower arm assembly 1004 which are vertically aligned with each other along a vertical track 1006. Upper arm assembly 1002 includes two horizontally opposed contacting arms 1008, 1010 while lower arm assembly 1004 includes two horizontally opposed contacting arms 1012, 1014. The horizontally opposed contacting arms are pivotably articulated to grip respective ends of a specimen (not shown). Typically, then the upper and lower arm assembly track the movement of engaged points on the sample thereby measuring strain in response to grips (not shown) which impart a stress on the sample. The resulting strain on the sample, in response to the stress, is measured and plotted in order to determine the characteristics of the sample. However, the device of Figure 1 does not use a linear encoder to measure the displacement of the arms.
Figures 2-4 show the details of the arm assemblies 1002, 1004 and the vertical track 1006 of the prior art embodiment of Figure 1.
Figures 5-7 are perspective views the lower arm mechanism 12 and associated rotating bar mechanism 14 of an embodiment of the extensometer 10 of the present disclosure. Lower arm mechanism 12 is mounted on a carriage 100 which rides on vertical tracks 102 in response to pulley mechanism 104. Lower arm mechanism 12 further includes first lower contacting arm 16 and second lower contacting arm 18 which can be urged together in a gripping configuration by contact force adjustment assembly 19, which may be manually operated. As best shown in Figure 7, first and second lever arms 20, 22 have respective first and second distal ends 24, 26 pivotably attached to the central interior portions of first and second lower contacting arms 16, 18. First and second lower lever arms 20, 22 further include respective first and second central pivot points 28, 30, pivotably mounted on cross-support member 32. First and second ends 33, 35 of cross-support member 32 provide a resilient flexible mount for the proximal ends 37, 39 of respective first and second lower contacting arms 16, 18. First and second lower lever arms 20, 22 further include first and second proximal ends 34, 36 which include respective first and second boss roller elements 38, 40. First and second boss roller elements 38, 40 are captured or engaged so as to travel within respective first and second inclined guide slots 42, 44 formed in a V-type configuration within wedge 46. Wedge 46 is biased by compression spring 48, mounted between first and second proximal ends 34, 36 of respective first and second lower lever arms, which urges first and second proximal ends 34, 36 apart, thereby urging wedge 46 in the left-hand direction of the orientation of the illustration in Figure 7. When compression spring 48 urges the wedge 46 to a more left-hand position than shown in Figure 7, the first and second roller elements 38, 40 are further separated from each other by the inclined configuration of guide slots 42, 44 thereby urging the first and second lever arms 20, 22 together thereby urging the first and second lower contacting arms 16, 18 together.
Wedge 46 is further attached to metal belt 50 (which may be implemented as a thin stainless steel shim), which is guided by rollers 52, 54, 56 and wrapped around spool 58 which is mounted on rotating bar 60. Rotating bar 60 goes through the arm assemblies inside of the extensometer. When bar 60 rotates, it winds the metal belt 50 around spool 58, thereby pulling wedge 46 to the right-most position in Figure 7 (acting against the force of compression spring 48), thereby urging the first and second roller elements 38, 40 toward each other and pivoting the first and second lower contacting arms 16, 18 to an open position. This operation is done with no direct cam action on the part of rotating bar 60, but rather by the motion of the metal belt 50. As the bar 60 rotates clockwise, the spool 58 coils up the metal belt 50 and it in turn goes around the main structure of the extensometer 10 by means of rollers 52, 54, 56 until it pulls on wedge 46 and causes the motions as described above. By way of compression spring 48 urging first and second proximal ends 34, 36 apart, the extensometer 10 works in the opposite way and returns to its closed position when the motor rotates bar 60 counter-clockwise. A single rotating bar 60 is provided for the extensometer 10, with a separate spool 58 provided on bar 60 for each of the lower and upper arm assemblies 12, 13. In this manner, the contacting arms of the lower and upper arm assemblies 12, 13 typically operate in unison.
Figure 7 further illustrates how the first embodiment of the present disclosure prevents contact with the rotating bar 60 during arm carriage motion. In an encoder-based extensometer architecture, having a rotating bar actuate the arms to open and close creates a substantial obstacle in that the bar 60 must stop making contact after opening and after closing. The requirement comes as a result of the added friction on the arm assemblies due to the bar 60 making contact with the rolling assemblies to which the arms are attached. An objective in a contacting extensometer may be the goal of making the complete arm subassembly carriage have reduced or eliminated running forces due to weight which impinge upon critical elements (i.e., sometimes referred to by those skilled in the art as being "weightless"). The arm carriages typically would have to be precisely counter-balanced and significant effort must be invested in keeping rolling surfaces as frictionless as possible. This is typically difficult to accomplish in order to maintain accuracy that having the bar making contact during testing is typically not practically feasible. The added friction would deflect the contacting arms and the forces required to move the carriages would typically both be expected to produce large errors.
As a result, a mechanism is provided to back-drive the bar 60 from its open or closed angular position to a free position where there is no contact with the spool 58, which is mounted on spool bearing 85 on base plate 87. As shown on Figure 8, a vertically camming bearing profile 66 is provided along the outer edge of spool 58, upon which small bearing 68 rides. The bearing 68 is attached to a spring-loaded flexure 70 (which may be provided by a torsion spring assembly) that always ensures downward preloading. The vertically camming bearing profile 66 upon which the bearing 68 rides has a pocket 72 to capture or to detent engage bearing 68 in the lower closed position, and another in the upper open position (not shown). The upper open position may also be implemented with a stop pin rather than a pocket, because spring-loaded flexure 70 forces in the arms to bias the mechanism towards this position. The force of the spring-loaded flexure 70 also typically requires a precise shaping of vertically camming bearing profile 66, as opposed to a horizontal surface which may cause the first and second contacting arms 16, 18 to snap closed, which is unacceptable as the sharp contact points in the arms may damage specimens. This mechanism is intended to eliminate bar contact during carriage travel. Additionally, the rear of carriage 100 includes a bearing 99 for riding in track 101.
In order to improve the performance of the vertically camming bearing profile, the motor typically must be controlled in such a way as to know when to stop turning and reverse direction, and when to stop the reverse motion and position itself in the free range. In other words, angular displacement must be limited so that the range of rotation of the rotating bar 60 is controlled. As shown on Figure 9a, in order to minimize or reduce expensive motion control, at the top of the bar 60 there is a flat wedge 76 with radial edges 78, 80 (i.e., pie-shaped or partially circular) that cross the path of a fixed optical switch 81 as it rotates with the bar 60. The radial edges 78, 80 break the optical signal and trigger the motor to stop or reverse, in effect acting as a rotary encoder. This not only typically rotationally positions the bar 60 to be in an accurate and repeatable stop in the contact-free zone, but also stops the motor reverse direction at a precise point without over-torqueing the carriage assemblies. Figure 9b shows a top view of the mechanism with the bar 60 in the middle of the contact-free position.
Figures 10a and 10b illustrate the advantages of moving the bar inside, to the back of the extensometer 10. An objective of an extensometer 10 may be to reach over a set of grips or other similar devices holding a specimen. As such, the amount of reach of the contacting arms is absolutely necessary for the instrument to be compatible with larger grips. There are, however, practical limitations as to how far arms can reach. The distance from the contacting point of the arms to the point where the measurement is made inside is incredibly sensitive to minute deflections, bearing surface imperfections, and increases in drag. Consequently, maximizing the amount of that distance devoted to actual test reach is crucial. This, in effect, means that any distance forward of the measurement encoder not free to clear grips is lost reach. Placing the mechanism at the back means zero reach lost to the actuation mechanism. For reference, note the difference in reach from an earlier concept using an external bar on Figure 10a versus the internal bar on Figure 10b. In an embodiment of the disclosure illustrated in Figure 10b, over 65 millimeters of additional reach resulted from the internal packaging of the bar at the rear of the extensometer, as compared to the extensometer of Figure 10a.
Figure 11 is a perspective view of an embodiment of extensometer 10, including lower arm mechanism 12 and upper arm mechanism 13 (with substantially the same structure as lower arm mechanism 12, but typically inverted) while Figures 12-14 include further alternative variations of the disclosure.
Figures 15 and 16 pertain to a mechanism of the spool bearing 85, mounted on base plate 87 of carriage 100, that holds the angular position of the rotating spool 58 to prevent contact with the bar 60. This design has a similar cam structure 66 as illustrated in Figure 8 and is based on the use of torsion springs 92 to pivotably mount plate 94 onto plate 96, wherein rollers 95 are mounted on plate 94 are biased against cam structure 66 by the force of torsion springs 92, rather than the spring-loaded flexure 70 of Figure 8, to provide substantially improved life. The ramp and pocket geometry is implemented by cam structure 66 and pocket 72, wherein pocket 72 can capture one of rollers 95.
The second embodiment of the disclosure is illustrated in Figures 17-21. Figure 17 is a perspective view of the opening bar system of the second embodiment of this disclosure. In this second embodiment, the rotating bar or opening bar 60 is supported on top and bottom by respective upper and lower pivots or bearings 82, 84 as shown in Figures 18a and 18b thereby allowing it to rotate along its length. The aspect ratio of the rotating bar 60 enables the device to be clear of the arms of lower and upper arm mechanisms 12, 13 in the closed arm position of Figure 19. This clearance is typically important as it eliminates friction between the opening bar 60 and the arms 16, 18 of the lower and upper arm mechanisms 12, 13, thereby enabling the arms to follow the test sample with minimal drag. When the bar 60 is rotated so that its wider dimension is transverse between the arms 16, 18, the arms 16, 18 are forced open, the edges of the bar 60 engage with the spring-loaded sliding rollers 86, 87 (which are freely rotating and traverse a longitudinal portion of arms 16, 18) thereby reducing the friction between the opening bar 60 and the arms 16, 18. The arms 16, 18 are forced open by the rotated bar 60 as illustrated in Figures 20 and 21. The opening bar 60 can be motor driven or manually operated. The arms 16, 18 themselves contain sliding runners that are free to rotate. The vertical rollers 90 illustrated in Figure 21 allow the lower and upper arm mechanisms 12, 13 to travel vertically while the opening bar is engaged. In summary, the rotating bar mechanism is used to open and close two sets of hinged mechanical arms on a long travel extensometer.
Figures 22-27 are further perspective views of the further embodiments of the present disclosure. These embodiments include a device to mitigate debris from entering the device by the use of a constant force spring acting as a roll-up shade-type configuration and an improved way to repeatably adjust the tension of the spring that controls the amount of force the contacting arms puts on the specimen.
The tensioner assembly, shown on Figures 24-26, includes knob 209 with markings which controls the extension of spring 211, which draws arms 214, 215 together. One end of spring 211 is held captive to arm 215 by means of a swiveling anchor, thereby allowing the spring to rotate freely on that end. At the other end of spring 211, the spring is held captive to arm 214 by being attached to threaded knob 209. Knob 209 is threaded against a threaded sleeve 208 that is fixed on to arm 214. As knob 209 is rotated, it changes the length of extension spring 211, altering the force with which spring 211 pulls the contacting arms 214, 215 together. In addition, as knob 209 is rotated along the threads, more or less of knob 209 is exposed from beneath threaded sleeve 208. The amount of knob 209 exposed can be quantified by markings on knob 209. As a result, a user can rotate knob 209 to a desired contacting force setting and use the exposed markings on it as reference to achieve the same contacting force in future tests.
Figures 22-24 and 27 show the debris shield assemblies. There are two debris shield assemblies (upper and lower, mirrored) including a constant-force-spring 200 coiled around a spool assembly 202. Spring 200 is fed along channels on bilateral extrusions 203 and attached to a bracket 204 by means of a clamp 212. Bracket 204 is secured onto extrusion 203 using slide 207 on the opposite side. These two parts are clamped together with knob 206. Indicator plate 205 covers slide 207. The travel limit assemblies can slide vertically along features on extrusion 203 until the desired location. The user then tightens knob 206 and the vertical location becomes fixed. The extensometer design makes use of travel limits to protect the arms assemblies from damage by running into fixed objects in the test setup. The apparatus makes use of these travel limit assemblies to uncoil and recoil the constant force spring covering up gaps between extrusions 203 on positions the contacting arms will not use during a test. As a result, the open area of the extensometer is minimized and can thus mitigate the amount of debris from broken specimens and other environmental contaminants from finding their way into the extensometer. Element 216 shows areas covered by the debris shield assembly and element 217 shows exposed areas open to the inside of the extensometer. As the user sets the limits of travel, the apparatus automatically covers up unused areas with a low-cost design.
In conclusion, the instrument will benefit from the inherent protection the mechanism gets by being inside the instrument. Specimen breaks can be very violent, dusty, and can send sections of specimens as projectiles. Also, any noise produced by the mechanism is muffled by being inside. The look of the instrument becomes cleaner and sleeker. Finally, this mechanism is less expensive, as there is no need for external covers or cosmetic consideration.
The resulting apparatus typically achieves several advantages. If using an external rotating bar to actuate the arms, redesigned arms would be required to develop a longer-reach variant extensometer, an expensive and difficult technical task considered a sub-project on its own. With this disclosure, the arms typically do not change. Typically only the simple piece connecting the arms to the carriage needs to grow along with the length of the simple metal belt. This advantage is in addition to the aforementioned gain in reach by removing the mechanism itself. Together, this disclosure improves feasible arm reach while keeping development and part costs low.
Similarly, there is a growing need in the marketplace to use extensometers in high-temperature applications. By removing the actuating mechanism form the front of the instrument and being able to extend just one part with a thin cross section to gain additional reach, this product will readily be able to be configured for use in high-temperature chambers inside of which the arms must fully reside. The design can be easily adapted to only have high temperature-safe materials where required and the chamber opening can remain small.
Thus the several aforementioned objects and advantages are most effectively attained. Although preferred embodiments of the invention have been disclosed and described in detail herein, it should be understood that this invention is in no sense limited thereby and its scope is to be determined by that of the appended claims.
1. An extensometer including:
a first arm assembly (12) and a second arm assembly (13), each arm assembly including first and second reciprocating contact arms (16, 18);
the first and second arm assemblies (12, 13) each including:
a camming element (46), each camming element including first and second inclined camming slots (42, 44), which are inclined with respect to each other,
a first lever arm (20) with a first proximal end (34) engaged within the first inclined camming slot (42) and a first distal end (24) engaged with the first contacting arm (16), and a first pivot point (28) between the first proximal end (34) and the first distal end (24);
a second lever arm (22) with a second proximal end (36) engaged within the second inclined camming slot (44) and a second distal end (26) engaged with the second contacting arm (18), and a second pivot point (30) between the second proximal end (36) and the second distal end (26);
a support member (32) upon which the first and second pivot points (38, 30) are pivotably mounted;
wherein when the camming element (46) is in a first position, the first and second contact arms (16, 18) are urged toward each other and wherein when the camming element (46) is in a second position, the first and second contact arms (16, 18) are urged away from each other; and
a drive mechanism configured to urge the camming element (46) from the first position to the second position, the drive mechanism being separated from the camming element; said extensometer further comprising a vertical track structure (102) upon which the first and second arm assemblies (12, 13) are configured to travel.
2. The extensometer of Claim 1 wherein each support member (32) includes a first end (33) to which a proximal end (37) of the first contact arm (16) is resiliently flexibly mounted, and a second end (35) to which a proximal end (39) of the second contact arm (18) is resiliently flexibly mounted.
3. The extensometer of Claim 2 wherein the camming element is a wedge (46) with said first and second inclined camming slots (42, 44), and wherein the first and second proximal ends (34, 36) of the respective first and second lever arms (20, 22) include respective first and second boss roller elements (38, 40) which are engaged so as to travel within the respective first and second inclined camming slots (42, 44).
4. The extensometer of Claim 3 wherein the first and second arm assemblies (12, 13) each include a spring (48) for biasing the camming element (46) toward the first position.
5. The extensometer of Claim 4 wherein the drive mechanism includes a rotating element (60) which rotates a spool (58), and wherein the extensometer further includes a belt (50) with a first end attached to the camming element (46) and a second end attached the spool (58), whereby when the rotating element (60) is rotated, the spool (58) rotates, thereby pulling the belt (50) and urging the camming element (46) from the first position to the second position.
6. The extensometer of Claim 1 wherein the first and second contact arms (16, 18) of the first and second arm assemblies (12, 13) are on a first side of the track structure (102) and the rotating element (60) is on the other side of the track structure.
7. The extensometer of Claim 6 wherein the rotating element is a rotating bar (60), and wherein the rotating bar is attached to an element with edges (78 80) which move in response to rotation of the rotating bar (60) and operate a switch (81) to indicate the desired range of motion of the rotating bar.
8. The extensometer of Claim 7 wherein the element (60) includes radially oriented edges and wherein the switch (81) is an optical switch.
9. The extensometer of Claim 8 wherein the spool (58) is mounted on a spool bearing (85), the spool bearing including a cammed surface with at least one pocket (72), and wherein the extensometer further includes a spring-loaded mechanism for engaging the at least one pocket (72) thereby maintaining an angular orientation of the spool (58).
10. The extensometer of Claim 5 wherein the belt (50) is mounted on at least one roller (52, 54, 56) so that the belt passes from the first side to the second side of the vertical track structure (102).
1. Dehnungsmesser, der Folgendes beinhaltet:
eine erste Armanordnung (12) und eine zweite Armanordnung (13), wobei jede Armanordnung erste und zweite wechselbewegliche Kontaktarme (16, 18) beinhaltet, wobei die ersten und zweiten Armanordnungen (12, 13) jeweils beinhalten:
ein Nockenelement (46), wobei jedes Nockenelement erste und zweite geneigte Nockenschlitze (42, 44) beinhaltet, die im Verhältnis zueinander geneigt sind;
einen ersten Hebelarm (20) mit einem ersten proximalen Ende (34), das in den ersten geneigten Nockenschlitz (42) eingreift, und mit einem ersten distalen Ende (24), das in den ersten Kontaktarm (16) eingreift, wobei sich ein erster Schwenkpunkt (28) zwischen dem ersten proximalen Ende (34) und dem ersten distalen Ende (24) befindet;
einen zweiten Hebelarm (22) mit einem zweiten proximalen Ende (36), das in den zweiten geneigten Nockenschlitz (44) eingreift, und mit einem zweiten distalen Ende (26), das in den zweiten Kontaktarm (18) eingreift, wobei sich ein zweiter Schwenkpunkt (30) zwischen dem zweiten proximalen Ende (36) und dem zweiten distalen Ende (26) befindet;
ein Stützelement (32), an dem die ersten und zweiten Schwenkpunkte (38, 30) schwenkbar montiert sind;
wobei, wenn sich das Nockenelement (46) in einer ersten Position befindet, die ersten und zweiten Kontaktarme (16, 18) zueinander hin gedrängt werden, und wobei, wenn sich das Nockenelement (46) in einer zweiten Position befindet, die ersten und zweiten Kontaktarme (16, 18) voneinander weggedrängt werden; und
einen Antriebsmechanismus, der konfiguriert ist, um das Nockenelement (46) aus der ersten Position in die zweite Position zu drängen, wobei der Antriebsmechanismus vom Nockenelement getrennt ist;
wobei der Dehnungsmesser weiterhin umfasst:
eine vertikale Schienenstruktur (102), die so konfiguriert ist, dass sich die ersten und zweiten Armanordnungen (12, 13) darauf bewegen können.
2. Dehnungsmesser nach Anspruch 1, wobei jedes Stützelement (32) ein erstes Ende (33), an dem ein proximales Ende (37) des ersten Kontaktarms (16) elastisch flexibel montiert ist, sowie ein zweites Ende (35) beinhaltet, an dem ein proximales Ende (39) des zweiten Kontaktarms (18) elastisch flexibel montiert ist.
3. Dehnungsmesser nach Anspruch 2, wobei das Nockenelement ein Keil (46) mit den ersten und zweiten geneigten Nockenschlitzen (42, 44) ist, und wobei die ersten und zweiten proximalen Enden (34, 36) der jeweiligen ersten und zweiten Hebelarme (20, 22) jeweilige erste und zweite Nabenrollenelemente (38, 40) beinhalten, die so in Eingriff stehen, dass sie sich innerhalb der jeweiligen ersten und zweiten geneigten Nockenschlitze (42,44) bewegen können.
4. Dehnungsmesser nach Anspruch 3, wobei die ersten und zweiten Armanordnungen (12, 13) jeweils eine Feder (48) beinhalten, um das Nockenelement (46) hin zur ersten Position vorzuspannen.
5. Dehnungsmesser nach Anspruch 4, wobei der Antriebsmechanismus ein rotierendes Element (60) beinhaltet, um eine Rolle (58) in Drehung zu versetzen, und wobei der Dehnungsmesser weiterhin einen Riemen (50) beinhaltet, dessen erstes Ende am Nockenelement (46) befestigt ist, und dessen zweites Ende an der Rolle (58) befestigt ist, wobei sich, wenn das rotierende Element (60) in Drehung versetzt wird, die Rolle (58) dreht, wodurch eine Zugkraft auf den Riemen (50) ausgeübt und das Nockenelement (46) aus der ersten Position in die zweite Position gedrängt wird.
6. Dehnungsmesser nach Anspruch 1, wobei sich die ersten und zweiten Kontaktarme (16, 18) der ersten und zweiten Armanordnungen (12, 13) auf einer ersten Seite der Schienenstruktur (102) befinden, und wobei sich das rotierende Element (60) auf der anderen Seite der Schienenstruktur befindet.
7. Dehnungsmesser nach Anspruch 6, wobei das rotierende Element ein rotierender Stab (60) ist, und wobei der rotierende Stab an einem Element mit Kanten (78, 80) befestigt ist, die sich in Reaktion auf eine Drehung des rotierenden Stabes (60) bewegen und einen Schalter (81) betätigen, um den gewünschten Bewegungsbereich des rotierenden Stabes anzuzeigen.
8. Dehnungsmesser nach Anspruch 7, wobei das Element (60) radial angeordnete Kanten beinhaltet, und wobei der Schalter (81) ein optischer Schalter ist.
9. Dehnungsmesser nach Anspruch 8, wobei die Rolle (58) auf einem Rollenlager (85) montiert ist, wobei das Rollenlager eine Nockenoberfläche mit mindestens einer Tasche (72) beinhaltet, und wobei der Dehnungsmesser weiterhin einen federbelasteten Mechanismus beinhaltet, um in die mindestens eine Tasche (72) einzugreifen, so dass eine Winkelanordnung der Rolle (58) aufrechterhalten wird.
10. Dehnungsmesser nach Anspruch 5, wobei der Riemen (50) auf mindestens einem Rollenelement (52, 54, 56) montiert ist, so dass der Riemen von der ersten Seite zur zweiten Seite der vertikalen Schienenstruktur (102) verläuft.
1. Extensomètre, comprenant:
un premier ensemble de bras (12) et un second ensemble de bras (13), chaque ensemble de bras comprenant des premier et second bras de contact alternatifs (16, 18), les premier et second ensembles de bras (12, 13) comprenant chacun:
un élément de came (46), chaque élément de came comportant des première et seconde fentes de came inclinées (42, 44), qui sont inclinées l'une par rapport à l'autre;
un premier bras de levier (20) qui présente une première extrémité proximale (34) engagée à l'intérieur de la première fente de came inclinée (42) et une première extrémité distale (24) engagée avec le premier bras de contact (16), et un premier point de pivot (28) entre la première extrémité proximale (34) et la première extrémité distale (24);
un second bras de levier (22) qui présente une seconde extrémité proximale (36) engagée à l'intérieur de la seconde fente de came inclinée (44) et une seconde extrémité distale (26) engagée avec le second bras de contact (18), et un second point de pivot (30) entre la seconde extrémité proximale (36) et la seconde extrémité distale (26);
un élément de support (32) sur lequel les premier et second points de pivot (38, 30) sont montés de façon pivotante;
dans lequel, lorsque l'élément de came (46) se trouve dans une première position, les premier et second bras de contact (16, 18) sont poussés l'un vers l'autre, et dans lequel, lorsque l'élément de came (46) se trouve dans une seconde position, les premier et second bras de contact (16, 18) sont poussés à l'écart l'un de l'autre; et
un mécanisme d'entraînement configuré de manière à pousser l'élément de came (46) à partir de la première position jusqu'à la seconde position, le mécanisme d'entraînement étant séparé de l'élément de came;
ledit extensomètre comprenant en outre une structure de piste verticale (102) sur laquelle les premier et second ensembles de bras (12, 13) sont configurés pour se déplacer.
2. Extensomètre selon la revendication 1, dans lequel chaque élément de support (32) présente une première extrémité (33) sur laquelle une extrémité proximale (37) du premier bras de contact (16) est montée de façon élastiquement flexible, et une seconde extrémité (35) sur laquelle une extrémité proximale (39) du second bras de contact (18) est montée de façon élastiquement flexible.
3. Extensomètre selon la revendication 2, dans lequel l'élément de came est un coin (46) qui présente lesdites première et seconde fentes de came inclinées (42, 44), et dans lequel les première et seconde extrémités proximales (34, 36) des premier et second bras de levier respectifs (20, 22) comprennent des premier et second éléments de rouleau à bosses respectifs (38, 40) qui sont engagés de manière à se déplacer à l'intérieur des première et seconde fentes de came inclinées respectives (42, 44).
4. Extensomètre selon la revendication 3, dans lequel les premier et second ensembles de bras (12, 13) comprennent chacun un ressort (48) pour pousser l'élément de came (46) en direction de la première position.
5. Extensomètre selon la revendication 4, dans lequel le mécanisme d'entraînement comprend un élément rotatif (60) qui fait tourner une bobine (58), et dans lequel l'extensomètre comprend en outre une courroie (50) qui présente une première extrémité attachée à l'élément de came (46) et une seconde extrémité attachée à la bobine (58), moyennant quoi, lorsque l'élément rotatif (60) est mis en rotation, la bobine (58) tourne, tirant de ce fait la courroie (50) et poussant l'élément de came (46) à partir de la première position jusqu'à la seconde position.
6. Extensomètre selon la revendication 1, dans lequel les premier et second bras de contact (16, 18) des premier et second ensembles de bras (12, 13) sont situés sur un premier côté de la structure de piste (102) et l'élément rotatif (60) est situé sur l'autre côté de la structure de piste.
7. Extensomètre selon la revendication 6, dans lequel l'élément rotatif est une barre rotative (60), et dans lequel la barre rotative est attachée à un élément comprenant des bords (78, 80) qui se déplacent en réponse à la rotation de la barre rotative (60) et qui actionnent un commutateur (81) pour indiquer la plage de mouvement souhaitée de la barre rotative.
8. Extensomètre selon la revendication 7, dans lequel l'élément (60) comprend des bords orientés radialement, et dans lequel le commutateur (81) est un commutateur optique.
9. Extensomètre selon la revendication 8, dans lequel la bobine (58) est montée sur un support de bobine (85), le support de bobine présentant une surface de came comportant au moins une poche (72), et dans lequel l'extensomètre comprend en outre un mécanisme chargé par ressort pour engager ladite au moins une poche (72), maintenant de ce fait une orientation angulaire de la bobine (58).
10. Extensomètre selon la revendication 5, dans lequel la courroie (50) est montée sur au moins un rouleau (52, 54, 56) de telle sorte que la courroie passe du premier côté au second côté de la structure de piste verticale (102).

REFERENCES CITED IN THE DESCRIPTION
This list of references cited by the applicant is for the reader's convenience only. It does not form part of the European patent document. Even though great care has been taken in compiling the references, errors or omissions cannot be excluded and the EPO disclaims all liability in this regard.

Patent documents cited in the description
- CN
201740701
U
[0008]
- US
2085687
A
[0009]