ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESMMA....MD..........
J
JDIM360 Ver 1.28 (29 Oct 2014) - 1100000/0
3056251
EUROPEAN PATENT APPLICATION
A1
20160817
EP
16382055.8
20160210
es
en
en
201530147 U
20150211
ES
20160817
201633
20160817
201633
A63B 69/00 20060101AFI20160615BHEP
A63B 71/00 20060101ALI20160615BHEP
A63B 21/04 20060101ALI20160615BHEP
A63B 21/055 20060101ALI20160615BHEP
de
TRAININGSGERÄT FÜR LAUFTRAINING
en
APPARATUS FOR HELPING TO RUN
fr
APPAREIL D'ENTRAINEMENT POUR LA COURSE À PIED
1
Gomez Cores, Arturo
101518583
EP3278.4
C/ Cabo Santiago Gomez n°5 piso 2° Izquierda
15004 A Coruna
ES
Gomez Cores, Arturo
C/ Cabo Santiago Gomez n°5 piso 2° Izquierda
15004 A Coruna
ES
Pons
101597830
Glorieta Ruben Dario 4
28010 Madrid
ES
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
MA
MD
The device (1) comprises: a support structure (2); fixing means, designed to attach the support structure (2) to a wall; and a harness (4) that is attached, on one end, to said structure (2) and, on the other, to the user, wherein the harness (4) comprises, at least, an elastic section (8) that provides the user with a certain freedom of movement beyond the maximum length of the harness (4). The harness (4) also incorporates anchoring means (5, 6) to be attached to the support structure (2) and to the user. The device (1) makes it possible for users to engage in running at home, without the need to purchase complex machines or devices.

OBJECT OF THE INVENTION
The field of application of the present invention falls within the industry sector devoted to the manufacturing of tools, equipment and devices designed to improve people's quality of life.
More particularly, the object of the invention focuses on a device whose purpose is to provide a practical, comfortable way of helping to run at home without the need to move away.

BACKGROUND OF THE INVENTION
As is commonly known, due to inclement weather conditions, sometimes it is not possible to leave home for running outdoors. The use of devices designed for indoor running has been disclosed, but these devices are very complex, sophisticated and expensive. The device for helping to run of the present invention makes it possible indoors running, in a simple manner and without the need to purchase costly devices.

DESCRIPTION OF THE INVENTION
In order to solve said problems, the invention proposes a device designed to helping to run, such that said exercise may be performed in a simple and comfortable manner wherever the device is installed, for example at home, without the need to move away.
To this end, said device is essentially comprises a support structure, equipped with fixing means for allowing fixing thereof to a wall, preferably by means of screws, and a harness that is attached to said structure and to the user, for which purpose it is equipped with fast anchoring means.
Moreover, said harness has, preferably at the end that is attached to the user, usually by the waist, a section of elastic material which allows for a certain freedom of movement beyond the maximum length of the harness and which, therefore, determines the user's effort to overcome the tension thereof, when attempting to run with the harness attached to the waist.
In addition, it is worth noting that, in the preferred embodiment of the invention, the support structure is configured as a casing, which creates a precisely-sized housing wherein the harness described above may be kept when not in use and, moreover, allows for it to be subsequently used in a fast, practical manner, since said harness may be kept in the housing without the need to disassemble the anchoring that connects it to the support structure. To this end, the aforementioned casing is preferably open at the top, with an exit located just beneath the aforementioned anchoring.
Therefore, the device has the advantage of helping to run whenever the user so desires, without having to go out or move away from home, and without having to purchase complex machines or devices.

DESCRIPTION OF THE DRAWINGS
In order to complement the description being made and in order to contribute to a better understanding of the characteristics of the invention, the present specification is accompanied, as an integral part thereof, by a diagram wherein, for illustrative, non-limiting purposes, the following is represented:
- Figure 1.- Shows an upper perspective view of an embodiment of the device of the invention, which presents the main parts and elements that it comprises, as well as the configuration and arrangement thereof.

PREFERRED EMBODIMENT OF THE INVENTION
In view of the figure described above, Figure 1, and, on the basis of the numbering adopted therein, we observe a preferred, non-limiting embodiment of the proposed device for helping to run, which comprises the parts and elements specified and described in detail below.
According to said Figure 1, it is to observe that the device (1) in question is configured on the basis of a support structure (2) equipped with fixing means that allow for fixation thereof to a wall, for example, two or three openings (3) designed for the insertion of sleeper screws, and a harness (4) which, equipped with anchoring means (5, 6), is attached, on one end, to said structure (2) and, on the other, to the user, for example, to his/her waist.
Preferably, these anchoring means (5, 6) are quick-fixation means, and are composed of, for example, a first flange (5), designed for fixation to the support structure (2), and a hook (6), designed to be attached to the user, and which generally includes a ring (7).
Moreover, the harness (4), preferably located at the end that is attached to the user, is equipped with, at least, an elastic section (8) which grants it a certain freedom of movement beyond the maximum length of the harness and which, therefore, determines the effort to be made by the user in order to overcome the tension thereof. In the example represented, this elastic section (8) is attached to the harness (4) by means of a second flange (5'), which, in turn, is attached to the end of a rope making part of the elastic section (8) of the harness (4), although this does not meant to be a limitation.
As mentioned in the preceding sections, in the preferred embodiment of the invention, the support structure (2) is configured as a casing (9) that defines a housing (10) suitable to keep the harness therein (4).
Finally, in the preferred configuration of said casing (9), an exit of the housing (10) is located on the upper part thereof, just beneath the anchoring (5) that attaches the harness (4) to the structure (2), such that the harness (4) may be kept inside said housing (10) without the need to disassemble said anchoring (5).
1. Device for helping to run, characterised in that it comprises a support structure (2) equipped with fixing means that allow for fixation thereof to a wall, and a harness (4) which, equipped with anchoring means (5, 6), is attached, on one end, to said structure (2) and, on the other, to the user, wherein this harness (4) is equipped with, at least, an elastic section (8) for providing the user with a certain freedom of movement beyond a maximum length of the harness (4).
2. Device for helping to run, according to claim 1, wherein the fixing means that allow for fixation of the support structure (2) to a wall comprise two or three openings (3) designed for the insertion of sleeper screws.
3. Device for helping to run, according to claims 1 or 2, wherein the anchoring means (5, 6) of the harness (4) are quick-fixation means.
4. Device for helping to run, according to claim 3, wherein the anchoring means (5, 6) of the harness (4) comprise a flange (5) designed to be attached to the support structure (2), and a hook (6) designed to be attached to the user.
5. Device for helping to run, according to any of claims 1-4, wherein the elastic section (8) of the harness (4) is located at the end of the harness (4) that is attached to the user.
6. Device for helping to run, according to any of claims 1-5, wherein the support structure (2) is configured as a casing (9) that defines a housing (10) designed to keep the harness therein (4).
7. Device for helping to run, according to claim 6, wherein the casing (9) is configured such that an exit of the housing (10) is located on the upper part and just beneath the anchoring (5) that attaches the harness (4) to the structure (2), in order to keep the harness (4) in said housing (10) when not in use, without the need to disassemble said anchoring (5).
EP3278.4
EP
16382055.8
Gomez Cores, Arturo
1
MN
20160621
A63B
DE
436348
C
GUSTAV HAGER SPORTARTIKELFABRI
19261030
X
1,3,5
Y
2,4,6,7
* page 1; figures *
US
3193288
A
DE SPAIN LE VELL ET AL
19650706
X
1,3,5
Y
2,4,6,7
* columns 1-3; figures *
DE
102012110051
A1
SCHEFFER HARALD [DE]
20130627
Y
2,4
* paragraphs [0021], [0023] - [0024], [0026]; figures *
US
518967
A
G.F. POOLE
18940501
Y
2
* figure 1 *
US
2014200122
A1
HALLMARK TIMOTHY M [US]
20140717
Y
4
* paragraph [0040]; figures *
US
5335794
A
REEDY MICHAEL H [US]
19940809
Y
6,7
* claims; figures *
US
4946057
A
CONNOLLY BRIAN D [US] ET AL
19900807
Y
6,7
* claims; figures *
Herry, Manuel
Munich
20160607
DE
436348
C
19261030
NONE
US
3193288
A
19650706
NONE
DE
102012110051
A1
20130627
AU
2012357215
A1
20140710
CA
2859845
A1
20130627
CN
104245059
A
20141224
DE
102012110051
A1
20130627
EA
201400747
A1
20140930
EP
2794036
A1
20141029
KR
20140107570
A
20140904
US
2015051056
A1
20150219
WO
2013091625
A1
20130627
US
518967
A
18940501
NONE
US
2014200122
A1
20140717
CN
104918664
A
20150916
JP
5925395
B2
20160525
JP
2016502908
A
20160201
US
2014200122
A1
20140717
WO
2014112991
A1
20140724
US
5335794
A
19940809
NONE
US
4946057
A
19900807
NONE