ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESMMA....MD..........
J
JDIM360 Ver 1.28 (29 Oct 2014) - 1100000/0
3112030
EUROPEAN PATENT APPLICATION
A1
20170104
EP
16382292.7
20160623
es
en
en
201531292 U
20150630
ES
20170104
201701
20170104
201701
B03C 3/74 20060101AFI20161103BHEP
de
SELBSTREGENERIERENDER ELEKTROSTATISCHER ABSCHEIDER
en
SELF-REGENERATIVE ELECTROSTATIC PRECIPIATOR
fr
PRÉCIPITATEUR ÉLECTROSTATIQUE AUTO-RÉGÉNÉRATEUR
1
Universidad de Vigo
101606503
16EPS007
Campus Universitario, s/n As Lagoas - Marcosende
36310 Vigo Pontevedra
ES
MÍGUEZ TABARÉS, Jose Luis
UNIVERSIDAD DE VIGO Campus Universitario, s/n As Lagoas - Marcosende
36310 VIGO (PONTEVEDRA)
ES
PORTEIRO FRESCO, Jacobo
UNIVERSIDAD DE VIGO Campus Universitario, s/n As Lagoas - Marcosende
36310 VIGO (PONTEVEDRA)
ES
PATIÑO VILAS, David
UNIVERSIDAD DE VIGO Campus Universitario, s/n As Lagoas - Marcosende
36310 VIGO (PONTEVEDRA)
ES
GRANADA ÁLVAREZ, Enrique
UNIVERSIDAD DE VIGO Campus Universitario, s/n As Lagoas - Marcosende
36310 VIGO (PONTEVEDRA)
ES
Temiño Ceniceros, Ignacio
101219028
Calle Amador de los Rios 1-1°
28010 Madrid
ES
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
MA
MD
The invention relates to a self-regenerative electrostatic precipitator (10) of the type comprising a discharge electrode (1) located inside a gas conduit (3) for generating a corona discharge and for depositing solid particles in suspension in a gas stream (11) circulating through the conduit (3) in a deposition layer (4) on the inner wall of the conduit (3). The electrostatic precipitator (10) comprises at least one cleaning assembly (7) arranged outside the conduit (3), each cleaning assembly (7) having at least one induction coil (6) wound around the conduit (3) for heating the wall of the conduit (3) by electromagnetic induction. The electrostatic precipitator (10) reduces emissions of solid particles in suspension in a gas stream.

TECHNICAL FIELD
The present invention is comprised in the field of systems or apparatus for reducing contaminating emissions in combustion systems, and more specifically for reducing emissions of particles in suspension in a gas stream generated, for example, by a biomass boiler or a diesel engine. The invention is particularly comprised in the field of electrostatic precipitators.

PRIOR ART
Any combustion system is susceptible to generating contaminating emissions. These emissions are gas emissions, but they can also contain solid or liquid particles in suspension as a result of an imperfect combustion or ash present in the fuel exiting the system with the gas stream. Solid (biomass and carbon) combustion systems as well as reciprocating internal combustion (particularly diesel) engines are particularly unique as regards emissions of this type. The reason for their risks resides in the large number of particles given off and their reduced size (smaller than 1 µm) which do not readily settle in the atmosphere and are impossible for the human respiratory system to filter out.
For the reasons set forth, it is common to introduce filtering elements into these combustion systems to minimize particle emissions. Though less widespread in the field of biomass boilers, particle filters are usually installed in diesel engines to comply with environmental regulations.
There are several strategies for reducing particle emissions. Among others, settling chambers or cyclones that separate the particles by centrifugal force, filtering systems that retain aerosols by means of a porous (for example fiber) bed, or electrostatic precipitators that electrically charge the particles to then remove them from the gas stream as a result of the strong electric field generated between two electrodes, can be used.
Each of the mentioned systems has features making them more or less advantageous depending on the type of combustion system. In many cases, one of the biggest problems for the application thereof is the removal of particles deposited throughout the service life of the filter. As an example, a filtering system is used in diesel engines that accumulates unburned particles (of an organic origin) over time, and every so often they use a regeneration cycle. In other words, they send very hot gases to the filter, and as a result of the high temperature reached they burn the deposited particles again, recovering the filtration element's efficiency.
In other cases, such as in electrostatic precipitators, for example, it is common to introduce a mechanical element on the deposition collector which shakes, scrapes or hits the collector every so often, causing the particles to become detached, which are then collected in a waste disposal element in the lower area.
In scientific and patent literature, there are a number of proposals for regenerating or cleaning particle filtering systems which are primarily based on regeneration cycles with hot gases or on applying electric heating techniques.
The present invention proposes a particle filtering system using electrostatic precipitation which solves the aforementioned problems in the prior art.

DISCLOSURE OF THE INVENTION
The present invention relates to a particle filtering system using electrostatic precipitation which is self-cleaning by means of heating the walls by electromagnetic induction. This self-cleaning method allows the continuous operation of the device and the removal of most of the trapped mass, thereby reducing emissions of solid particles in suspension in a gas stream in a continuous manner.
The present invention proposes a system for filtering solid particles resulting from combustion by means of a self-regenerative electrostatic precipitator. A cylindrical precipitator with a high-voltage electrode in the center of the chimney or gas conduit generates a strong electric field which results in the creation of a corona discharge region. The particles in suspension in the gas stream, most of which are of a carbon origin (unburned), are ionized and deflected towards the deposition electrode by the same electric field that charged them or by another different one (a one- or two-stage precipitator). The deposition electrode of the present invention will be the outer cylindrical body of the conduit (or conduits) in which deposition takes place.
As material is being deposited on the chimney, and always before the electric field weakens and filtering efficiency becomes impaired, a series of induction coils outside the tube will be electrically activated. These coils wound around the conduit will receive high-frequency alternating current, generating electromagnetic induction in the wall of the conduit and thereby heating it with the currents induced in same. This will lead to a rise in the temperature of the wall until it is high enough to start burning the particles that are deposited on the inner face of the conduit. If the deposition surface is larger than the surface covered by the induction coils, two alternatives are provided: relative movement of the coils with respect to the conduit, or the existence of various coils which are sequentially activated to heat the entire surface.
A first aspect of the invention relates to a self-regenerative electrostatic precipitator, of the type comprising a discharge electrode located inside a gas conduit for generating a corona discharge and for depositing solid particles in suspension in a gas stream circulating through the conduit in a deposition layer on the inner wall of the conduit. The self-regenerative electrostatic precipitator comprises at least one cleaning assembly arranged outside the conduit, each cleaning assembly having at least one induction coil wound around the conduit for heating the wall of the conduit by electromagnetic induction.
The at least one induction coil of each cleaning assembly is preferably surrounded by at least one layer of insulating material. The electrostatic precipitator preferably comprises at least one securing element for fixing the discharge electrode inside the conduit.
In a preferred embodiment, the electrostatic precipitator comprises several cleaning assemblies the induction coils of which are activated together or sequentially. In another embodiment, the electrostatic precipitator comprises means for moving the cleaning assembly (or assemblies) along a section of the conduit.
The electrostatic precipitator can further comprise high-frequency alternating current generating means in the at least one induction coil.

BRIEF DESCRIPTION OF THE DRAWINGS
A series of drawings which helps to better understand the invention and is expressly related to an embodiment of said invention presented as a non-limiting example thereof is very briefly described below.
- Figure 1 is a cross-section view of the present invention.
- Figure 2 shows a detailed cross-section view of the cleaning and regeneration assembly.
- Figure 3 shows a cross-section view of a constructive variant of the present invention.

DETAILED DISCLOSURE OF THE INVENTION
The particle retaining equipment used in the present invention is a cylindrical electrostatic precipitator. Figure 1 depicts a cross-section view of the electrostatic precipitator 10 formed by a discharge electrode 1, securing elements 2 for securing the discharge electrode and a gas conduit 3 through the inside of which the combustion gases circulate and in which the collected particles accumulate in a deposition layer 4 having an increasing thickness. The regeneration system is formed by assemblies of induction coils 6, lead cable, and layers of insulating material 5.
The discharge electrode 1 generates the corona discharge for charging the solid particles in the combustion gases with particles 11 (the fume stream). In the same region, or in another one located thereafter, the electric field generated between the discharge electrode 1 and the wall of the conduit 3 (the deposition electrode) deflects the particles in suspension and causes them to be trapped, clean, particle-free gases 12 exiting the filtering system. The central discharge electrode 1 can be secured in various manners (separating arms, floating electrode, etc.), without this affecting the nature of the present invention. In the example shown in Figure 1, it is done by means of securing arms 2 built using an electrically insulating material.
When the electrostatic precipitator 10 is working, the particles will be retained, creating a deposition layer 4 having an increasing thickness adhered to the outer electrode. As this deposition layer 4 grows, the operation of the system worsens and the retaining efficiency gradually decreases due to the weakening of the electric field and to the increasing more likely reinsertion of particles deposited by erosion with the gas itself. It is therefore necessary to periodically eliminate or reduce the layer of dirt. To that end, the present invention incorporates a regeneration or self-cleaning system. It is formed by a series of induction coils 6 wound around the conduit 3. To protect them against the high temperature and to prevent unwanted electrical contacts they are internally and externally insulated with layers of insulating material 5. When the cleaning sequence is run, the induction coils 6 are subjected to a high-frequency alternating current, causing the induction electric currents in the body of the deposition electrode 3. As a result of this induction, the temperature of the conduit will increase up to values exceeding the ignition temperature of the particles deposited in the deposition layer 4. These particles, in the presence of oxygen that may be contained in combustion gases with particles 11 flowing through the inside of the conduit 3 and the high temperature in the wall, will burn and the mass and thickness of the deposition layer 4 will thereby be reduced.
The cleaning process is therefore based on burning the deposited particles again using the high temperature generated by means of electromagnetic induction on the deposition electrode.
The cleaning and regeneration system can be formed by several cleaning assemblies 7, as shown in Figure 1, where four independent cleaning assemblies 7 can be seen, each being formed by a wound induction coil 6 and two layers of insulating material 5. Figure 2 shows a view of detail A of Figure 1, in which a cleaning and regeneration assembly can be seen. The regeneration system is therefore formed by different assemblies of induction coils 6 and layers of insulating material 5. As many cleaning assemblies as required for burning the particles deposited on the entire wall of the conduit 3 can be used. Furthermore, the different cleaning assemblies do not have to be activated at the same time, but rather they can be activated in an alternating manner, depending on cleaning needs.
If required, there could be just one cleaning assembly 7 and it could move along the conduit 3 as shown in Figure 3. The operation of the invention is the same as that described above but now the regeneration or cleaning system moves vertically by means of a mechanical, electrical or magnetic mechanism to the area of the conduit that must be cleaned. Once the position is reached, it is electrically actuated, volatilizing the particles located in that area.
1. A self-regenerative electrostatic precipitator, comprising a discharge electrode (1) located inside a gas conduit (3) for generating a corona discharge and for depositing solid particles in suspension in a gas stream (11) circulating through the conduit (3) in a deposition layer (4) on the inner wall of the conduit (3), characterized in that the electrostatic precipitator (10) comprises at least one cleaning assembly (7) arranged outside the conduit (3), each cleaning assembly (7) having at least one induction coil (6) wound around the conduit (3) for heating the wall of the conduit (3) by electromagnetic induction.
2. The self-regenerative electrostatic precipitator according to claim 1, characterized in that the at least one induction coil (6) of each cleaning assembly (7) is surrounded by at least one layer of insulating material (5).
3. The self-regenerative electrostatic precipitator according to any of the preceding claims, characterized in that it comprises at least one securing element (2) for fixing the discharge electrode (1) inside the conduit (3).
4. The self-regenerative electrostatic precipitator according to any of the preceding claims, characterized in that it comprises a plurality of cleaning assemblies (7) the induction coils (6) of which are activated together or sequentially.
5. The self-regenerative electrostatic precipitator according to any of the preceding claims, characterized in that it comprises means for moving the at least one cleaning assembly (7) along a section of the conduit (3).
6. The self-regenerative electrostatic precipitator according to any of the preceding claims, comprising high-frequency alternating current generating means in the at least one induction coil (6).
16EPS007
EP
16382292.7
Universidad de Vigo
1
DH
20161110
B03C
F23J
JP
2002047914
A
YAMAGUCHI TAKASHI
20020215
X
1-6
* abstract *
* paragraphs [0005], [0006] *
* the whole document *
US
2005262817
A1
HATANAKA YOSHIHIRO [JP]
20051201
A
1,6
* the whole document *
US
2009074630
A1
GONZE EUGENE V [US] ET AL
20090319
A
1,4
* the whole document *
DE
10345925
A1
OPEL ADAM AG [DE]
20050504
A
1
* the whole document *
JP
2004132338
A
TAMA TLO KK
20040430
A
1-6
* abstract *
* the whole document *
US
6092387
A
HIRONAKA YASUMASA [JP] ET AL
20000725
A
1-6
* column 4, line 5 - line 29 *
WO
2005097332
A1
EMPA [CH]; SCHMATLOCH VOLKER [CH]
20051020
A
1
* abstract *
* paragraphs [0001], [0012], [0013] *
EP
2583755
A1
KARLSRUHER INST TECHNOLOGIE [DE]
20130424
A
1
* paragraphs [0001], [0048], [0051] *
DE
202007004263
U1
OTTO SPANNER GMBH [DE]
20070705
A
1
* abstract *
* paragraphs [0002], [0009], [0010], [0015] *
Holubov, Carol
The Hague
20161101
JP
2002047914
A
20020215
JP
3443733
B2
20030908
JP
2002047914
A
20020215
US
2005262817
A1
20051201
AU
2003292635
A1
20040722
CN
1732329
A
20060208
EP
1580410
A1
20050928
JP
3899404
B2
20070328
JP
2004204824
A
20040722
KR
20050091748
A
20050915
US
2005262817
A1
20051201
WO
2004059135
A1
20040715
US
2009074630
A1
20090319
CN
101403330
A
20090408
DE
102008047392
A1
20090514
US
2009074630
A1
20090319
DE
10345925
A1
20050504
NONE
JP
2004132338
A
20040430
NONE
US
6092387
A
20000725
CN
1227905
A
19990908
JP
H11237071
A
19990831
US
6092387
A
20000725
WO
2005097332
A1
20051020
AT
431190
T
20090515
EP
1732695
A1
20061220
WO
2005097332
A1
20051020
EP
2583755
A1
20130424
NONE
DE
202007004263
U1
20070705
DE
202007004263
U1
20070705
EP
1958696
A2
20080820