ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESMMA....MD..........
J
BDM Ver 0.1.63 (23 May 2017) - 1100000/0
3446583
EUROPEAN PATENT APPLICATION
A1
20190227
EP
17187427.4
20170823
en
en
en
20190227
201909
20190227
201909
A41D 19/00 20060101AFI20180125BHEP
de
HANDSCHUH MIT RINGFÖRMIGER MARKIERUNG
en
GLOVE WITH RING MARK
fr
GANT AVEC MARQUAGE EN FORME D'ANNEAU
1
PM Gloves
101687956
P67976
2F., No.68, Sec. 1, Neihu Rd. Neihu Dist.
Taipei City 114
TW
LIN HUANG, Hsun-Hui
2F., No.68, Sec. 1, Neihu Rd., Neihu Dist.
114 Taipei City
TW
Viering, Jentschura & Partner mbB Patent- und Rechtsanwälte
101239391
Kennedydamm 55 / Roßstrasse
40476 Düsseldorf
DE
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
MA
MD
A glove' s color beading ring comprises a glove body (1), the glove is provided with one or more colored ring marks (2) at the cuff lip, and the colored ring mark (2) employing different colors, linetypes, patterns, thickness lines as an identification manner to determine the use area of the glove and allowing the staff members to readily interpret the difference of the glove so as to wear a suitable pair of gloves in working.

BACKGROUND OF THE INVENTION

1. Field of the invention
The present invention relates to the field of glove, in particular, to an identification structure of distinguishing the use area of glove by arranging a ring mark at the glove cuffs.

2. Description of the prior art
Glove is a common and necessary tool for those who needs a clean work, especially for medical staff who need to wear glove at any time since they have to often touch with objects having pollutants, pathogens, so the medical staff must be ensured to be isolated from the objects being touched for protecting health and safety of the medical staff.
Objects touched by each working staff is different according to their different working areas, therefore the glove is also needed to be classified so as to provide appropriate needs for different working staff while avoiding concerns about the pollution resulted from mixed use by the working staff in different areas.
However, as medical glove is disposable equipment, quite simple design of it leads to an uneasily identification from the appearance, thus it is hard to recognize for working staff even they have wore the gloves of different areas, thereby causing security risks.
To this end, an identification mark should be designed on the medical glove, and this design should be simple, readily identifiable and not be an interruption for wearing and working according to the properties of the medical glove, being beneficial for the working staff to use.
In view of this, since there is a significant problem needed to be improved in the traditional design of medical glove still, it is not a good design.
As such, in the light of above problem of traditional medical glove, the inventor of this application has finally developed the structure of glove's color beading ring after long-term researches and practices by active improvement and experience and expertise from long-term work in the art.

SUMMARY OF THE INVENTION
The main purpose of the present invention is to provide a glove' s color beading ring, which promotes the identification of glove, enables a direct visual determination on selecting a suitable pair of gloves and hence a safe, rapid access into working for the user.
Another purpose of the present invention is to provide a glove' s color beading ring with simple design, low cost, strong effect, and enhancement for the safe use of glove.
A glove' s color beading ring which can achieve one of above purposes mainly comprises a glove, and the use area, stage or procedure of the glove is distinguished by arranging the glove with a ring mark at the cuff or lip.
And the ring mark can be arranged to be one or more, by the design of different numbers, stuff member of different working area, stage or procedure is distinguished to use, and the stuff can find a suitable pair of gloves for quick access by a direct visualization of the color ring mark.
Or, the ring mark may also be provided with different color designs as identification method.
Or, the ring mark may also be provided with different linetype designs as identification method.
Or, the ring mark may also be provided with different pattern designs as identification method.
Or, the ring mark may also be provided with different thickness line designs as identification method.
Furthermore, the ring mark can be combined with aforementioned various identification methods to strengthen the distinction effect.

BRIEF DESCRIPTION OF THE DRAWINGS
- Fig. 1 is a structural perspective of the glove' s color beading ring of the present invention;
- Fig. 2 is a view for the number variation of the ring mark of the glove' s color beading ring;
- Fig. 3 is a view for the linetype variation of the ring mark of the glove' s color beading ring;
- Fig. 4 is a view for the pattern variation of the ring mark of the glove' s color beading ring; and
- Fig. 5 is a view for the thickness line variations of the ring mark of the glove' s color beading ring.

[Symbol Description of Main Element]
1 | glove | 2 | ring mark

DETAILED DESCRIPTION OF THE PREFERRED EMBODIMENT
With reference to Fig. 1, the present invention provides a glove' s color beading ring mainly comprising a body of glove 1, the glove 1 is arranged with a ring mark 2 at the cuff, and the ring mark 2 is used to distinguish different working areas, stages or procedures of the glove 1.
For example, different ring marks 2 can be selected firstly according to each working area to inform the user in this area, then the user can readily find a suitable pair of the gloves 1 to wear only by visually observing the ring mark 2 on the glove 1 without the occurrence of interactive contamination or infection due to mixed use.
With reference to Fig. 1 and 2, the ring mark 2 is provided with at least one, different ring marks 2 are arranged according to the number of working areas, stages or procedures and then distinguished to the stuff member in different working areas, stages or procedures for use by utilizing different number designs.
In another way, with reference to Fig. 3, the ring mark 2 may be also provided with a linetype, for example, solid line, broken line, as an identification, polyline etc., and different linetypes can be used to distinguish the working area, stage or procedure.
Or, with reference to Fig. 4, the ring mark 2 can also be provided with a pattern as an identification.
Or, with reference to Fig. 5, the ring mark 2 can also be provided with a thickness line as an identification.
Certainly, with combination of above-mentioned identification methods, a more precise distinguish effect can be obtained through configuring alternately the ring marks 2 with different number, colors, linetypes, patterns, thickness lines by the ring mark 2.
Many changes and modifications in the above described embodiment of the invention can, of course, be carried out without departing from the scope thereof. Accordingly, to promote the progress in science and the useful arts, the invention is disclosed and is intended to be limited only by the scope of the appended claims.
1. A glove' s color beading ring comprising a glove, characterized in that arranging the glove with a ring mark at the cuff or lip to distinguish the use area, stage or procedure of the glove.
2. The glove' s color beading ring according to Claim 1, wherein the ring mark is provided with one or more for identification.
3. The glove' s color beading ring according to Claim 2, wherein the ring mark is provided with a color for identification.
4. The glove' s color beading ring according to Claim 2, wherein the ring mark is provided with a linetype for identification.
5. The glove' s color beading ring according to Claim 2, wherein the ring mark is provided with a pattern for identification.
6. The glove' s color beading ring according to Claim 2, wherein the ring mark is provided with a thickness line for identification.
P67976
EP
17187427.4
PM Gloves
1
DH
20180201
A41D
A61B
GB
2493288
A
ALI FAISAL [GB]
20130130
X
1-4,6
* page 3, line 19 - line 20 *
* page 6, line 10 - line 18; figures 1,3-14 *
WO
2014056640
A1
GLOVAC APS [DK]
20140417
X
1-4,6
* page 7, line 17 - line 19 *
* page 8, line 3 - line 17 *
* page 9, line 23 - line 25 *
* page 13, line 21 - line 30; figures 10,11A,11B *
US
2011067166
A1
JALBERT COURTNEY [US]
20110324
X
1-6
* paragraph [0014] - paragraph [0018] *
* paragraph [0028] - paragraph [0039] *
* paragraph [0049] - paragraph [0053]; figures 1-4 *
GB
758742
A
LONDON RUBBER COMPANY LTD
19561010
X
1-3
* the whole document *
US
3852826
A
SCHINDLER O
19741210
X
1-3,6
* abstract; figures 2,3 *
* column 2, line 7 - line 20 *
* column 4, line 44 - line 55 *
US
2012030853
A1
MOUNTFORT ANNA-MARIA [CA]
20120209
X
1-3
* paragraph [0030]; figures 1-4 *
FR
1047096
A
RUBBERFABRIEKEN IR L M GLAZENE
19531210
A
1-6
* the whole document *
Thielgen, Robert
The Hague
20180123
GB
2493288
A
20130130
NONE
WO
2014056640
A1
20140417
CA
2886039
A1
20140417
CA
2986637
A1
20140417
DK
2903484
T3
20161219
EP
2903484
A1
20150812
EP
3132722
A1
20170222
US
2015265085
A1
20150924
US
2018199744
A1
20180719
WO
2014056640
A1
20140417
US
2011067166
A1
20110324
NONE
GB
758742
A
19561010
NONE
US
3852826
A
19741210
AT
355795
B
19800325
BE
824487
A
19750515
BR
7500306
A
19751104
DE
2501606
A1
19750724
ES
433848
A1
19770216
FR
2258162
A1
19750818
GB
1499380
A
19780201
IL
45580
A
19790725
JP
S50113086
A
19750904
NL
7500607
A
19750722
SE
7406082
A
19750721
US
3852826
A
19741210
US
2012030853
A1
20120209
CA
2715696
A1
20120205
US
2012030853
A1
20120209
FR
1047096
A
19531210
NONE