ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESMMAKHTNMD..........
J
BDM Ver 0.1.67 (18 Oct 2017) - 1100000/0
3502305
EUROPEAN PATENT APPLICATION
A1
20190626
EP
18214948.4
20181220
en
en
en
201715852558
20171222
US
20190626
201926
20190626
201926
C23C 14/04 20060101AFI20190507BHEP
B05C 13/02 20060101ALI20190507BHEP
C23C 14/50 20060101ALI20190507BHEP
H01J 37/20 20060101ALI20190507BHEP
H01J 37/32 20060101ALI20190507BHEP
de
SICHTLINIENBESCHICHTUNGSARMATUR UND -VORRICHTUNG
en
LINE-OF-SIGHT COATING FIXTURE AND APPARATUS
fr
ÉLÉMENT DE FIXATION ET APPAREIL DE REVÊTEMENT À VISIBILITÉ DIRECTE
1
United Technologies Corporation
101597495
72.80.140499
10 Farm Springs Road
Farmington, CT 06032
US
JORZIK, Eric
679 Fieldstone Drive
Annville, PA Pennsylvania 17003
US
Dehns
101728904
St. Brides House 10 Salisbury Square
London EC4Y 8JD
GB
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
KH
MA
MD
TN
An embodiment of a line-of-sight coating fixture (10) includes a support structure (12), a spindle (16), and a shadow structure (18). The support structure (12) includes a plurality of compartments (20A-C) disposed below a platter (14), each compartment (20A-C) having an opening (30A-C) on a periphery of the support structure (12). Each compartment (20A-C) is adapted to receive and secure a base of a workpiece (50A-C) such that a body of each workpiece (50A-C) to be coated is disposed about a periphery of the support structure (12) and extends above the platter (14). The spindle (16) is disposed through a center of the platter (14) or support structure (12) for rotating the workpieces (50A-C) thereabout. The shadow structure (18) is disposed about the spindle (16), inside of the periphery, the shadow structure (18) sized and adapted to shield a portion of each workpiece (50A-C) from line-of-sight coating material.

BACKGROUND
The disclosure is related generally to fixtures for line-of-sight coating apparatus, and more specifically to fixtures for optimizing throughput of line-of-sight coating apparatus.
Many vapor coating, and other line-of-sight coating fixtures, in particular for airfoils, are limited to hold a single part per fixture. Attempts to increase the number of workpieces on a single fixture often lead to uneven coating application, either due to inadvertent blocking of the coating stream by portions of the fixture, or by uneven heating throughout the chamber, leading to differences in adhesion and microstructure of the coating.
As such, conventional approaches utilize multiple fixtures, each with a single workpiece, fixed to a rake or other device disposed at the base of the chamber in order to somewhat increase efficiency and throughput for a batch coating process. However, each coating machine is limited in how many fixtures it can hold, and the cost of additional machines can be cost-prohibitive when trying to ramp up production from a product introduction to sustained long-term operation.

SUMMARY
An embodiment of a line-of-sight coating fixture includes a support structure, a spindle, and a shadow structure. The support structure includes a plurality of compartments disposed below a platter, each compartment having an opening on a periphery of the support structure. Each compartment is adapted to receive and secure a base of a workpiece such that a body of each workpiece to be coated is disposed about a periphery of the support structure and extends above the platter. The spindle is disposed through a center of the platter or support structure for rotating the workpieces thereabout. The shadow structure is disposed about the spindle, inside of the periphery, the shadow structure sized and adapted to shield a portion of each workpiece from line-of-sight coating material.
A method of line-of-sight coating includes securing a base of a workpiece to a support structure including a plurality of compartments disposed below a platter. Each compartment has an opening on a periphery of the support structure for receiving each workpiece base, such that a body of each workpiece to be coated is disposed about a periphery of the support structure and extends above the platter. The workpieces are rotated about a spindle disposed through a center of the platter or support structure. A portion of each workpiece is shielded from a stream of line-of-sight coating material via a shadow structure disposed about the spindle, inside of the periphery.

BRIEF DESCRIPTION OF THE DRAWINGS
- FIG. 1 is a top view of a non-limiting example embodiment of a line-of-sight coating fixture according to the disclosure.
- FIG. 2 is a side view of the example coating fixture of FIG. 1 and the example workpiece of FIG. 3.
- FIG. 3 is a non-limiting example workpiece for which the example coating fixture of FIGS. 1 and 2 is adapted.
- FIG. 4 is an example line-of-sight coating apparatus with multiple instances of the example embodiment disposed therein.
- FIG. 5 is an example insert for a dovetail root.
- FIG. 6 is an example insert for a single-lobe root.

DETAILED DESCRIPTION
FIG. 1 is a top view, and FIG. 2 is a side view of a non-limiting example embodiment of a line-of-sight coating fixture 10. Referring first to FIG. 1, fixture 10 includes support structure 12, platter 14, spindle 16, shadow structure 18, compartments 20A, 20B, 20C, and workpieces 50A, 50B, 50C (example workpiece shown in FIG. 3). Support structure 12, in this example, includes three coating positions 22A, 22B, 22C to retain workpieces 50A, 50B, 50C about a periphery. Spindle 16 retains support structure 12 and includes hole 24 disposed through a center of support structure 12 for rotating workpieces 50A, 50B, 50C thereabout.
Also visible in FIG. 1 is shadow structure 18 disposed about spindle 16, inward of the periphery. In this example having three coating positions 22A, 22B, 22C, shadow structure 18 includes three respective shadow bars 26A, 26B, and 26C, each adapted to shield a portion of workpieces 50A, 50B, 50C from a line-of-sight coating or other stream (shown in FIG. 4). Each compartment 20A, 20B, 20C has a respective opening 30A, 30B, 30C on the periphery of support structure 12 below platter 14.
Moving to FIG. 2 (but still partially visible in FIG. 1), compartments 20A, 20B, 20C are each adapted to receive and secure a base of respective workpieces 50A, 50B, 50C such that a body of each workpiece to be coated extends above platter 14 and is disposed about periphery of support structure 12. One or more of compartments 20A, 20B, 20C, can optionally be an enclosure having one or more hinged doors 32A, 32B, 32C to fully shield the base of each workpiece.
As already seen from FIGS. 1 and 2, one or more of workpieces 50A, 50B, 50C can include a plurality of rotor blades, an example of which is seen in FIG. 3. Referring momentarily to FIG. 3, example rotor blade 50 includes, inter alia, airfoil 52, root 54, and platform 56. Other elements of blade 50 will be described with respect to FIGS. 3 and 4 as they relate to the coating apparatus and method.
Returning to FIGS. 1 and 2, for purposes of coating a rotor blade, each compartment 20A, 20B, 20C is adapted to receive and secure root 54 such that airfoil portion 52, to be coated, is disposed about the periphery of support structure 12 and extends above platter 14. In certain embodiments, upper surface of platter 14 can be shaped to conform to platform(s) 56 of each of the rotor blades 50, such that upper surface 60 of platform 56 is exposed in the same manner of airfoil 52, while a lower surface 62 of platform 56 is shielded in the manner of root 52.
For flexibility in coating different types of workpieces on the same equipment, the inside surfaces of one or more of compartments 20A, 20B, 20C can be shaped and adapted to conform to the base or root of each workpiece. In the example blade shown in FIG. 3, root 54 is of a dovetail type with multiple lobes 66 of decreasing dimension. As such, inside surfaces of e.g., compartment 20A can be provided with corresponding lobes (examples shown in FIGS. 5 and 6) to closely receive and securely retain the blade. Alternately, a workpiece may have a single lobe, and as such these surfaces can conform accordingly. This optional adjustment to compartments 20A, 20B, 20C can be done on either a temporary or permanent basis. For purposes of illustration, this disclosure illustrates (in FIGS. 5 and 6) two example pairs of removable inserts adapted to conform to the compartment and to two common types of roots for such workpieces. It will be appreciated that shrouds or other mounting structures can be made.
This arrangement also allows a span of each of the plurality of airfoils 52 to be aligned with a rotational axis A of the fixture / spindle. Further, in this example, the plurality of shadow bars 26A, 26B, 26C include walls defining a recess for receiving parts of the airfoil that are not to be coated. Here, as shown in FIGS. 1 and 2, these recesses separately cover each trailing edge 68 of the plurality of airfoils 52. The recesses defined by the plurality of shadow bars also cover a portion of the pressure surface 76 adjacent to the trailing edge 68. This may be, for example, to cover windows, outlets, and or cooling slots 80 in trailing edge 68 and prevent coating material from infiltrating the interior of airfoil 52.
FIG. 4 shows a line-of-sight coating apparatus 100 in which multiple fixtures can be used. Generally, apparatus 100 includes coating chamber 102 defined by chamber walls 104, vacuum / environmental port(s) 106, and at least one line-of-sight coating source 108 disposed along at least one wall 104. Source 108, which can include an EB-PVD coating source, is directed toward a plurality of fixtures 110A, 110B, 110C, at least one of which includes an embodiment of the above described fixture 10.
As shown in FIG. 4, fixtures 110A, 110B, 110C are arranged linearly and/or longitudinally opposed to coating source 108, selectively exposing surfaces of workpieces 150 to be coated. As described with respect to FIGS. 1 and 2, compartments 120 are operative to shield at least the base of each workpiece 150 from the line-of-sight coating material. As above, workpieces 150 can include a plurality of rotor blades, so that compartments 120 each include a wall or walls adapted to receive and secure a root portion of a rotor blade such that a platform portion and an airfoil portion extend above the platform in a first orientation. An upper surface of the blade platform is exposed to the line-of-sight coating source and a lower surface of the platform is shielded from the line-of-sight coating source, and the plurality of shadow bars 126 cover each trailing edge and a portion (e.g., windows, outlets, and/or slots) of the pressure surface adjacent to the trailing edge of the plurality of airfoils.
The arrangement shown in FIG. 4 is but one example of increasing coating throughput using the disclosed subject matter. Since the multi-piece fixtures shown herein are larger than a single-piece fixture known in the art, fewer multi-piece fixtures can fit into a coating chamber of a given size. However, the example shown still results in increased throughput, as three of the example three-piece fixtures can fit into a chamber previously known to hold five single-piece fixtures. This is a throughput increase of about 80%.
This not only increases the total number of parts which are coated per charge in the machine, but also created a more stable temperature gradient due to the added, consistent thermal mass. This even temperature leads to a more consistent coating from part to part, even when located on different fixtures.
FIG. 5 shows a removable insert 200 for one or more compartments 20, and includes a first insert piece 202 and a second insert piece 204 adapted to conform to first and second sides of a dovetail (multi-lobe) root. Here, outer side walls 206, 208 of respective insert pieces 202, 204 are generally straight, while inner side walls 210, 212 define multiple lobes 214 corresponding to the negative surfaces of root 54 in blade 50. These inserts 202, 204 are inserted into compartment 20 as shown (in FIGS. 1 and 2) so that the blade is held upright for airfoil coating.
FIG. 6 shows a removable insert 250 for one or more compartments 20, and includes a first insert piece 252 and a second insert piece 254 adapted to conform to first and second sides of a single-lobe root. As in FIG. 5, outer side walls 256, 258 are generally straight to conform to compartment 20, and inner side walls have a single lobe 260 corresponding to the neck of blade 50 (between airfoil 52 and root lobe 56). As with FIG. 5, these are inserted into compartment 20 as shown so that the blade is held upright for airfoil coating. In either case, however, these example inserts can be adapted for blades having roots arranged transverse to the blade chord, rather than collinear.
Summarizing a method of line-of-sight coating using the apparatus disclosed herein, a base of a workpiece is secured to a support structure including a plurality of compartments disposed below a platter. Each compartment has an opening on a periphery of the support structure for receiving each workpiece base, such that a body of each workpiece to be coated is disposed about a periphery of the support structure and extends above the platter. The workpieces are rotated about a spindle disposed through a center of the platter / support structure. A portion of each workpiece is shielded from one or more streams of line-of-sight coating material via a shadow structure disposed about the spindle.
As previously described, the plurality of workpieces can include one or more rotor blades, and as such, each compartment can be adapted to receive and secure a root of each rotor blade workpiece such that an airfoil portion of each rotor blade workpiece to be coated is disposed about a periphery of the support structure and extends above the platter. The platter can be shaped to conform to a platform of each of the plurality of rotor blades, such that an upper surface of the platform is exposed and a lower surface of the platform is shielded.

Discussion of Possible Embodiments
The following are non-exclusive descriptions of possible embodiments of the present disclosure.
An embodiment of a line-of-sight coating fixture includes a support structure, a spindle, and a shadow structure. The support structure includes a plurality of compartments disposed below a platter, each compartment having an opening on a periphery of the support structure. Each compartment is adapted to receive and secure a base of a workpiece such that a body of each workpiece to be coated is disposed about a periphery of the support structure and extends above the platter. The spindle is disposed through a center of the platter or support structure for rotating the workpieces thereabout. The shadow structure is disposed about the spindle, inside of the periphery, the shadow structure sized and adapted to shield a portion of each workpiece from line-of-sight coating material.
The fixture of the preceding paragraph can optionally include, additionally and/or alternatively, any one or more of the following features, configurations and/or additional components:
A line-of-sight coating fixture, according to an exemplary embodiment of this disclosure, among other possible things includes a support structure including a plurality of compartments disposed below a platter, each compartment having an opening on a periphery of the support structure, and each compartment adapted to receive and secure a base of a workpiece such that a body of each workpiece to be coated is disposed about a periphery of the support structure and extends above the platter; a spindle disposed through a center of the platter or support structure for rotating the workpieces thereabout; and a shadow structure disposed about the spindle, inside of the periphery, the shadow structure sized and adapted to shield a portion of each workpiece from line-of-sight coating material.
A further embodiment of the foregoing fixture, wherein the compartment is defined by an enclosure including at least one hinged door.
A further embodiment of any of the foregoing fixtures, wherein the plurality of workpieces include a plurality of rotor blades.
A further embodiment of any of the foregoing fixtures, wherein each compartment is adapted to receive and secure a root of a workpiece such that an airfoil portion of each workpiece to be coated is disposed about a periphery of the support structure and extends above the platter.
A further embodiment of any of the foregoing fixtures, wherein the platter is shaped to conform to a platform of each of the plurality of rotor blades, such that an upper surface of the platform is exposed and a lower surface of the platform is shielded.
A further embodiment of any of the foregoing fixtures, further comprising at least one removable insert adapted to conform to the root of each workpiece.
A further embodiment of any of the foregoing fixtures, wherein the at least one removable insert includes a first insert and a second insert adapted to conform to first and second sides of a dovetail root.
A further embodiment of any of the foregoing fixtures, wherein a span of the plurality of airfoils are aligned with a rotational axis of the fixture / spindle.
A further embodiment of any of the foregoing fixtures, wherein the shadow structure includes a plurality of shadow bars including a plurality of shadow walls defining a recess for separately covering each trailing edge of the plurality of airfoils.
A further embodiment of any of the foregoing fixtures, wherein the recesses defined by the plurality of shadow bars also cover a window or outlet portion of the pressure surface adjacent to the trailing edge.
A line-of-sight coating apparatus including a coating chamber defined by at least one wall and a line-of-sight coating source disposed along the at least one wall and directed toward a plurality of fixtures according to an embodiment of any of the foregoing fixtures.
A further embodiment of the foregoing apparatus, wherein the plurality of fixtures are arranged linearly or longitudinally opposed to the coating source.
A further embodiment of any of the foregoing apparatus, wherein the compartments are operative to shield at least the base of each workpiece from the line-of-sight coating material.
A further embodiment of any of the foregoing apparatus, wherein the coating source includes an EB-PVD coating source.
A further embodiment of any of the foregoing apparatus, wherein the plurality of workpieces include a plurality of rotor blades, and wherein the plurality of compartments each include at least one removable insert adapted to receive and secure a root portion of a rotor blade such that a platform portion and an airfoil portion extend above the platform in a first orientation.
A further embodiment of any of the foregoing apparatus, wherein the platter is shaped to conform to a platform contour of each of the plurality of rotor blades, such that an upper surface of the platform is exposed to the line-of-sight coating source and a lower surface of the platform is shielded from the line-of-sight coating source.
A further embodiment of any of the foregoing apparatus, wherein the shadow structure includes a plurality of shadow bars including at least one wall defining a recess for separately covering each trailing edge and a window or outlet portion of the pressure surface adjacent to the trailing edge of the plurality of airfoils.
A method of line-of-sight coating includes securing a base of a workpiece to a support structure including a plurality of compartments disposed below a platter. Each compartment has an opening on a periphery of the support structure for receiving each workpiece base, such that a body of each workpiece to be coated is disposed about a periphery of the support structure and extends above the platter. The workpieces are rotated about a spindle disposed through a center of the platter or support structure. A portion of each workpiece is shielded from a stream of line-of-sight coating material via a shadow structure disposed about the spindle, inside of the periphery.
The method of the preceding paragraph can optionally include, additionally and/or alternatively, any one or more of the following features, configurations and/or additional components:
A method according to an exemplary embodiment of this disclosure, among other possible things includes securing a base of a workpiece to a support structure including a plurality of compartments disposed below a platter, each compartment having an opening on a periphery of the support structure for receiving each workpiece base, such that a body of each workpiece to be coated is disposed about a periphery of the support structure and extends above the platter; rotating the workpieces about a spindle disposed through a center of the platter or support structure; and shielding a portion of each workpiece from a stream of line-of-sight coating material via a shadow structure disposed about the spindle, inside of the periphery.
A further embodiment of the foregoing method, wherein the plurality of workpieces include a plurality of rotor blades; and wherein each compartment is adapted to receive and secure a root of each rotor blade workpiece such that an airfoil portion of each rotor blade workpiece to be coated is disposed about a periphery of the support structure and extends above the platter.
A further embodiment of any of the foregoing methods, wherein the platter is shaped to conform to a platform of each of the plurality of rotor blades, such that an upper surface of the platform is exposed and a lower surface of the platform is shielded.
While the invention has been described with reference to an exemplary embodiment(s), it will be understood by those skilled in the art that various changes may be made and equivalents may be substituted for elements thereof without departing from the scope of the invention. In addition, many modifications may be made to adapt a particular situation or material to the teachings of the invention without departing from the essential scope thereof. Therefore, it is intended that the invention not be limited to the particular embodiment(s) disclosed, but that the invention will include all embodiments falling within the scope of the appended claims.
1. A line-of-sight coating fixture (10, 110A-C) comprising:
a support structure (12) including a plurality of compartments (20A-C) disposed below a platter (14), each compartment (20A-C) having an opening (30A-C) on a periphery of the support structure (12), and each compartment (20A-C) adapted to receive and secure a base of a workpiece (50A-C) such that a body of each workpiece (50A-C) to be coated is disposed about a periphery of the support structure (12) and extends above the platter (14);
a spindle (16) disposed through a center of the platter (14) or support structure (12) for rotating the workpieces (50A-C) thereabout; and
a shadow structure (18) disposed about the spindle (16), inside of the periphery, the shadow structure (18) sized and adapted to shield a portion of each workpiece (50A-C) from line-of-sight coating material.
2. The fixture (10, 110A-C) of claim 1, wherein the compartment (20A-C) is defined by an enclosure including at least one hinged door (32A-C).
3. The fixture (10, 110A-C) of claim 1 or 2, wherein the plurality of workpieces (50A-C) include a plurality of rotor blades (50).
4. The fixture (10, 110A-C) of claim 3, wherein each compartment (20A-C) is adapted to receive and secure a root (54) of a workpiece (50A-C) such that an airfoil portion (52) of each workpiece (50A-C) to be coated is disposed about a periphery of the support structure (12) and extends above the platter (14).
5. The fixture (10, 110A-C) of claim 4, wherein the platter (14) is shaped to conform to a platform (56) of each of the plurality of rotor blades (50), such that an upper surface (60) of the platform (56) is exposed and a lower surface (62) of the platform (56) is shielded.
6. The fixture (10, 110A-C) of claim 4 or 5, further comprising at least one removable insert (200; 250) adapted to conform to the root (54) of each workpiece (50A-C), wherein, optionally, the at least one removable insert (200) includes a first insert (202) and a second insert (204) adapted to conform to first and second sides of a dovetail root (54).
7. The fixture (10, 110A-C) of any of claims 3 to 6, wherein a span of the plurality of airfoils (52) are aligned with a rotational axis (A) of the fixture (10) or spindle (16).
8. The fixture (10, 110A-C) of any of claims 3 to 7, wherein the shadow structure (18) includes a plurality of shadow bars (26A-C) including a plurality of shadow walls defining a recess for separately covering each trailing edge (68) of the plurality of airfoils (52), and wherein, optionally, the recesses defined by the plurality of shadow bars (26A-C) also cover a window or outlet portion (80) of a pressure surface (76) adjacent to the trailing edge (68).
9. A line-of-sight coating apparatus (100) comprising:
a coating chamber (102) defined by at least one wall (104);
a line-of-sight coating source (108) disposed along the at least one wall (104) and directed toward a plurality of fixtures (10, 110A-C) according to any preceding claim.
10. The apparatus (100) of claim 9, wherein:
the plurality of fixtures (10, 110A-C) are arranged linearly or longitudinally opposed to the coating source (108); and/or
the coating source (108) includes an EB-PVD coating source.
11. The apparatus (100) of claim 9 or 10, wherein the compartments (20A-C) are operative to shield at least the base of each workpiece (50A-C) from the line-of-sight coating material.
12. The apparatus (100) of claims 3 and 9, 10 or 11, wherein the plurality of compartments (20A-C) each include at least one removable insert (200; 250) adapted to receive and secure a root portion (54) of a rotor blade (50) such that a platform portion (56) and an airfoil portion (52) extend above the platform (56) in a first orientation.
13. A method of line-of-sight coating comprising:
securing a base of a workpiece (50A-C) to a support structure (12) including a plurality of compartments (20A-C) disposed below a platter (14), each compartment (20A-C) having an opening (30A-C) on a periphery of the support structure (12) for receiving each workpiece base, such that a body of each workpiece (50A-C) to be coated is disposed about a periphery of the support structure (12) and extends above the platter (14);
rotating the workpieces (50A-C) about a spindle (16) disposed through a center of the platter (14) or support structure (12); and
shielding a portion of each workpiece (50A-C) from a stream of line-of-sight coating material via a shadow structure (18) disposed about the spindle (16), inside of the periphery.
14. The method of claim 13, wherein the plurality of workpieces (50A-C) include a plurality of rotor blades (50), and wherein each compartment (20A-C) is adapted to receive and secure a root (54) of each rotor blade workpiece (50A-C) such that an airfoil portion (52) of each rotor blade workpiece (50A-C) to be coated is disposed about a periphery of the support structure (12) and extends above the platter (14).
15. The method of claim 14, wherein the platter (14) is shaped to conform to a platform (56) of each of the plurality of rotor blades (50), such that an upper surface (60) of the platform (56) is exposed and a lower surface (62) of the platform (56) is shielded.
72.80.140499
EP
18214948.4
United Technologies Corporation
1
DH
20190513
C23C
H01J
B05C
US
2013149450
A1
FEUERSTEIN ALBERT [US] ET AL
20130613
X
1-15
* paragraphs [0019] - [0024], [0033]; figures 2,3,5 *
US
9381537
B2
MCPHERSON DAVID A [US]; FEUERSTEIN ALBERT [US] ET AL.
20160705
X
1-15
* col. 2, l. 58 - col. 6, l. 14;;figures 4,6,7 *
Peijzel, Paul
The Hague
20190503
US
2013149450
A1
20130613
CA
2858093
A1
20130613
EP
2788525
A2
20141015
KR
20140108252
A
20140905
SG
11201402968X
A
20141030
US
2013149450
A1
20130613
WO
2013086286
A2
20130613
US
9381537
B2
20160705
CA
2858188
A1
20130613
EP
2788526
A2
20141015
KR
20140108253
A
20140905
SG
11201402975S
A
20141030
US
2013177707
A1
20130711
WO
2013086339
A2
20130613