ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESMMAKHTNMD..........
J
BDM Ver 0.1.67 (18 Oct 2017) - 1100000/0
3511630
EUROPEAN PATENT APPLICATION
A1
20190717
EP
19151808.3
20190115
en
en
en
18151649
20180115
EP
20190717
201929
20190717
201929
F24C 15/06 20060101AFI20190322BHEP
de
ABDECKPLATTE, INSBESONDERE FÜR EIN HAUSHALTSGERÄT
en
COVER PANEL, PARTICULARLY FOR A DOMESTIC APPLIANCE
fr
PANNEAU DE COUVERTURE POUR APPAREIL DOMESTIQUE
1
ELECTROLUX APPLIANCES AKTIEBOLAG
101657649
P-62058/EP1
S:t Göransgatan 143
105 45 Stockholm
SE
VOGT, Tobias
Electrolux Rothenburg GmbH Factory and Development Bodelschwinghstr. 1
91541 Rothenburg ob der Tauber
DE
BOß, Sebastian
Electrolux Rothenburg GmbH Factory and Development Bodelschwinghstr. 1
91541 Rothenburg ob der Tauber
DE
SUNDBLAD, Linus
AB Electrolux S:t Göransgatan 143
105 45 Stockholm
SE
WESTMAN, Elina
AB Electrolux S:t Göransgatan 143
105 45 Stockholm
SE
FESER, Jürgen
Electrolux Rothenburg GmbH Factory and Development Bodelschwinghstr. 1
91541 Rothenburg ob der Tauber
DE
Electrolux Group Patents
101617600
AB Electrolux Group Patents
105 45 Stockholm
SE
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
KH
MA
MD
TN
The present invention relates to a cover panel (10), particularly for a domestic appliance. The cover panel (10) comprises a glass panel (12) and at least one elongated straight-lined profile element (14). The profile element (14) is glued at a straight-lined side of the glass panel (12). At least a part of the profile element (14) has an L-shaped cross-section. A first leg (16) of the L-shaped cross-section covers at least partially a narrow side of the glass panel (12). A second leg (18) of the L-shaped cross-section extends parallel to a large-area side of the glass panel (12). The glass panel (12) includes a recess (20) for receiving the second leg (18) of the L-shaped cross-section, while the first leg (18) of the L-shaped cross-section is arranged outside of said recess (20).
The present invention relates to a cover panel, particularly for a domestic appliance. Further, the present invention relates to a domestic appliance.
A cover panel with a glass panel, particularly provided for a domestic appliance, is often equipped with a metal or plastic trim element. Said trim element is glued onto the glass panels. Further, the trim element is very thin, so that the trim element does not considerably overhang from the glass panel. Thus, the trim element cannot effectively protect the glass panel from impacts and scratches in sensible areas. Moreover, the thin trim element itself is sensitive to impacts and scratches.
Furthermore, the design effect of such a trim element is not satisfactory, since the front sides of the trim element and the glass panel have different heights. Said different heights lead also to problems in cleaning the cover panel.
It is an object of the present invention to provide a cover panel including a glass panel and at least one trim element, wherein the trim element provides an effective protection of the glass panel and the cover panel has an improved design.
The object of the present invention is achieved by the cover panel according to claim 1.
According to the present invention a cover panel, particularly for a domestic appliance is provided. Said cover panel comprises a glass panel and at least one elongated straight-lined profile element, wherein
- the profile element is glued at a straight-lined side of the glass panel,
- at least a part of the profile element has an L-shaped cross-section,
- a first leg of the L-shaped cross-section covers at least partially a narrow side of the glass panel,
- a second leg of the L-shaped cross-section extends parallel to a large-area side of the glass panel, and
- the glass panel includes a recess for receiving the second leg of the L-shaped cross-section, while the first leg of the L-shaped cross-section is arranged outside of said recess.
The main idea of the present invention is that a part of the profile element is received by the recess of the glass panel. On the one hand, the profile element acts as a trim element providing a flush transition between the profile element and the glass panel. On the other hand, the profile element acts as a protection device for the edge of said glass panel.
The recess forms a step in the glass panel, wherein the edges of said step extend parallel to the straight-lined side of the glass panel. The recess has a simple geometric structure and can be easily manufactured. The recess is substantially complementary to the second leg of the L-shaped cross-section. For example, the first leg of the L-shaped cross-section extends like a cantilever above, beside or beneath the narrow side of the glass panel. Alternatively, the first leg of the L-shaped cross-section may be aligned at the narrow side of the glass panel.
Preferably, an outer surface of the large-area side of the glass panel and an outer surface of the second leg are arranged at the same level. This provides an improved design and allows an easy cleaning of the cover panel.
For example, the second leg of the L-shaped cross-section is longer than the first leg of said L-shaped cross-section.
Further, the first leg of the L-shaped cross-section may cover completely the narrow side of the glass panel. This contributes to the improved design and easy cleaning of the cover panel.
According to the preferred embodiment of the present invention the glass panel is rectangular.
Particularly, the profile element is made of metal, for example stainless steel or aluminium, or made of plastics.
Preferably, the profile element and the recess extend along the entire length of the straight-lined side of the glass panel. Alternatively, the profile element extends along the nearly entire length of the straight-lined side of the glass panel, while the recess extend along the entire length of the straight-lined side of the glass panel. This allows an efficient protection of the edge of the glass panel.
For example, the profile element is glued at the glass panel by at least one silicon adhesive.
Alternatively, the profile element may be glued at the glass panel by hot melt.
Further, the profile element may be glued at the glass panel by at least one UV adhesive.
Moreover, the profile element may be glued at the glass panel by at least one double-sided adhesive tape.
Optionally, the first leg of the L-shaped cross-section is spaced from the narrow side of the glass panel.
Preferably, a milling edge is formed between the outer surface of the large-area side of the glass panel and the recess.
Furthermore, the cover panel may comprise at least one ground element arranged between the profile element and the glass panel.
For example, the ground element is U-shaped and protrudes at the opposite side of the second leg.
At last, the present invention relates to a domestic appliance comprising at least one cover panel mentioned above.
Novel and inventive features of the present invention are set forth in the appended claims.
The present invention will be described in further detail with reference to the drawing, in which
FIG 1
illustrates a schematic sectional side view of a cover panel according to a preferred embodiment of the present invention,
FIG 2
illustrates a schematic perspective view of the cover panel according to the preferred embodiment of the present invention, and
FIG 3
illustrates a schematic perspective view of a door with the cover panel according to the preferred embodiment of the present invention.
FIG 1 illustrates a schematic sectional side view of a cover panel 10 according to a preferred embodiment of the present invention. Particularly, the cover panel 10 is provided for a domestic appliance. For example, the cover panel 10 is attached at a front wall or at a door of said domestic appliance.
The cover panel 10 comprises a glass panel 12 and a profile element 14. The glass panel 12 includes a recess 20. In this example, the recess 20 is elongated and extends along an edge of the glass panel 12. The profile element 14 acts as a trim element, which improves the design of the cover panel 10. Moreover, the profile element 14 acts as a protection device for the edge of the glass panel 12.
The profile element 14 has an L-shaped cross-section with a first leg 16 and second leg 18. The outer edge between the first leg 16 and the second leg 18 is rounded. The first leg 16 covers an upper narrow side of the glass panel 12. The second leg 18 is received by the recess 20. The outer surface of the large-area side of the glass panel 12 and the outer surface of the second leg 18 are arranged at the same level. The recess 20 is obtained by removing material from the glass panel 12.
The first leg 16 and the second leg 18 of the profile element 14 have a thickness between 0.5 mm and 1.0 mm. The relative high thickness of the profile element 14 provides increased elastic properties, which improves the protection of the underlying glass panel 12 against impacts and collision with other part.
The profile element 14 is glued at the glass panel 12 by an adhesive 22, wherein said adhesive is arranged between the recess 20 and a rear side of the second leg 18 of the profile element 14. For example, the profile element 14 is glued at the glass panel 12 by a silicon adhesive. Tolerances of the profile element 14 and the recess 20 may be compensated by the silicon adhesive. Alternatively, the profile element 12 may be glued at the glass panel 12 by hot melt 22. Said hot melt 22 has a fast hardening and can compensate tolerances of the profile element 14 and the recess 20. Further, the profile element 12 may be glued at the glass panel 12 by at least one UV adhesive 22. The UV adhesive 22 has a very fast hardening and can also compensate tolerances of the profile element 14 and the recess 20. Moreover, the profile element may be glued at the glass panel 12 by at least one double-sided adhesive tape 22. Said double-sided adhesive tape 22 allows an immediately fixing of the profile element 14 at the glass panel 12. The double-sided adhesive tape 22 can be applied manually without any tool.
Preferably, the profile element 14 and the recess 20 extend along the entire length of the straight-lined side of the glass panel 12. Alternatively, the profile element 14 extends along the nearly entire length of the straight-lined side of the glass panel 12, while the recess 20 extends along the entire length of the straight-lined side of the glass panel 12. Thus, the profile element 14 acts as protection device for the edge of the glass panel 12. Moreover, the profile element 14 acts as trim element providing the flush transition between said profile element 14 and the glass panel 12. The recess 20 extending along the entire length of the glass panel 12 can be easily manufactured.
Preferably, a milling edge 24 is formed between the outer surface of the large-area side of the glass panel 12 and the recess 20. Said milling edge 24 can be executed in different angles. The milling edge 24 improves the optical appearance of the cover panel 10, since the milling edge 24 provides a narrow slit between the profile element 14 and the large-area side of the glass panel 12.
The first leg 16 of the L-shaped cross-section of the profile element 14 may be spaced from the narrow side of the glass panel 12.
Optionally, the cover panel 10 comprises at least one ground element 26 made of metal. Preferably, the ground element 26 is arranged between the profile element 14 and the glass panel 12. In this example, the ground element 26 is U-shaped and protrudes at the opposite side of the second leg 18 of said profile element 14. The ground element 26 allows an earthing of the profile element 14. This is advantageous, if sensitive electronic circuits are arranged behind or closed to the cover panel 10.
In this example, the profile element 14 has an L-shaped cross-section and is elongated and straight-lined. In general, the profile element 14 may have an arbitrary geometric structure. The profile element 14 is made of metal, for example stainless steel or aluminium, or made of plastics. The profile element 14 may be manufactured by extrusion, bending, stamping and injection moulding.
FIG 2 illustrates a schematic perspective view of the cover panel 10 according to the preferred embodiment of the present invention. FIG 2 shows the upper portion of said cover panel 10.
The cover panel 10 comprises the glass panel 12 and the profile element 14. In the preferred embodiment, the profile element 14 extends along the entire length of the straight-lined side of the glass panel 12. Alternatively, the profile element 14 extends along the nearly entire length of the straight-lined side of the glass panel 12, while the recess 20 extends along the entire length of the straight-lined side of the glass panel 12. The recess 20 extending along the entire length of the glass panel 12 can be easily manufactured. The profile element 14 acts as protection device for the edge of the glass panel 12. Moreover, the profile element 14 acts as trim element providing the flush transition between said profile element 14 and the glass panel 12 and improves the design of the cover panel 10.
The profile element 14 has the L-shaped cross-section with the first leg 16 and the second leg 18. The outer edge between the first leg 16 and the second leg 18 is rounded. The first leg 16 covers the upper narrow side of the glass panel 12. In this example, the first leg 16 of the L-shaped cross-section extends like a cantilever above the narrow side of the glass panel 12. Alternatively, the first leg 16 of the L-shaped cross-section may be aligned on the narrow side of the glass panel 12.
The second leg 18 of the L-shaped cross-section is received by the recess 20, while the first leg 16 of the L-shaped cross-section is arranged outside of said recess 20. The recess 20 has a simple geometric structure and can be easily manufactured. The recess 20 is substantially complementary to the second leg 18 of the L-shaped cross-section. The outer surface of the large-area side of the glass panel 12 and the outer surface of the second leg 18 are arranged at the same level. The recess 20 is obtained by removing material from the glass panel 12.
FIG 3 illustrates a schematic perspective view of a door 30 with the cover panel 10 according to the preferred embodiment of the present invention. FIG 3 shows the upper portion of said door 30. Preferably, the door 30 is provided for the domestic appliance.
The door 30 includes a door frame 28 and the cover panel 10. The cover panel 10 is attached at a front side of the door frame 28. The door frame 28 and the cover panel 10 have substantially the same heights and widths. In this example, the profile element 14 is arranged at the upper end of the door 30. Alternatively or additionally, the profile element 14 may be arranged at the lower end of said door 30. Moreover, the profile element 14 may be arranged at one or both lateral ends of the door 30.
Further, the cover panel 10 may be attached at a front frame of the domestic appliance, so that the cover panel 10 and the front frame form a front panel for the domestic appliance. For example, said front panel may be a cover panel or a control panel. Further, the front panel may be a cover panel of a drawer of the domestic appliance. For example, the front panel may be a cover panel of a water drawer of a steam cooking oven.
The present invention provides the profile element 14 received by the recess 20 in the glass panel 12. On the one hand, the profile element 14 acts as trim element providing the flush transition between the profile element 14 and the glass panel 12. On the other hand, the profile element 14 acts as protection device for the edge of said glass panel 12.
Although an illustrative embodiment of the present invention has been described herein with reference to the accompanying drawing, it is to be understood that the present invention is not limited to that precise embodiment, and that various other changes and modifications may be affected therein by one skilled in the art without departing from the scope or spirit of the invention. All such changes and modifications are intended to be included within the scope of the invention as defined by the appended claims.

List of reference numerals
10
cover panel
12
glass panel
14
profile element
16
first leg
18
second leg
20
recess
22
adhesive, hot melt, adhesive tape
24
milling edge
26
ground element
28
door frame
30
door
1. A cover panel (10), particularly for a domestic appliance, comprising:
- a glass panel (12) and
- at least one elongated straight-lined profile element (14), wherein
- the profile element (14) is glued at a straight-lined side of the glass panel (12),
- at least a part of the profile element (14) has an L-shaped cross-section,
- a first leg (16) of the L-shaped cross-section covers at least partially a narrow side of the glass panel (12),
- a second leg (18) of the L-shaped cross-section extends parallel to a large-area side of the glass panel (12), and
- the glass panel (12) includes a recess (20) for receiving the second leg (18) of the L-shaped cross-section, while the first leg (18) of the L-shaped cross-section is arranged outside of said recess (20).
2. The cover panel according to claim 1,
characterised in that
an outer surface of the large-area side of the glass panel (12) and an outer surface of the second leg (18) are arranged at the same level.
3. The cover panel according to claim 1 or 2,
characterised in that
the second leg (18) of the L-shaped cross-section is longer than the first leg (16) of said L-shaped cross-section.
4. The cover panel according to any one of the preceding claims,
characterised in that
the first leg (16) of the L-shaped cross-section covers completely the narrow side of the glass panel (12).
5. The cover panel according to any one of the preceding claims,
characterised in that
the glass panel (12) is rectangular.
6. The cover panel according to any one of the preceding claims,
characterised in that
the profile element (14) is made of metal, for example stainless steel or aluminium, or made of plastics.
7. The cover panel according to any one of the preceding claims,
characterised in that
the profile element (14) and/or the recess (20) extend along the entire length of the straight-lined side of the glass panel (12).
8. The cover panel according to any one of the preceding claims,
characterised in that
the profile element (14) is glued at the glass panel (12) by at least one silicon adhesive (22).
9. The cover panel according to any one of the preceding claims,
characterised in that
the profile element (14) is glued at the glass panel (12) by hot melt (22).
10. The cover panel according to any one of the preceding claims,
characterised in that
the profile element (14) is glued at the glass panel (12) by at least one UV adhesive (22).
11. The cover panel according to any one of the preceding claims,
characterised in that
the profile element (14) is glued at the glass panel (12) by at least one double-sided adhesive tape (22).
12. The cover panel according to any one of the preceding claims,
characterised in that
the first leg (16) of the L-shaped cross-section is spaced from the narrow side of the glass panel (12).
13. The cover panel according to any one of the preceding claims,
characterised in that
a milling edge (24) is formed between the outer surface of the large-area side of the glass panel and the recess.
14. The cover panel according to any one of the preceding claims,
characterised in that
the cover panel (10) comprises at least one ground element (26) arranged between the profile element and the glass panel, wherein preferably the ground element (26) is U-shaped and protrudes at the opposite side of the second leg (18) .
15. A domestic appliance,
characterised in that
the domestic appliance comprises at least one cover panel (10) according to any one of the claims 1 to 14.
P-62058/EP1
EP
19151808.3
ELECTROLUX APPLIANCES AKTIEBOLAG
1
DH
20190328
F24C
DE
102015212002
A1
BSH HAUSGERÄTE GMBH [DE]
20170216
X
1-15
* figures 1,2 *
* paragraphs [0019] - [0022] *
EP
2722594
A1
BSH BOSCH SIEMENS HAUSGERAETE [DE]
20140423
A
1-15
* figures 1-4 *
* paragraphs [0039], [0040] *
EP
2660524
A1
BSH BOSCH SIEMENS HAUSGERAETE [DE]
20131106
A
1-15
* figures 1,2 *
* paragraphs [0020] - [0023] *
Moreno Rey, Marcos
The Hague
20190320
DE
102015212002
A1
20170216
NONE
EP
2722594
A1
20140423
EP
2722594
A1
20140423
ES
2456826
A2
20140423
EP
2660524
A1
20131106
EP
2660524
A1
20131106
ES
2429913
A2
20131118