ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESMMAKHTNMD..........
J
BDM Ver 1.7.2 (20 November 2019) - 1100000/0
3851293
EUROPEAN PATENT APPLICATION
A1
20210721
EP
21382039.2
20210119
es
en
en
202030081 U
20200120
ES
20210721
202129
20210721
202129
B43L 15/00 20060101AFI20210525BHEP
A47B 97/04 20060101ALI20210525BHEP
B44D 3/00 20060101ALI20210525BHEP
de
MALSTOCK
en
MAHLSTICK
fr
APPUIE-MAIN
6
Castro Dominguez, Tomas
101884938
20-008-B/OT111888
Passeig de Rocafonda, 51 5º 1ª
08304 Mataro
ES
Castro Dominguez, Tomas
Passeig de Rocafonda, 51 5º 1ª
08304 Mataro
ES
Isern Patentes y Marcas S.L.
101725318
Avda. Diagonal, 463 Bis, 2°
08036 Barcelona
ES
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
KH
MA
MD
TN
The present invention relates to a mahlstick for painting which comprises an elongated body of variable length that extends axially, which includes a securing portion located at one end of the elongated body, which protrudes perpendicular to the longitudinal axis of the elongated body, the securing portion being configured by way of support point to be locatable on an upper edge of a surface to be painted, including a stepped portion located prior to the securing portion.

Object of the Invention
The object of this application is the registration of a mahlstick for painting.
More specifically, the invention proposes the development of an accessory to paint a canvas, painting or similar that facilitates the execution thereof for the painter, being an accessory that is simple to manufacture and use.

Background of the invention
It is common that when a painting is being painted, it is necessary to support the hand of the painter to be able to make various detail strokes that the work requires. The problem is that normally the paint is never dry enough to be able to touch the material or surface with your hands, and even less to lean on it. This problem is solved by using an accessory called a mahlstick, which consists of a tool that is used as a support element that enables high-precision brush strokes to be made.
For use thereof, the painter must hold the mahlstick with one hand while brushing with the other hand, which can be somewhat cumbersome and complicated for the painter since he must be aware of correctly holding the mahlstick, so his concentration for brushing is diminished due to ensuring an adequate control and grip of the mahlstick.
Furthermore, the applicant is not currently aware of an invention that has all the features described in this specification.

Description of the invention
The present invention has been developed in order to provide a mahlstick for painting that is a novelty within the field of application and solves the aforementioned drawbacks, further contributing other additional advantages that will be apparent from the description that follows.
It is therefore an object of the present invention to provide a mahlstick for painting, characterised in that it comprises an elongated body of variable length that extends axially, which includes a securing portion located at one end of the elongated body, which protrudes perpendicular to the longitudinal axis of the elongated body, the securing portion being configured by way of support point to be locatable on an upper edge of a surface to be painted, including a stepped portion located prior to the securing portion.
Preferably, the mahlstick can be made of wood or similar material.
Alternatively, the mahlstick can be made of a plastic material, or even a metal material such as, for example, aluminium, that enables the reduction of the weight thereof.
Preferably, the aforementioned securing portion defines a right angle with respect to the elongated body.
Alternatively, in the mahlstick, the elongated body may exhibit a longitudinal through groove and incorporates support means arranged in the same groove; said groove being arranged in the same longitudinal extension of the elongated body; and said support means being enabled to be movable and fixable along the same groove, and further enabled for a support resulting from the same elongated body on a lower edge of a board on which the surface to be painted extends.
Additionally, the support means in the mahlstick may comprise a stop and screw elements, which are mutually enabled and in relation to the groove itself for the longitudinal movement thereof along the same groove; and also enabled for fixing the same stop in a desired position in the longitudinal extension of the same groove and a support of the same stop on the lower edge of the board on which the surface to be painted extends.
Due to these features, a mahlstick is obtained that provides all the advantages of using a mahlstick, but that also facilitates the handling thereof since the user does not have to hold it, given that due to the configuration thereof it can rest on the board, canvas, painting or similar, that has the surface to be brushed, the contact points of this mahlstick being the upper and lower edges of the board. The arrangement of the step prevents the mahlstick from contacting the painted surface, avoiding damage to the painting at all times.
This tool enables the artist to achieve much more precise brush strokes and with more nuances during the execution of the painting that can be much more complicated to obtain without this accessory.
Thus, the described mahlstick represents an innovative structure with structural and constitutive features hitherto unknown for the intended purpose thereof, reasons that together with the practical utility thereof, provide it with a sufficient foundation to obtain the privilege of exclusivity that is requested.
Other features and advantages of the mahlstick object of the present invention will be apparent from the description of a preferred, but not exclusive, embodiment, illustrated by way of nonlimiting example in the attached drawings, in which:

Brief description of the drawings
- Figure 1 is a side elevation view of the mahlstick according to the present invention;
- Figure 2 is a front elevation view of the mahlstick represented in Figure 1;
- Figure 3 is a schematic side elevation view of the mahlstick of the invention placed on a surface of a canvas to be painted;
- Figure 4 is a schematic front elevation view of the mahlstick of the invention placed on a surface of a canvas to be painted;
- Figure 5 is a schematic view from different perspectives of another preferred embodiment of the mahlstick of the present invention; and
- Figure 6 is a schematic perspective view and indicative of a use of a preferred embodiment represented in Figure 5 of the mahlstick of the present invention.

Description of a preferred embodiment
In view of the aforementioned figures and, according to the numbering adopted, a preferred exemplary embodiment of the invention can be seen therein, which comprises the portions and elements that are indicated and described in detail below.
The mahlstick for painting, indicated generally with the numerical reference (1), especially applicable to artistic painting, basically comprises an elongated body (2) of variable length that extends axially, which includes a securing portion (3) located at one end or close to one end of the elongated body (2), which extends perpendicular to the longitudinal axis of the elongated body, the securing portion (3) being configured by way of a support point to be locatable on an upper edge of a board (10) with a surface to be painted (see Figures 3 and 4), including a stepped portion (4) located prior to the securing portion (3).
The mahlstick (1) can be made of wood, a plastic material of a known type such as, for example, polypropylene, aluminium or a combination thereof.
As can be seen more clearly in Figure 1, the securing portion (3) defines a right angle with respect to the elongated body (2), in other words, in side elevation view, it defines a substantially inverted L-shape during use thereof.
In another preferred embodiment of the mahlstick of the proposed invention, the elongated body (2) may exhibit a longitudinal through groove (21), arranged and concordant with the same longitudinal extension of the elongated body (2), as seen in Figure 5 and from different perspectives.
In this same preferred embodiment, the elongated body (2) incorporates support means that are movable along the groove (21). Said support means are enabled to support the same elongated body (2) on a lower edge of the board (10).
In this preferred embodiment represented in Figure 5, the support means comprise a stop (22) and screw elements (23), mutually enabled and in relation to the groove itself (21) for the longitudinal movement thereof along the same groove (21) as indicated by the arrows in Figure 5, and also enabled for fixing the same stop (22) in a desired position in the longitudinal extension of the same groove (21).
As seen in Figure 6, indicative of a use of this preferred embodiment of the mahlstick of the present invention, the stop (22) can be supported on a lower edge of the board (10), with the aforementioned added advantage of being able to move along the groove (21) as indicated by the arrows in Figure 6, and therefore being adaptable to any size that the board (10) may exhibit.
This preferred embodiment explained and schematically represented in Figures 5 and 6, further provides the added advantage that when the easel or board (10) is at 90 degrees with respect to the ground, the mahlstick for painting of the invention is held without touching the material of the surface to be painted arranged on the same board (10).
Details, shapes, dimensions and other accessory elements, used in the manufacture of the mahlstick of the invention may be conveniently replaced by others that do not depart from the scope defined by the claims included below.
1. A mahlstick for painting, characterised in that it comprises an elongated body of variable length that extends axially, which includes a securing portion located at one end of the elongated body, which protrudes perpendicular to the longitudinal axis of the elongated body, the securing portion being configured by way of support point to be locatable on an upper edge of a surface to be painted, including a stepped portion located prior to the securing portion.
2. The mahlstick for painting according to claim 1, characterised in that it is made of wood or similar.
3. The mahlstick for painting according to claim 1, characterised in that it is made of a plastic material.
4. The mahlstick for painting according to claim 1, characterised in that it is made of aluminium or similar.
5. The mahlstick for painting according to any of the preceding claims, characterised in that the securing portion defines a right angle with respect to the elongated body.
6. The mahlstick for painting according to any of the preceding claims, characterised in that the elongated body exhibits a longitudinal through groove and incorporates support means arranged in the same groove; said groove being arranged in the same longitudinal extension of the elongated body; and said support means being enabled to be movable and fixable along the same groove, and further enabled for a support resulting from the same elongated body on a lower edge of a board on which the surface to be painted extends.
7. The mahlstick for painting according to claim 6, characterised in that the support means comprise a stop and screw elements, which are mutually enabled and in relation to the groove itself for the longitudinal movement thereof along the same groove; and also enabled for fixing the same stop in a desired position in the longitudinal extension of the same groove and a support of the same stop on the lower edge of the board on which the surface to be painted extends.
20-008-B/OT111888
EP
21382039.2
Castro Dominguez, Tomas
6
MN
20210531
B43L
A47B
B44D
US
5172883
A
AMIRIAN ACOP J [US]
19921222
X
1-7
* the whole document *
US
4134614
A
FIELDING SR GORDON W
19790116
A
1-7
* the whole document *
Kelliher, Cormac
Munich
20210520
US
5172883
A
19921222
NONE
US
4134614
A
19790116
NONE