ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSK..HRIS..MTNORS..SM..................
J
BDM Ver 2.0.14 (4th of August) - 1100000/0
This application was filed on 25-05-2021 as a divisional application to the application mentioned under INID code 62.
Claims filed after the date of receipt of the divisional application (Rule 68(4) EPC).
3943042
EUROPEAN PATENT APPLICATION
A1
20220126
EP
21175783.6
20131220
en
en
en
201261740351 P
20121220
US
201361907345 P
20131121
US
20220126
202204
20220126
202204
A61C 17/02 20060101AFI20211207BHEP
A61C 17/20 20060101ALI20211207BHEP
A61C 5/40 20170101ALI20211207BHEP
A61C 17/02 20130101 FI20210120RHEP
A61C 17/20 20130101 LA20140516BHEP
A61C 5/40 20170201 LI20170201BHEP
de
VORRICHTUNG ZUM REINIGEN DER ZÄHNE UND DER ZAHNWURZELKANÄLE
en
APPARATUS FOR CLEANING TEETH AND ROOT CANALS
fr
APPAREIL DE NETTOYAGE DE DENTS ET DE CANAUX RADICULAIRES
1a
19166433.3
3572036
20190331
13824566.7
2934364
20131220
SONENDO, INC.
101551723
P1883EP02
26061 Merit Circle, Suite 101
Laguna Hills, CA 92653
US
KHAKPOUR, Mehrzad
Laguna Hills, 92653
US
BERGHEIM, Bjarne
Laguna Hills, 92653
US
TEBBS, Richard S.
Laguna Hills, 92653
US
KIPA AB
101881921
Drottninggatan 11
252 21 Helsingborg
SE
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
An apparatus is disclosed for treating a tooth. The apparatus comprises a chamber (6) to be positioned against a tooth; and a fluid motion generator coupled to the chamber (6) and configured to generate a rotational motion of fluid in the chamber (6). When the chamber is positioned against the tooth, the fluid motion generator is positioned outside the tooth. The apparatus is preferably configured to clean a root canal of the tooth. The root canal has a central axis, and the fluid motion generator is preferably configured to generate the rotational motion about an axis transverse to the central axis of the root canal. Embodiments are disclosed for cleaning and/or obturating the tooth..

CROSS-REFERENCE TO RELATED APPLICATIONS
This application claims the benefit of U.S. Provisional Patent Application No. 61/740,351, filed December 20, 2012, entitled "APPARATUS AND METHODS FOR CLEANING TEETH AND ROOT CANALS," and U.S. Provisional Patent Application No. 61/907,345, filed November 21, 2013, entitled "APPARATUS AND METHODS FOR CLEANING TEETH AND ROOT CANALS," each of which is hereby incorporated by reference herein in its entirety and for all purposes.

BACKGROUND

Field of the Invention
The present disclosure relates generally to dentistry and endodontics and to apparatus, methods, and compositions for treating a tooth.

Description of the Related Art
In conventional dental and endodontic procedures, mechanical instruments such as drills, files, brushes, etc. are used to clean unhealthy material from a tooth. For example, dentists often use drills to mechanically break up carious regions (e.g., cavities) in a surface of the tooth. Such procedures are often painful for the patient and frequently do not remove all the diseased material. Furthermore, in conventional root canal treatments, an opening is drilled through the crown of a diseased tooth, and endodontic files are inserted into the root canal system to open the canal spaces and remove organic material therein. The root canal is then filled with solid matter such as gutta percha or a flowable obturation material, and the tooth is restored. However, this procedure will not remove all organic material from the canal spaces, which can lead to post-procedure complications such as infection. In addition, motion of the endodontic file and/or other sources of positive pressure may force organic material through an apical opening into periapical tissues. In some cases, an end of the endodontic file itself may pass through the apical opening. Such events may result in trauma to the soft tissue near the apical opening and lead to post-procedure complications. Accordingly, there is a continuing need for improved dental and endodontic treatments.

SUMMARY
Various non-limiting aspects of the present disclosure will now be provided to illustrate features of the disclosed apparatus, methods, and compositions. Examples of apparatus, methods, and compositions for endodontic treatments are provided.
In one embodiment, an apparatus for treating a tooth is disclosed. The apparatus can comprise a chamber having an access port which places the chamber in fluid communication with a treatment region of the tooth when the chamber is coupled to tooth. The apparatus can include a fluid motion generator coupled to the chamber, the fluid motion generator configured to direct fluid across the access port to generate fluid motion in the chamber.
In another embodiment, an apparatus for treating a tooth is disclosed. The apparatus can comprise a chamber configured to couple to a tooth. A fluid motion generator can be disposed in the chamber and configured to generate a rotational motion of fluid in the chamber. When the chamber is coupled to the tooth, the fluid motion generator can be positioned outside the tooth.
In another embodiment, a method of treating a tooth is disclosed. The method can include positioning a fluid motion generator near an access opening of the tooth. The fluid motion generator can be activated to pass a stream of fluid across the access opening of the tooth. Fluid motion can be generated at a treatment region of the tooth.
In another embodiment, a method of treating a tooth is disclosed. The method can include coupling a chamber to the tooth. The chamber can have a fluid motion generator disposed therein. The fluid motion generator can be disposed outside the tooth. The fluid motion generator can be activated to generate a rotational motion of fluid in the chamber.
In another embodiment, an apparatus for treating a tooth is disclosed. The apparatus can include a chamber configured to couple to a tooth. The apparatus can include a fluid motion generator disposed in the chamber and configured to generate a rotational motion of fluid in the chamber.
In yet another embodiment, an apparatus for treating a tooth is disclosed. The apparatus can comprise a chamber configured to couple to the tooth. A plurality of fluid motion generators can be disposed in the chamber.
In another embodiment, a method for treating a tooth is disclosed. The method can include coupling a chamber to the tooth. The chamber can include a plurality of fluid motion generators disposed therein. The plurality of fluid motion generators can be activated to clean the tooth.
In another embodiment, a method for treating a tooth is disclosed. The method can include forming an access opening in the tooth. The method can include applying a tooth seal around a perimeter of the access opening, the tooth seal having a peripheral boundary. The method can include positioning a chamber within the peripheral boundary of the tooth seal to secure the chamber to the tooth seal.
For purposes of this summary, certain aspects, advantages, and novel features of certain disclosed inventions are summarized. It is to be understood that not necessarily all such advantages may be achieved in accordance with any particular embodiment of the invention. Thus, for example, those skilled in the art will recognize that the inventions disclosed herein may be embodied or carried out in a manner that achieves one advantage or group of advantages as taught herein without necessarily achieving other advantages as may be taught or suggested herein. Further, the foregoing is intended to summarize certain disclosed inventions and is not intended to limit the scope of the inventions disclosed herein.

BRIEF DESCRIPTION OF THE DRAWINGS
The foregoing and other features, aspects, and advantages of the embodiments of the apparatus and methods of cleaning teeth are described in detail below with reference to the drawings of various embodiments, which are intended to illustrate and not to limit the embodiments of the invention. The drawings comprise the following figures in which:
- Figure 1A is a schematic diagram of a system that includes components capable of removing unhealthy or undesirable materials from a root canal tooth.
- Figure 1B is a schematic diagram of a system that includes components capable of removing unhealthy or undesirable material from a treatment region on an exterior surface of the tooth.
- Figure 2A is a schematic side cross-sectional view of a coupling member coupled to a tooth and a pressure wave generator having a distal end portion disposed in a chamber outside the tooth.
- Figure 2B is a schematic side cross-sectional view of a coupling member coupled to a tooth and a pressure wave generator having a distal end portion disposed inside the tooth.
- Figure 3A is a block diagram that schematically illustrates an embodiment of a system adapted to generate a high-velocity jet of fluid for use in dental procedures.
- Figure 3B is a schematic side view illustrating an embodiment of a handpiece comprising a guide tube for delivery of a liquid jet to a portion of the tooth.
- Figures 4A and 4B are graphs that schematically illustrate possible examples of power generated by different embodiments of the pressure wave generators disclosed herein.
- Figure 4C is a graph of an acoustic power spectrum 1445 generated at multiple frequencies.
- Figure 5 is a schematic cross-sectional side view of a coupling member having a fluid inlet passing therethrough.
- Figure 6 is a schematic cross-sectional side view of a coupling member having a fluid inlet and a fluid outlet passing therethrough.
- Figure 7A is a schematic cross-sectional side view of a coupling member having a fluid inlet, a fluid outlet, and a vent configured to regulate a pressure inside the chamber and/or tooth.
- Figure 7B is a schematic cross-sectional side view of a plurality of pressure wave generators coupled with a coupling member.
- Figure 8A is a schematic side cross-sectional view of a coupling member attached or coupled to a tooth by way of a locking tooth seal.
- Figure 8B is a schematic side cross-sectional view of a coupling member having a curved distal end portion shaped to mate with a curved surface of a tooth seal.
- Figure 8C is a schematic side cross-sectional view of a coupling member having an alignment feature comprising a mating tube sized and shaped to fit through an access opening formed in the tooth.
- Figure 9A is a schematic side cross-sectional view of a coupling member and a pressure wave generator comprising a liquid jet device.
- Figure 9B is a schematic side cross-sectional view of a coupling member and a pressure wave generator comprising a light emitting element.
- Figure 9C is a schematic side cross-sectional view of a coupling member and a pressure wave generator comprising a vibrating mechanical element.
- Figure 9D is a schematic side cross-sectional view of a coupling member 3 and a pressure wave generator comprising a stirring element.
- Figure 10A is a side cross-sectional view of a coupling member having a pressure wave generator comprising a fluid inlet configured to generate a rotational fluid motion in a chamber of a coupling member.
- Figure 10B is a side cross-sectional view of a coupling member having a pressure wave generator comprising a liquid jet device configured to generate a rotational fluid motion in a chamber of the coupling member.
- Figure 10C is a side cross-sectional view of a coupling member having a pressure wave generator comprising a light emitting device configured to generate a rotational fluid motion in a chamber of the coupling member.
- Figure 10D is a side cross-sectional view of a coupling member having a pressure wave generator substantially aligned with a central axis Z of the root canal.
- Figure 10E is a side cross-sectional view of a coupling member having a first pressure wave generator and a second pressure wave generator.
- Figure 10F is a schematic top view of a pressure wave generator at least partially disposed in a chamber and configured to generate swirl in the chamber.
- Figure 10G is a schematic top view of multiple pressure wave generators at least partially disposed in a chamber and configured to generate counter-swirl fluid motion in the chamber.
- Figure 11A is a schematic diagram of an experimental setup designed to measure the power output of various tooth cleaning devices.
- Figure 11B is a plot of the voltage (in volts) output by the hydrophone over time (in seconds) for each device tested.
- Figure 12A illustrates images of root canals that compare the use of non-degassed liquid and degassed liquid in the disclosed pressure wave generators.
- Figure 12B is a plot comparing the power output for techniques using non-degassed and degassed liquids.
- Figure 13 is a plot comparing the rates of tissue dissolution (in units of % per second) for Applicant's device versus other devices, for different treatment fluids and compositions.
- Figures 14A-14B are plots relating to the pressure measured at or near the apical opening of the root canal during treatment.
- Figure 14C is a plot of the mass of material extruded through the apex for various simulated peri-apical pressures for Applicant's system and for various needles.
Throughout the drawings, reference numbers may be re-used to indicate a general correspondence between referenced elements. The drawings are provided to illustrate example embodiments described herein and are not intended to limit the scope of the disclosure.

DETAILED DESCRIPTION
The present disclosure describes apparatus, methods, and compositions for performing dental and/or endodontic procedures. Various embodiments disclosed herein can effectively and safely remove unhealthy material from a treatment region of a tooth, e.g., from within the tooth and/or from outside surfaces of the tooth. In particular, the embodiments disclosed herein can remove unhealthy materials, such as unhealthy organic matter, inorganic matter, pulp tissue, caries, stains, calculus, plaque, biofilm, bacteria, pus, decayed tooth matter, and food remnants from the treatment region without substantially damaging healthy dentin or enamel. For example, the disclosed apparatus, methods, and compositions advantageously may be used with root canal cleaning treatments, e.g., to efficiently remove unhealthy or undesirable materials such as organic and/or inorganic matter from a root canal system and/or to disinfect the root canal system. Organic material (or organic matter) includes organic substances typically found in healthy or diseased teeth or root canal systems such as, for example, soft tissue, pulp, blood vessels, nerves, connective tissue, cellular matter, pus, and microorganisms, whether living, inflamed, infected, diseased, necrotic, or decomposed. Inorganic matter includes calcified tissue and calcified structures, which are frequently present in the root canal system. In some embodiments, the root canal can be filled with an obturation material (e.g., a flowable obturation material that can be hardened into a solid or semi-solid state, gutta percha or other solid or semi-solid materials) after treatment of the root canal.

I. Overview of Various Disclosed Embodiments

A. System Overview
Figure 1A is a schematic diagram of a system 1 that includes components capable of removing unhealthy or undesirable materials from a tooth 10. The tooth 10 illustrated in Figure 1A is a premolar tooth, e.g., a tooth located between canine and molar teeth in a mammal such as a human. The tooth 10 includes hard structural and protective layers, including a hard layer of dentin 16 and a very hard outer layer of enamel 17. A pulp cavity 11 is defined within the dentin 16. The pulp cavity 11 comprises one or more root canals 13 extending toward an apex 14 of each root 12. The pulp cavity 26 and root canal 13 contain dental pulp, which is a soft, vascular tissue comprising nerves, blood vessels, connective tissue, odontoblasts, and other tissue and cellular components. Blood vessels and nerves enter/exit the root canal 13 through a tiny opening, the apical foramen or apical opening 15, near a tip of the apex 14 of the root 12. It should be appreciated that, although the tooth 10 illustrated herein is a premolar, the embodiments disclosed herein can advantageously be used to treat any suitable type of tooth, including molars, canines, incisors, etc.
As illustrated in Figure 1A, the system 1 can be used to remove unhealthy materials (such as organic and inorganic matter) from an interior of the tooth 10, e.g., from the root canal 13 of the tooth 10. For example, an endodontic access opening 18 can be formed in the tooth 10, e.g., on an occlusal surface, a buccal surface, or a lingual surface. The access opening 18 provides access to a portion of a pulp cavity 11 of the tooth 10. The system 1 can include a console 2, a pressure wave generator 5, and a coupling member 3 adapted to couple to the tooth 10. The coupling member 3 can define a chamber 6 configured to retain fluid therein. One or more conduits 4 can electrically, mechanically, and/or fluidly connect the console 2 with the coupling member 3 and pressure wave generator 5. The console 2 can include a control system and various fluid management systems configured to operate the pressure wave generator 5 during a treatment procedure.
As explained herein, the system 1 can be used in cleaning procedures to clean substantially the entire root canal system. In other embodiments, such as obturation procedures, the system 1 can be used to fill substantially the entire root canal system with an obturation or filler material. For example, in various embodiments disclosed herein, the pressure wave generator 5 can generate pressure waves 23 of sufficient power and relatively low frequencies to produce fluid motion 24 in the chamber 6 - such that the pressure wave generators 5 disclosed herein can act as a fluid motion generator - and can generate pressure waves of sufficient power and relatively higher frequencies to produce surface effect cavitation on a dental surface, either inside or outside the tooth. That is, for example, the pressure wave generators 5 disclosed herein can act as fluid motion generators to generate large-scale or bulk fluid motion 24 in or near the tooth 10, and can also generate smaller-scale fluid motion at higher frequencies. In some arrangements, the fluid motion 24 in the chamber 6 can generate induced fluid motion such as vortices 75, swirl 76 (see Figure 2B), etc. in the tooth 10 and root canal 13 that can clean and/or fill the canal 13.
Figure 1B is a schematic diagram of a system 1 that includes components capable of removing unhealthy or undesirable material from a treatment region 91 on an exterior surface of the tooth. For example, as in Figure 1A, the system 1 can include a coupling member 3 and a pressure wave generator 5. The coupling member 3 can communicate with a console 2 by way of one or more conduits 4. Unlike the system 1 of Figure 1A, however, the coupling member 3 is coupled to a treatment region 91 on an exterior surface of the tooth 10. For example, the system 1 of Figure 1B can be activated to clean an exterior surface of the tooth 10, e.g., a carious region of the tooth 10. In other embodiments, the system 1 can be activated to fill a treated region on the exterior surface of the tooth 10. As with the embodiment of Figure 1A, fluid motion 24 can be generated in the coupling member 3 and chamber, which can act to clean and/or fill the treatment region 91 of the tooth 10.
Figure 2A is a schematic side cross-sectional view of a coupling member 3 coupled to a tooth 10 and a pressure wave generator 5 having a distal end portion 25 disposed in a chamber 6 outside the tooth 10. The coupling member 3 can be adapted to couple to the tooth 10 to provide a stable platform during the dental procedure. The coupling member 3 can define or include a chamber 6 configured to retain fluid 22. For example, the chamber 6 can be substantially filled with a fluid 22 o provide a propagation medium upon and/or through which the pressure wave generator 5 acts. The fluid 22 can be a treatment fluid in various cleaning treatments to substantially clean a treatment region of the tooth (such as in root canal treatments, treatments of carious regions, treatments of plaque and other unhealthy deposits). Alternatively, in obturation treatments, the fluid 22 can comprise a flowable obturation material having a flowable state that can be hardened into a solid state, and the pressure wave generator 5 can be activated to substantially fill or obturate the treatment region. The obturation material, once it fills the treatment region, can be hardened by a catalyst, be it heat, light, or chemical.
Moreover, the chamber 6 and coupling member 3 can prevent fluid 22 and/or waste materials from leaving the tooth 10. In various embodiments, the coupling member 3 can also be configured to regulate fluid pressure in the tooth 10 such that liquid can flow out from the chamber 6 if pressure rises above a predetermined threshold. In the embodiment of Figure 2A, the coupling member 3 comprises a distal portion 21 of a handpiece 20 (see, e.g., Figure 3B). For example, the distal portion 21 of the handpiece 20 can be shaped to define walls enclosing the chamber 6. In other embodiments, the coupling member 3 can be applied to the tooth 10 with a mechanical clasp or clamp, a dental adhesive, or by pressure applied by the patient by biting on the coupling member 3. In still other embodiments, a separate cap or fluid retainer can be removably coupled to the distal portion 21 of the handpiece 20.
During a dental treatment, a clinician can apply the coupling member 3 to the tooth 10. As illustrated in Figures 1A and 2A, for example, the clinician can apply the coupling member 3 over the access opening 18. The clinician can secure the coupling member 3 to the tooth 10 by way of a tooth seal 26. In some embodiments, one or more alignment features can be applied to align the coupling member 3 to the treatment region of the tooth 10 (see, e.g., Figures 8A-8C). In some embodiments, the coupling member 3 can be attached to the tooth 10 in a manner that permits the clinician to rotate or otherwise orient the coupling member 3 and pressure wave generator 5 at a desired orientation relative to the tooth 10 (see, e.g., Figure 8B). In still other embodiments, the clinician can apply the coupling member 3 and pressure wave generator 5 to an exterior surface of the tooth 10. For example, the clinician can apply the coupling member 3 over a carious region formed near an outer surface of the tooth 10. In yet other embodiments, the clinician or a user can apply the coupling member 3 over an exterior surface of the tooth 10 to remove undesirable dental deposits, such as plaque, calculus, biofilms, etc.
The pressure wave generator 5 can be coupled with or integrally formed with the coupling member 3. In some embodiments, the pressure wave generator 5 can comprise an elongated member extending from the coupling member 3 through a portion of the chamber 6. As shown in Figures 1A and 2A, the distal end portion 25 of the pressure wave generator 5 can be disposed in the chamber 5 defined by the coupling member 3. As shown in Figure 2A, the distal end portion 25 of the pressure wave generator 5 can be disposed outside the tooth 10, e.g., outside the pulp cavity 11. In other embodiments, the distal end portion 25 of the pressure wave generator 5 can extend into an interior space of the tooth 10, e.g., the pulp cavity 11. For example, Figure 2B is a schematic side cross-sectional view of a coupling member 3 coupled to a tooth 10 and a pressure wave generator 5 having a distal end portion 25 disposed inside the tooth 10, e.g., inside a portion of the pulp cavity 11.
During cleaning procedures, the distal end portion 25 of the pressure wave generator 5 can be submerged in treatment fluid retained in the chamber 6 by the coupling member 3. The pressure wave generator 5 can be activated, and unhealthy materials (e.g., unhealthy organic matter, inorganic matter, pulp tissue, caries, stains, calculus, plaque, biofilm, bacteria, pus, decayed tooth matter, and food remnants) can be safely and efficiently removed from the tooth 10. For example, in the embodiments illustrated in Figures 1A-2B, diseased pulp and other undesirable materials can be removed from the pulp cavity 11 and root canal 13 of the tooth 10.
The pressure wave generator 5 can clean treatment regions of the tooth 10 that are remote from the pressure wave generator 5. For example, in root canal procedures, the pressure wave generator can clean substantially the entire root canal 13, including laterally-extending tubules and various small cracks and crevices that are formed in the tooth 10. Similarly, in other cleaning procedures, such as procedures that clean carious regions, plaque, other dental deposits, etc., the pressure wave generators 5 disclosed herein can clean substantially the entire treatment region of the tooth. The pressure wave generators 5 disclosed herein can therefore improve patient outcomes by removing unhealthy materials from the entire treatment region, which reduces the risk of infection or recurrences of unhealthy material at the treatment region.
In other embodiments, the pressure wave generator 5 can fill or obturate the treatment region of the tooth (e.g., a cleaned root canal space, a cleaned carious region on an exterior surface of the tooth, etc.) after cleaning. For example, in root canal procedures, the disclosed pressure wave generators 5 can substantially fill the entire root canal system, including the main canals, laterally-extending tubules, and various small cracks, spaces, crevices, etc. The improved obturation provided by the pressure wave generators 5 disclosed herein can improve patient outcomes by reducing the risk of infection from unobturated spaces in cleaned canals.
Various embodiments of the pressure wave generator 5 disclosed herein can clean and/or fill the tooth 10 by way of a combination of several different phenomena. For example, the pressure wave generator 5 can generate pressure waves 23 that propagate through the fluid 22 and inside the tooth 10, and the pressure wave generator 5 can also act as a fluid motion generator to generate a motion 24 of fluid 22 in the chamber 6.
The fluid motion 24 generated by the fluid motion generators disclosed herein (e.g., the pressure wave generators 5) can be induced by flowing the fluid across an access port of the chamber 6 and/or the coupling member 3. For example, the fluid 22 can be flowed across the access port in a direction substantially parallel to a plane of the access port and/or perpendicular to the central axis of the root canal 13. The fluid motion 24 described in each embodiment disclosed herein can comprise rotational or non-rotational flow patterns in the chamber 6. The fluid motion 24 can be laminar or turbulent. For example, in laminar fluid motions 24, larger or bulk fluid motion may be generated. In turbulent fluid motions 24, smaller fluid motions or perturbations can be generated. In some arrangements, a combination of laminar and turbulent flow may be generated. The fluid flow 24 in the chamber and the induced flow (e.g., vortices, swirl, etc.) in the tooth can be generated in a substantially continuous manner or can be intermittent or periodic. In some embodiments, the fluid motion 24 can comprise rotational motion, e.g., the fluid can rotate about an axis transverse to a central axis of the root canal 13 (see, e.g., Figure 2A). In some arrangements, the fluid motion 24 can induce vortices 75 flowing about an axis substantially perpendicular to the central axis of the root canal 13 (see, e.g., Figure 2A). In other embodiments, the fluid motion 24 can be generated about the central axis of the root canal 13 and can generate a swirl flow 76 that can propagate through the canal 13 (see, e.g., Figure 2B). In still other embodiments, the fluid motion 24 can comprise planar fluid flow, e.g., fluid flow that comprises planar wavefronts. In some embodiments, the fluid motion 24 can comprise unsteady or chaotic flow.
As explained herein, the pressure waves 23 can enhance the chemical reactions produced between treatment fluids and the unhealthy material to enable the detachment of unhealthy materials from the tooth 10 in a safe and efficient manner. For example, the pressure wave generator 5 can be configured to induce acoustic cavitation throughout the tooth 10, which can assist in removing unhealthy materials from larger spaces in the tooth, such as the main root canal 13, as well as from extremely small spaces in the tooth 10, such as tubules and various cracks and crevices that may be formed in the tooth 10.
In tooth cleaning procedures, the motion 24 of the fluid 22 can also improve the cleaning of the tooth 10 by refreshing the chemical reactants used in the fluid 22, which can act to speed up the chemical reactions between the fluid 22 and the unhealthy materials in the tooth. Furthermore, the motion 24 of the fluid 22 can impart momentum in the tooth 10 that helps to dislodge the unhealthy or undesirable materials from the tooth 10 and to irrigate the dislodged materials out of the tooth 10. As explained herein, the motion 24 of the fluid 22 can also reduce apical pressures at or near the apical opening 15 of the tooth 10.
Accordingly, the pressure waves 23 and motion 24 generated by the systems disclosed herein can improve patient outcomes as compared with other treatments by cleaning unhealthy materials from both large and small spaces of the tooth, and by enhancing the chemical reactions between the fluid 22 and the unhealthy materials to be removed from the tooth 10. Furthermore, because the tooth 10 is cleaned without the use of a file, drill, brush, or other abrasive instrument, the systems and methods disclosed herein can clean the tooth with little or no discomfort to the patient. In addition, in obturation procedures, the embodiments disclosed herein can advantageously obturate or fill substantially the entire canal(s) and/or branch structures therefrom, as explained in greater detail below.
In various implementations, the pressure wave generator 5 comprises one or more embodiments of the various apparatus described herein. For example, the pressure wave generator 5 can include a liquid jet device. In some embodiments, the liquid jet device comprises a positioning member (e.g., a guide tube) having a channel or lumen along which or through which a liquid jet can propagate. The distal end portion of the positioning member may include an impingement surface on which the liquid jet impinges and is deflected into jets or spray. The distal end portion of the positioning member may include one or more openings that permit the jet to interact with the fluid in the surrounding environment (e.g., fluid in the tooth chamber) and also permit the deflected liquid to exit the positioning member and interact with the surrounding environment and fluid 22 in the chamber 6 and/or tooth 10. The result of these interactions can be the generation of pressure waves and fluid motion in the tooth 10, which can at least partially clean the tooth 10. By generating fluid motion 24 in the tooth 10, the pressure wave generators 5 may act as fluid motion generators. In some treatment methods, the openings disposed at or near the distal end portion of the positioning member are submerged in the fluid 22 retained in the chamber 6 by the coupling member 3.
In some embodiments, the pressure wave generator 5 may include a sonic, ultrasonic, or megasonic device (e.g., a sonic, ultrasonic, or megasonic paddle, horn, or piezoelectric transducer), a mechanical stirrer (e.g., a motorized propeller or paddle or rotating/vibrating/pulsating disk or cylinder), an optical system that can provides optical energy to the chamber 6 (e.g., an optical fiber that propagates laser light into the chamber 6), or any other device that can cause sufficient rotational fluid motion and acoustic waves to be generated in the tooth or in a propagation medium in the tooth (e.g., the fluid retained in a tooth chamber).

B. Enhancing the Treatment of Teeth
The embodiments disclosed herein can advantageously remove undesirable or unhealthy materials from a tooth such that substantially all the unhealthy material is removed while inducing minimal or no discomfort and/or pain in the patient. For example, when activated by the clinician, the pressure wave generator 5 can induce various fluidic effects that interact with the unhealthy material to be removed, even when the pressure wave generator 5 is disposed at a position remote from the treatment region of the tooth, e.g., the region of the tooth that includes the unhealthy or undesirable material to be removed. The pressure wave generator 5 can impart energy to the fluid 22 that induces the relatively large-scale or bulk circulation or movement 24 of liquid in the chamber 6 and tooth 10, and that also generates pressure waves 23 that propagate through the fluid 22 and tooth 10. The generated fluid motion 24 and pressure waves 23 can magnify or enhance the properties of the fluid 22 to enhance cleaning of the tooth 10. In some embodiments, the pressure wave generator 5 can be used to obturate or fill the root canals and/or other treated regions of the tooth.

(1) Chemistry of Various Treatment Fluids
As explained above, in cleaning procedures, the fluid 22 can comprise a treatment fluid that can be introduced into the tooth 10 and the chamber 6 to assist in removing unhealthy or undesirable materials from the tooth 10. The treatment fluids can be selected based on the chemical properties of the fluids when reacting with the undesirable or unhealthy material to be removed from the tooth 10. The treatment fluids disclosed herein can include any suitable fluid, including, e.g., water, saline, etc. Various chemicals can be added to treatment fluid for various purposes, including, e.g., tissue dissolving agents (e.g., NaOCl or bleach), disinfectants (e.g., chlorhexidine), anesthesia, fluoride therapy agents, ethylenediaminetetraacetic acid (EDTA), citric acid, and any other suitable chemicals. For example, any other antibacterial, decalcifying, disinfecting, mineralizing, or whitening solutions may be used as well. The clinician can supply the various fluids to the tooth in one or more treatment cycles, and can supply different fluids sequentially or simultaneously.
During some treatment cycles, bleach-based solutions (e.g., solutions including NaOCl) can be used to dissociate diseased tissue (e.g., diseased organic matter in the root canal 13) and/or to remove bacteria from the tooth 10. One example of a treatment solution comprises water or saline with 0.3% to 6% bleach (NaOCl). In some methods, tissue dissolution and dental deposit removal in the presence of bleach may not occur when the bleach concentration is less than 1%. In some treatment methods disclosed herein, tissue dissolution and dental deposit removal can occur at smaller (or much smaller) concentrations.
During other treatment cycles, the clinician can supply an EDTA-based solution to remove undesirable or unhealthy calcified material from the tooth 10. For example, if a portion of the tooth 10 and/or root canal 13 is shaped or otherwise instrumented during the procedure, a smear layer may form on the walls of the canal 13. The smear layer can include a semi-crystalline layer of debris, which may include remnants of pulp, bacteria, dentin, and other materials. Treatment fluids that include EDTA may be used to remove part or all of the smear layer, and/or calcified deposits on the tooth 10.
During yet other cycles, for example, the clinician may supply a treatment fluid that comprises substantially water. The water can be used to assist in irrigating the tooth before, during, and/or after the treatment. For example, the water can be supplied to remove remnants of other treatment fluids (e.g., bleach or EDTA) between treatment cycles. Because bleach has a pH that tends to be a base and because EDTA is an acid, it can be important to purge the tooth 10 and chamber 6 between bleach and EDTA treatments to avoid potentially damaging chemical reactions. Furthermore, the water can be supplied with a sufficient momentum to help remove detached materials that are disrupted during the treatment. For example, the water can be used to convey waste material from the tooth 10.
Various solutions may be used in combination at the same time or sequentially at suitable concentrations. In some embodiments, chemicals and the concentrations of the chemicals can be varied throughout the procedure by the clinician and/or by the system to improve patient outcomes. For example, during an example treatment procedure, the clinician can alternate between the use of water, bleach, and EDTA, in order to achieve the advantages associated with each of these chemicals. In one example, the clinician may begin with a water cycle to clean out any initial debris, then proceed with a bleach cycle to dissociate diseased tissue and bacteria from the tooth. A water cycle may then be used to remove the bleach and any remaining detached materials from the tooth 10. The clinician may then supply EDTA to the tooth to remove calcified deposits and/or portions of a smear layer from the tooth 10. Water can then be supplied to remove the EDTA and any remaining detached material from the tooth 10 before a subsequent bleach cycle. The clinician can continually shift between cycles of treatment fluid throughout the procedure. The above example is for illustrative purposes only. It should be appreciated that the order of the cycling of treatment liquids may vary in any suitable manner and order.
Thus, the treatment fluids used in the embodiments disclosed herein can react chemically with the undesirable or unhealthy materials to dissociate the unhealthy materials from the healthy portions of the tooth 10. The treatment fluids can also be used to irrigate waste fluid and/or detached or delaminated materials out of the tooth 10. In some embodiments, as explained in more detail herein in Section VIII, the treatment solution (including any suitable composition) can be degassed, which may improve cavitation and/or reduce the presence of gas bubbles in some treatments. In some embodiments, the dissolved gas content can be less than about 1% by volume. Additional properties and characteristics of the treatment fluid 22 are presented in more detail herein in Section VII.

(2) Enhancement of Cleaning Using Pressure Waves
As explained herein, a pressure wave generator 5 can remove unhealthy materials from a tooth by propagating pressure waves 23 through a propagation medium (e.g., the treatment fluid) to the treatment region, which can include one or more teeth and/or gums. Without being limited by theory, a few potential ways that the pressure waves 23 remove undesirable materials are presented herein. Note that these principles, and the principles described above, may be generally applicable for each embodiment disclosed herein.
In some arrangements, cavitation may be induced by the generated pressure waves 23. Upon irradiation of a liquid (e.g., water or other treatment fluid) with high intensity pressure or pressure waves 23, acoustic cavitation may occur. The oscillation or the implosive collapse of small cavitation bubbles can produce localized effects, which may further enhance the cleaning process, e.g., by creating intense, small-scale localized heat, shock waves, and/or microjets and shear flows. Therefore, in some treatment methods, acoustic cavitation may be responsible for or involved in enhancing the chemical reactions, sonochemistry, sonoporation, soft tissue/cell/bacteria dissociation, delamination and breakup of biofilms.
For example, if the treatment liquid contains chemical(s) that act on a particular target material (e.g., diseased organic or inorganic matter, stains, caries, dental calculus, plaque, bacteria, biofilms, etc.), the pressure waves 23 (acoustic field) and/or the subsequent acoustic cavitation may enhance the chemical reaction via agitation and/or sonochemistry. Indeed, the pressure waves 23 can enhance the chemical effects that each composition has on the unhealthy material to be removed from the tooth. For example, with a bleach-based treatment fluid, the generated pressure waves 23 can propagate so as to dissociate tissue throughout the entire tooth 10, including in the dentinal tubules and throughout tiny cracks and crevices of the tooth 10. As another example, with an EDTA-based treatment fluid, the generated pressure waves 23 can propagate so as to remove the smear layer and/or calcified deposits from the tooth 10, including in the tubules and/or in tiny cracks and crevices formed in the tooth 10. With a water-based treatment fluid, the generated pressure waves 23 can propagate so as to flush and/or irrigate undesirable materials from the tooth, including in tubules and tiny cracks and crevices. Accordingly, the generated pressure waves 23 can enhance the removal of undesirable or unhealthy materials from the tooth 10 by magnifying the chemical effects of whatever treatment fluid composition is used during a particular treatment cycle.
Furthermore, sonoporation, which is the process of using pressure waves and/or the subsequent acoustic cavitation to modify the permeability of the bacterial cell plasma membrane, may also expedite the chemical reaction that removes the microorganisms from the tooth. It should also be appreciated that generated pressure waves, and/or the subsequent acoustic cavitation of certain frequencies, may result in cellular and bacterial rupture and death (e.g., lysis) as well as removal of decayed and weakened dentin and enamel. The cellular and bacterial rupture phenomenon may kill bacteria which might otherwise reinfect the gingival pockets and/or the oral cavity.
Generated pressure waves and/or the subsequent acoustic cavitation may also loosen the bond of the structure of the unhealthy material (e.g., diseased tissue, calculus, biofilm, caries, etc.), and/or the pressure waves may dissociate the unhealthy material from the tooth 10. In some cases, pressure waves and/or acoustic cavitation may loosen the bond between the cells and the dentin and/or delaminate the tissue from the tooth. Furthermore, the pressure waves and/or the subsequent acoustic cavitation may act on decayed hard tissue (which may be relatively weak and loosely connected) through vibrations and/or shock waves, and/or the microjets created as a result of cavitation bubble implosion, to remove decayed hard tissue from other healthy portions of the tooth.
Additional details of the acoustic effects produced by the pressure wave generators disclosed herein may be found herein in more detail in Section VII.

(3) Enhancement of Cleaning Using Large-Scale Fluid Motion
In some arrangements, bulk fluid motion 24 (e.g., fluid rotation, convection, planar flow, chaotic flow, etc.) can enhance the cleaning of unhealthy material from a diseased tooth. For example, the fluid motion 24 generated in the chamber 6 and/or tooth 10 can impart relatively large momentum to the tooth, which can help dissociate and irrigate unhealthy materials from the tooth. Furthermore, the fluid motion 24 can induce vortices 75 and/or swirl 76 in the tooth 10 that can result in negative pressures (or low positive pressures) near the apical opening 15 of the tooth 10. The resulting negative pressures at the apical opening 15 can prevent or reduce an amount of material extruded through the apical opening 15 and into the jaw of the patient. By preventing or reducing the amount of extruded material, the risk of infection can be lowered or eliminated, and patient outcomes can be substantially improved.
In addition, due to relatively short time scales of the chemical reaction processes between the fluid 22 and the unhealthy materials as compared to that of diffusion mechanisms, a faster mechanism of reactant delivery such as "macroscopic" liquid circulation may be advantageous in some of the embodiments disclosed herein. For example, liquid circulation with a time scale comparable to (and preferably faster than) that of chemical reaction may help replenish the reactants at the chemical reaction front and/or may help to remove the reaction byproducts from the reaction site. The relatively large convective time scale, which may relate to effectiveness of the convection process, can be adjusted and/or optimized depending on, e.g., the location and characteristics of the source of circulation. Furthermore, it should be appreciated that the introduction of liquid circulation or other fluid motion 24 generally does not eliminate the diffusion process, which may still remain effective within a thin microscopic layer at the chemical reaction front. Liquid circulation can also cause a strong irrigation effect at the treatment site (e.g. removing diseased tissue deep in the canal 13 and/or tubules and small spaces and cracks of the tooth 10) and may therefore result in loosening and/or removing large and small pieces of debris from the treatment site.
In some arrangements, various properties can be adjusted to enhance bulk fluid motion and/or fluid circulation, e.g., fluid motion in the chamber 6. For example, the position of the pressure wave generator 5 relative to the location of the treatment site can be adjusted. As explained herein, in some embodiments, the pressure wave generator 5 is disposed such that the pressure wave generator 5 passes a stream of liquid across the access opening 18. For example, the pressure wave generator 5 can be disposed to induce fluid motion 24 about an axis transverse to a central axis of the root canal 13, which can generate vortices 75 that propagate throughout the canal 13. In some embodiments, the fluid motion 24 can be generated about the central axis of the root canal 13, which can induce swirl motion 76 in the root canal 13. The fluid flow 24 over the access port or access opening of the tooth 10 can be varied. For example, the momentum of the fluid 24 can be varied to create the desired flow in the root canals 13. Furthermore, the angle of the fluid flow 24 relative to the access port can be varied to control the apical pressure in the canals 13, e.g., to induce apical pressures that are more positive, more negative, etc. The geometry of the space surrounding the pressure wave generator 5 and treatment site (e.g., the geometry of the coupling member 3) can also be varied. It should also be appreciated that circulation may be affected by the viscosity of the fluid 22 and/or the mechanism of action of the pressure wave generator 5. For example, the pressure wave generator 5, such as a jet of liquid ejected through an inlet opening, a stirrer such as a propeller or a vibrating object, etc., can be selected to enhance fluid motion of the treatment fluid. In some aspects, the input power of the source of liquid circulation can also be adjusted, such as the source of a pump that drives a liquid jet in some embodiments.

(4) Enhancement of Other Dental and Endodontic Procedures
In some embodiments, the pressure wave generators 5 disclosed herein can enhance other dental and endodontic procedures. For example, after cleaning a tooth (e.g., a root canal inside the tooth, a carious region on or near an exterior surface of the tooth, etc.), the treatment region can be filled with an obturation or filler material. In some embodiments, the filler material can be supplied to the treatment region as a flowable material and can be hardened to fill the treatment region (e.g., the cleaned root canal or carious region, etc.). In some embodiments, a pressure wave generator 5 can be activated to supply the obturation material throughout the treatment region.
For example, after a root canal procedure, the pressure wave generator can supply the flowable obturation material into the tooth and root canal. The large-scale fluid movement generated by the pressure wave generator 5 can assist in propagating the obturation material throughout relatively large spaces, such as the main root canal or canals. For example, the pressure wave generator 5 may introduce sufficient momentum such that the flowable obturation material propagates throughout the canal space without introducing additional instrumentation into the tooth. For example, the bulk fluid motion of the obturation material into the canal may be such that the clinician may not need to or desire to enlarge the canals. By reducing or eliminating canal enlargement, patient outcomes and pain levels can be improved. In some arrangements, the bulk fluid motion of the flowable obturation material can be generated at relatively low frequencies produced by the pressure wave generator.
In addition to generating large-scale or bulk fluid motion of the obturation material throughout the canal, the pressure wave generators 5 disclosed herein can generate higher frequency perturbations to propagate the obturation material into smaller cracks, spaces, and crevices in the tooth. For example, higher-frequency effects, such as acoustic cavitation, can assist in propagating the filler material throughout the tooth.
Accordingly, the pressure wave generators disclosed herein can enhance the filling of a treatment region such as a root canal, carious region of the tooth, etc. For example, the obturation material can be propagated at a distance such that it flows into the treatment region from a remote pressure wave generator 5 (which may be disposed outside the tooth). Large-scale or bulk fluid motion of the obturation material can fill larger canal spaces or other treatment regions without further enlargening the treatment region. Smaller-scale and/or higher frequency agitation by the pressure wave generator 5 can propagate the obturation material into smaller cracks and spaces of the tooth. By filling substantially all the cleaned spaces of the tooth, the disclosed methods can improve patient outcomes relative to other methods by reducing the risk of infection in spaces unfilled by the obturation material.

II. Overview of Features of the Disclosed Systems

A. Pressure Wave Generators
A pressure wave generator 5 can be used in various disclosed embodiments to clean a tooth 10, e.g., from interior or exterior portions of the tooth 10 and/or gums. In other embodiments, the pressure wave generator 5 can be used to fill or obturate a cleaned root canal or other treatment region of the tooth 10. In some embodiments, the pressure wave generator 5 can comprise an elongated member having an active distal end portion 25. The active distal end portion 25 can be activated by a user to apply energy to the treatment tooth 10 to remove unhealthy or undesirable material from the tooth 10.
As explained herein, the disclosed pressure wave generators 5 can be configured to generate pressure waves 23 and fluid motion 24 with energy sufficient to clean undesirable material from a tooth 10. The pressure wave generator 5 can be a device that converts one form of energy into acoustic waves and bulk fluid motion (e.g., rotational motion) within the fluid 22. The pressure wave generator 5 can induce, among other phenomena, both pressure waves and bulk fluid dynamic motion in the fluid 22 (e.g., in the chamber 6), fluid circulation, turbulence, vortices and other conditions that can enable the cleaning of the tooth. The pressure wave generator 5 disclosed in each of the figures described herein may be any suitable type of pressure wave generator.
The pressure wave generator 5 can be used to clean the tooth 10 by creating pressure waves that propagate through the fluid 22, e.g., through treatment fluid at least partially retained in the chamber 6. In some implementations, the pressure wave generator 5 may also create cavitation, acoustic streaming, turbulence, etc. In various embodiments, the pressure wave generator 5 can generate pressure waves or acoustic energy having a broadband power spectrum (see, e.g., Figures 4A-4C). For example, the pressure wave generator 5 can generate pressure waves at multiple different frequencies, as opposed to only one or a few frequencies. Without being limited by theory, it is believed that the generation of power at multiple frequencies can help to remove various types of organic and/or inorganic materials that have different material or physical characteristics at various frequencies.
The pressure wave generator 5 (e.g., high-speed liquid jet, ultrasonic transducer, a laser fiber, etc.) can be placed at the desired treatment location in or on the tooth 10. The pressure wave generator 5 can create pressure waves 23 and fluid motion 24 within the fluid 22 inside a substantially-enclosed chamber 6. In general, the pressure wave generator 5 can be sufficiently strong to remove unhealthy materials such as organic and/or inorganic tissue from teeth 10. In some embodiments, the pressure wave generator 5 can be configured to avoid substantially breaking down or harming natural dentin and/or enamel.

(1) Liquid Jet Apparatus
For example, in some embodiments, the pressure wave generator 5 can comprise a liquid jet device. The liquid jet can be created by passing high pressure liquid through an orifice. The liquid jet can create pressure waves within the treatment liquid. In some embodiments, the pressure wave generator 5 comprises a coherent, collimated jet of liquid. The jet of liquid can interact with liquid in a substantially-enclosed volume (e.g., the chamber and/or the mouth of the user) and/or an impingement member to create the acoustic waves. In addition, the interaction of the jet and the treatment fluid, as well as the interaction of the spray which results from hitting the impingement member and the treatment fluid, may assist in creating cavitation and/or other acoustic effects to clean the tooth.
In various embodiments, the liquid jet device can comprise a positioning member (e.g., a guide tube) having a channel or lumen along which or through which a liquid jet can propagate. The distal end portion of the positioning member can include one or more openings that permit the deflected liquid to exit the positioning member and interact with the surrounding environment in the chamber 6 or tooth 10. In some treatment methods, the openings disposed at or near the distal end portion of the positioning member can be submerged in liquid that can be at least partially enclosed in the chamber 6 attached to or enclosing a portion of the tooth 10. In some embodiments, the liquid jet can pass through the guide tube and can impact an impingement surface. The passage of the jet through the surrounding treatment fluid and impact of the jet on the impingement surface can generate the acoustic waves in some implementations. The flow of the submerged portion of the liquid jet may generate a cavitation cloud within the treatment fluid. The creation and collapse of the cavitation cloud may, in some cases, generate a substantial hydroacoustic field in or near the tooth. Further cavitation effects may be possible, including growth, oscillation, and collapse of cavitation bubbles. In addition, as explained above, bulk fluid motion, such as rotational flow, may be induced. The induced rotational flow can enhance the cleaning process by removing detached material and replenishing reactants for the cleaning reactions. These (and/or other) effects may lead to efficient cleaning of the tooth.
Figure 3A is a block diagram that schematically illustrates an embodiment of a system 38 adapted to generate a high-velocity jet 60 of fluid for use in dental procedures. The system 38 comprises a motor 40, a motor controller 54, a fluid source 44, a pump 46, a pressure sensor 48, a system controller 51, a user interface 53, and a handpiece 20 that can be operated by a dental practitioner to direct the jet 60 toward desired locations in a patient's mouth. The pump 46 can pressurize fluid received from the fluid source 44. The pump 46 may comprise a piston pump in which the piston is actuatable by the motor 40. The motor 40 can be controlled by way of the motor controller 54. The high-pressure liquid from the pump 46 can be fed to the pressure sensor 48 and then to the handpiece 20, for example, by a length of high-pressure tubing 49. The pressure sensor 48 may be used to sense the pressure of the liquid and communicate pressure information to the system controller 51. The system controller 51 can use the pressure information to make adjustments to the motor 40 and/or the pump 46 to provide a target pressure for the fluid delivered to the handpiece 20. For example, in embodiments in which the pump 46 comprises a piston pump, the system controller 51 may signal the motor 40 to drive the piston more rapidly or more slowly, depending on the pressure information from the pressure sensor 48. In some embodiments, the pressure of the liquid that can be delivered to the handpiece 20 can be adjusted within a range from about 500 psi to about 50,000 psi (1 psi is 1 pound per square inch and is about 6895 Pascal (Pa)). In certain embodiments, it has been found that a pressure range from about 2,000 psi to about 15,000 psi produces jets that are particularly effective for endodontic treatments. In some embodiments, the pressure is about 10,000 psi.
The fluid source 44 may comprise a fluid container (e.g., an intravenous bag) holding any of the treatments fluids described herein. The treatment fluid may be degassed, with a dissolved gas content less than normal (e.g., non-degassed) fluids. Examples of treatment fluids include sterile water, a medical-grade saline solution, an antiseptic or antibiotic solution (e.g., sodium hypochlorite), a solution with chemicals or medications, or any combination thereof. More than one fluid source may be used. In certain embodiments, it is advantageous for jet formation if the liquid provided by the fluid source 44 is substantially free of dissolved gases, which may reduce the effectiveness of the jet and the pressure wave generation. Therefore, in some embodiments, the fluid source 44 comprises degassed liquid such as, e.g., degassed distilled water. A bubble detector (not shown) may be disposed between the fluid source 44 and the pump 46 to detect bubbles in the liquid and/or to determine whether liquid flow from the fluid source 44 has been interrupted or the container has emptied. Also, as discussed above degassed fluids may be used. The bubble detector can be used to determine whether small air bubbles are present in the fluid that might negatively impact jet formation or acoustic wave propagation. Thus in some embodiments, a filter or de-bubbler (not shown) can be used to remove small air bubbles from the liquid. The liquid in the fluid source 44 may be at room temperature or may be heated and/or cooled to a different temperature. For example, in some embodiments, the liquid in the fluid source 44 can be chilled to reduce the temperature of the high velocity jet 60 generated by the system 38, which may reduce or control the temperature of the fluid inside a tooth 10. In some treatment methods, the liquid in the fluid source 44 can be heated, which may increase the rate of chemical reactions that may occur in the tooth 10 during treatment.
The handpiece 20 can be configured to receive the high pressure liquid and can be adapted at a distal end to generate a high-velocity beam or jet 60 of liquid for use in dental procedures. In some embodiments, the system 38 may produce a coherent, collimated jet of liquid. The handpiece 20 may be sized and shaped to be maneuverable in the mouth of a patient so that the jet 60 may be directed toward or away from various portions of the tooth 10. In some embodiments, the handpiece 20 comprises a distal housing or coupling member that can be coupled to the tooth 10.
The system controller 51 may comprise a microprocessor, a special or general purpose computer, a floating point gate array, and/or a programmable logic device. The system controller 51 may be used to control safety of the system 38, for example, by limiting system pressures to be below safety thresholds and/or by limiting the time that the jet 60 is permitted to flow from the handpiece 20. The system 38 may also include a user interface 53 that outputs relevant system data or accepts user input (e.g., a target pressure). In some embodiments, the user interface 53 comprises a touch screen graphics display. In some embodiments, the user interface 53 may include controls for a dental practitioner to operate the liquid jet apparatus. For example, the controls can include a foot switch to actuate or deactuate the jet. In some embodiments, the motor 40, motor controller 54, pump 46, fluid source 44, pressure sensor 48, system controller 51, and user interface 53 can be integrated in the console 2 illustrated schematically in Figures 1A-1B.
The system 38 may include additional and/or different components and may be configured differently than shown in Figure 3A. For example, the system 38 may include an aspiration pump that is coupled to the handpiece 20 (or an aspiration cannula) to permit aspiration of organic matter from the mouth or tooth 10. In other embodiments, the system 38 may comprise other pneumatic and/or hydraulic systems adapted to generate the high-velocity beam or jet 60.
Additional details of a pressure wave generator and/or pressure wave generator that includes a liquid jet device may be found at least in [0045]-[0050], [0054]-[0077] and various other portions of U.S. Patent Publication No. US 2011/0117517, published May 19, 2011, and in [0136]-[0142] and various other portions of U.S. Patent Publication No. US 2012/0237893, published September 20, 2012, each of which is incorporated by reference herein in its entirety and for all purposes.
As has been described, a pressure wave generator can be any physical device or phenomenon that converts one form of energy into acoustic waves within the treatment fluid and that induces rotational fluid motion in the chamber 6 and/or tooth 10. Many different types of pressure wave generators (or combinations of pressure wave generators) are usable with embodiments of the systems and methods disclosed herein.

(2) Mechanical Energy
Mechanical energy pressure wave generators can also include rotating objects, e.g. miniature propellers, eccentrically-confined rotating cylinders, a perforated rotating disk, etc. These types of pressure wave generators can also include vibrating, oscillating, or pulsating objects such as sonication devices that create pressure waves via piezoelectricity, magnetostriction, etc. In some pressure wave generators, electric energy transferred to a piezoelectric transducer can produce acoustic waves in the treatment fluid. In some cases, the piezoelectric transducer can be used to create acoustic waves having a broad band of frequencies.

(3) Electromagnetic Energy
An electromagnetic beam of radiation (e.g., a laser beam) can propagate energy into a chamber, and the electromagnetic beam energy can be transformed into acoustic waves as it enters the treatment fluid. In some embodiments, the laser beam can be directed into the chamber 6 as a collimated and coherent beam of light. The collimated laser beam can be sufficient to generate pressure waves as the laser beam delivers energy to the fluid. Furthermore, in various embodiments, the laser beam can be focused using one or more lenses or other focusing devices to concentrate the optical energy at a location in the treatment fluid. The concentrated energy can be transformed into pressure waves sufficient to clean the undesirable materials. In one embodiment, the wavelength of the laser beam or electromagnetic source can be selected to be highly absorbable by the treatment fluid in the chamber or mouth (e.g., water) and/or by the additives in the treatment fluid (e.g., nanoparticles, etc.). For example, at least some of the electromagnetic energy may be absorbed by the fluid (e.g., water) in the chamber, which can generate localized heating and pressure waves that propagate in the fluid. The pressure waves generated by the electromagnetic beam can generate photo-induced or photo-acoustic cavitation effects in the fluid. In some embodiments, the localized heating can induce rotational fluid flow in the chamber 6 and/or tooth 10 that further enhances cleaning of the tooth 10 (see, e.g., Figure 10C). The electromagnetic radiation from a radiation source (e.g., a laser) can be propagated to the chamber by an optical waveguide (e.g., an optical fiber), and dispersed into the fluid at a distal end of the waveguide (e.g., a shaped tip of the fiber, e.g., a conically-shaped tip). In other implementations, the radiation can be directed to the chamber by a beam scanning system.
The wavelength of the electromagnetic energy may be in a range that is strongly absorbed by water molecules. The wavelength may in a range from about 300 nm to about 3000 nm. In some embodiments, the wavelength is in a range from about 400 nm to about 700 nm, about 700 nm to about 1000 nm (e.g., 790 nm, 810 nm, 940 nm, or 980 nm), in a range from about 1 micron to about 3 microns (e.g., about 2.7 microns or 2.9 microns), or in a range from about 3 microns to about 30 microns (e.g., 9.4 microns or 10.6 microns). The electromagnetic energy can be in the ultraviolet, visible, near-infrared, mid-infrared, microwave, or longer wavelengths.
The electromagnetic energy can be pulsed or modulated (e.g., via a pulsed laser), for example with a repetition rate in a range from about 1 Hz to about 500 kHz. The pulse energy can be in a range from about 1 mJ to about 1000 mJ. The pulse width can be in a range from about 1 µs to about 500 µs, about 1 ms to about 500 ms, or some other range. In some cases, nanosecond pulsed lasers can be used with pulse rates in a range from about 100 ns to about 500 ns. The foregoing are non-limiting examples of radiation parameters, and other repetition rates, pulse widths, pulse energies, etc. can be used in other embodiments.
The laser can include one or more of a diode laser, a solid state laser, a fiber laser, an Er:YAG laser, an Er:YSGG laser, an Er,Cr:YAG laser, an Er,Cr:YSGG laser, a Ho:YAG laser, a Nd:YAG laser, a CTE:YAG laser, a CO_2 laser, or a Ti:Sapphire laser. In other embodiments, the source of electromagnetic radiation can include one or more light emitting diodes (LEDs). The electromagnetic radiation can be used to excite nanoparticles (e.g., light-absorbing gold nanorods or nanoshells) inside the treatment fluid, which may increase the efficiency of photo-induced cavitation in the fluid. The treatment fluid can include excitable functional groups (e.g., hydroxyl functional groups) that may be susceptible to excitation by the electromagnetic radiation and which may increase the efficiency of pressure wave generation (e.g., due to increased absorption of radiation). During some treatments, radiation having a first wavelength can be used (e.g., a wavelength strongly absorbed by the liquid, for instance water) followed by radiation having a second wavelength not equal to the first wavelength (e.g., a wavelength less strongly absorbed by water) but strongly absorbed by another element, e.g. dentin, or nanoparticles added to solution. For example, in some such treatments, the first wavelength may help create bubbles in the fluid, and the second wavelength may help disrupt the tissue.
The electromagnetic energy can be applied to the chamber 6 for a treatment time that can be in a range from about one to a few seconds up to about one minute or longer. A treatment procedure can include one to ten (or more) cycles of applying electromagnetic energy to the tooth. A fluid can circulate or otherwise move in the chamber during the treatment process, which advantageously may inhibit heating of the tooth 10 (which may cause discomfort to the patient). The movement or circulation of treatment fluid (e.g., water with a tissue dissolving agent) in the chamber 6 can bring fresh treatment fluid to tissue and organic matter as well as flush out dissolved material from the treatment site. In some treatments using electromagnetic radiation, movement of the treatment fluid can increase the effectiveness of the cleaning (as compared to a treatment with little or no fluid circulation).
In some implementations, electromagnetic energy can be added to other fluid motion generation modalities. For example, electromagnetic energy can be delivered to a chamber in which another pressure wave generator (e.g., a liquid jet) is used to generate the acoustic waves.

(4) Acoustic Energy
Acoustic energy (e.g., ultrasonic, sonic, audible, and/or lower frequencies) can be generated from electric energy transferred to, e.g., an ultrasound or other transducer or an ultrasonic tip (or file or needle) that creates acoustic waves in the treatment fluid. The ultrasonic or other type of acoustic transducer can comprise a piezoelectric crystal that physically oscillates in response to an electrical signal or a magnetostrictive element that converts electromagnetic energy into mechanical energy. The transducer can be disposed in the treatment fluid, for example, in the fluid inside the chamber. As explained herein with respect to Figures 4A-4C, for example, ultrasonic or other acoustic devices used with the embodiments disclosed herein are preferably broadband and/or multi-frequency devices. For example, unlike the power spectra of the conventional ultrasonic transducer shown in Figure 4B, ultrasonic or other acoustic devices used with the disclosed embodiments preferably have broadband characteristics similar to those of the power spectra of Figures 4A-4B (acoustic power of a liquid jet device).

(5) Further Properties of Some Pressure Wave Generators
A pressure wave generator 5 can be placed at a desired location with respect to the tooth 10. The pressure wave generator 5 creates pressure waves within the fluid 22 inside the chamber 6 (the generation of acoustic waves may or may not create or cause cavitation). The acoustic or pressure waves 23 propagate throughout the fluid 22 inside the chamber 6, with the fluid 22 in the chamber 6 serving as a propagation medium for the pressure waves 23. The pressure waves 23 can also propagate through tooth material (e.g., dentin). It is believed, although not required, that as a result of application of a sufficiently high-intensity acoustic wave, acoustic cavitation may occur. The collapse of cavitation bubbles may induce, cause, or be involved in a number of processes described herein such as, e.g., sonochemistry, tissue dissociation, tissue delamination, sonoporation, and/or removal of calcified structures. In some embodiments, the pressure wave generator can be configured such that the acoustic waves (and/or cavitation) do not substantially break down natural dentin in the tooth 110. The acoustic wave field by itself or in addition to cavitation may be involved in one or more of the abovementioned processes.
In some implementations, the pressure wave generator 5 generates primary cavitation, which creates acoustic waves, which may in turn lead to secondary cavitation. The secondary cavitation may be weaker than the primary cavitation and may be non-inertial cavitation. In other implementations, the pressure wave generator 5 generates acoustic waves directly, which may lead to secondary cavitation.
The energy source that provides the energy for the pressure wave generator 5 can be located outside the handpiece 20, inside the handpiece 20, integrated with the handpiece 20, etc.
Additional details of pressure wave generators (e.g., which may comprise a pressure wave generator) that may be suitable for use with the embodiments disclosed herein may be found, e.g., in [0191]-[0217], and various other portions of U.S. Patent Publication No. US 2012/0237893, published September 20, 2012, which is incorporated by reference herein for all purposes.
Other pressure wave generators may be suitable for use with the disclosed embodiments. For example, a fluid inlet can be disposed at a distal portion of a handpiece and/or can be coupled to a fluid platform in some arrangements. The fluid inlet can be configured to create movement of the fluid in a chamber 6, turbulence in the fluid in the chamber, fluid motion 24 of the fluid 22 in the chamber 6 and/or produce other dynamics in the fluid in the chamber 6r. For example, the fluid inlet can inject fluid into or on the tooth to be treated. In addition, mechanical stirrers and other devices can be used to enhance fluid motion and cleaning. The fluid inlet can improve the circulation of the treatment fluid in a chamber, which can enhance the removal of unhealthy materials from the tooth 10. For example, as explained herein, faster mechanisms of reactant delivery such as "macroscopic" liquid circulation may be advantageous in some of the embodiments disclosed herein.
In some embodiments, multiple pressure wave generators can be disposed in or on the chamber 6. As explained herein, each of the multiple pressure wave generators can be configured to propagate acoustic waves at a different frequency or range of frequencies. For example, different acoustic frequencies can be used to remove different types of materials. The multiple pressure wave generators can be activated simultaneously and/or sequentially in various arrangements.

B. Coupling Members
The coupling members 3 disclosed herein can be adapted to couple or orient the pressure wave generator 5 relative to the tooth 10. In some embodiments disclosed herein, the coupling member 3 can be configured to retain fluid 22 in a treatment chamber 6. In some embodiments, the coupling member 3 can be coupled to or formed with a distal portion 21 of the handpiece 20. The coupling member 3 can include or define the chamber 6 configured to retain fluid 22. Liquid can be introduced into the chamber 6 through a fluid inlet connected to, or disposed in or on, the handpiece 20. Waste treatment liquid can be removed through the coupling member 3 by way of a fluid outlet and further into the handpiece 20. In various arrangements, the coupling member 3 may be configured to cover a portion of a tooth, a whole surface of the tooth, and/or multiple teeth.
In some embodiments, the coupling member 3 can be applied to the tooth 10 with a mechanical clasp or clamp, a dental adhesive, or by pressure applied by the patient by biting on the coupling member 3. In still other embodiments, a separate cap or fluid retainer can be removably coupled to the distal portion 21 of the handpiece 20.
Additional details of coupling members 3 may be similar to those of fluid retainers, flow restrictors or caps disclosed, e.g., in [0052]-[0053], [0115]-[0117] and various other portions of U.S. Patent Publication No. US 2011/0117517, published May 19, 2011, and in [0040]-[0043], [0170]-[01 [0293]-[0299], [0316]-[0319] and various other portions of U.S. Patent Publication No. US 2012/0237893, published September 20, 2012, each of which is incorporated by reference herein for all purposes.
The coupling member 3 can also include various components that enhance aspiration and irrigation before, during, and/or after the treatment procedure. In some embodiments, fluid 22 can enter the chamber 6 via a fluid inlet, such as a treatment liquid inflow conduit. The fluid inlet can pass through or along the handpiece 20. Under steady state operation, the amount of liquid entering the at least partially enclosed chamber 6 can be substantially the same as the amount of liquid leaving chamber 6 through the fluid outlet. In some embodiments, the fluid inlet can be driven by a pump, which can be controlled by the console 2. Furthermore, the fluid inlet can be the same as the pressure wave generator 5 in some embodiments, such as in embodiments that employ a liquid jet device. Additional details of fluid inlets that may be suitable for use with the embodiments disclosed herein may be found, e.g., in [0075]-[0078] and various other portions of U.S. Patent Publication No. US 2012/0237893, published September 20, 2012, which is incorporated by reference herein for all purposes.
As explained above, the coupling member 3 can also have a fluid outlet, e.g., an outflow conduit to transfer liquid out of the chamber 6 during the procedure. In some embodiments, waste treatment liquid may be allowed to spill directly into the patient's mouth. In other embodiments, however, waste treatment liquid (as well as removed material and byproduct gases) can be transferred through the fluid outlet, which can pass through or along the handpiece 20. The fluid outlet can be active or passive. In the case of a passive fluid outlet, the waste treatment liquid may move through the fluid outlet due to capillary forces, gravity, or because of a slight overpressure created in the enclosed chamber 6. In the case of an actively pumped fluid outlet, the waste liquid can be transferred using a pump, suction, or other device that draws liquid out through the outlet. In one example, the fluid outlet is connected to the suction system and/or vacuum lines in the clinician's office. For example, in some embodiments, the inlet and outlet can be adjusted to maintain a balanced amount of fluid in coupling member 3. Additional details of fluid outlets that may be suitable for use with the embodiments disclosed herein may be found, e.g., in [0079]-[0081] and various other portions of U.S. Patent Publication No. US 2012/0237893, published September 20, 2012, which is incorporated by reference herein for all purposes.
As explained herein, the coupling member 3 can also include one or more vents to regulate pressure of the fluid 22. The vents can be disposed in a portion of the handpiece 20 in some arrangements, such as along a waste line or fluid outlet. The vents can take the form of a permeable or semi-permeable material (e.g., a sponge), openings, pores, or holes, etc. Additional details of vents that may be suitable for use with the embodiments disclosed herein may be found, e.g., in [0071]-[0073], [0082]-[0086], [0177]-[0194] and various other portions of U.S. Patent Publication No. US 2012/0237893, published September 20, 2012, which is incorporated by reference herein for all purposes.

C. Handpiece
The systems disclosed herein can include a handpiece 20. The handpiece 20 can be configured to apply the coupling member 3 to the tooth 10 and/or to position the pressure wave generator 5 relative to the treatment site. Treatment liquids can be transferred into and out of the chamber 6 by way of the handpiece 20.
The handpiece 20 can provide the operator, user or clinician with a handheld device to hold during the procedure. For example, the handpiece 20 can include user-friendly grips and a user-friendly shape to grasp. The clinician can manipulate the handpiece 20 to accurately position the coupling member 3 and/or pressure wave generator 5 at a desired position on the tooth 10. In addition, the handpiece 20 can allow the clinician to move or rotate the coupling member 3 and pressure wave generator 5 during the procedure so as to dispose the pressure wave generator 5 at a desirable position relative to the treatment region in the tooth 10. Alternatively, the handpiece 20 can also provide a device for the operator to clamp or attach to the tooth 10 such that the handpiece 20 does not require substantial user intervention during the procedure. The handpiece 20 can be disposable (e.g., single-use), or the handpiece 20 can be reusable. In one embodiment, the handpiece 20 is disposable, but the pressure wave generator 5 is reusable. The handpiece 20 can be formed of any suitable material. In some embodiments, the handpiece 20 can be formed of a plastic material. In other embodiments, the handpiece 20 can be formed of a metal. Additional details of handpieces that may be suitable for use with the embodiments disclosed herein may be found, e.g., in [0107], [0138]-[0142], [0156]-[0161] and various other portions of U.S. Patent Publication No. US 2012/0237893, published September 20, 2012, which is incorporated by reference herein for all purposes.
For example, Figure 3B is a schematic side view illustrating an embodiment of a handpiece 20 comprising an embodiment of a guide tube 27 for delivery of a liquid jet to a portion of a tooth 10. The handpiece 20 comprises an elongated tubular barrel 29 having a proximal end 31 that is adapted to engage tubing 32 from the system 38 and a distal end 21 adapted to be coupled or attached to the tooth 10. The barrel 29 may include features or textures 28 that enhance grasping the handpiece 20 with the fingers and thumb of the operator. The handpiece 20 can be configured to be handheld. In some cases, the handpiece 20 can be configured to be portable, movable, orientable, or maneuverable with respect to the patient. In some implementations, the handpiece 20 can be configured to be coupled to a positioning device (e.g., a maneuverable or adjustable arm). The distal end 21 of the handpiece 20 can comprise the coupling member 3 that can be coupled to the tooth 10.
The handpiece 20 may include a fluid inlet for delivering fluid 22 to the chamber 6, a fluid outlet for removing fluid from the tooth 10 (e.g., waste fluid), a pressure wave generator 5, a power line (e.g., to provide energy to a pressure wave generator), or a combination of some or all of the foregoing. The handpiece 20 may include other components such as, e.g., an irrigation line to irrigate the tooth area, a light source to illuminate the tooth area, etc. In some cases, the pressure wave generator 5 (e.g., a liquid jet) comprises the fluid inlet (e.g., the jet). The handpiece 20 can be used to apply the pressure wave generator 5 relative to the tooth 10. The handpiece 20 can be applied to the tooth 10 so as to create a substantially closed fluid circuit as the distal end 21 of the handpiece 20 engages the tooth 10, thereby enabling fluid to be delivered into and out of the chamber 6 without substantial spillage or leakage into the patient's mouth. As described herein, the handpiece 20 and/or the coupling member 3 may include a fluid retention member (e.g., sponge or vent) to reduce the likelihood of fluid leakage and/or to allow fluid to flow from the chamber 6 (e.g., to inhibit overpressurization or under-pressurization). The fluid retention member can be configured to inhibit air from entering the chamber 6 and tooth 10 (which may reduce the effectiveness of cavitation) while permitting air to enter a fluid outlet (e.g., suction line).

D. Tooth Seal and Alignment Features
A tooth seal 26 disclosed herein can be configured to temporarily secure the coupling member 3 to the tooth 10. The tooth seal 26 can be configured to flow onto or near an occlusal surface of the tooth in a flowable state. The tooth seal 26 can be configured to set and/or harden to hold its shape during treatment. In addition, the tooth seal 26 can be easily removed or pulled from the tooth 10 after use. In some arrangements, the sealing material can easily be reshaped using tools such as a dental bur, knife, etc. For example, in various embodiments, the sealing material can be shaped (e.g., planarized or curved) to support a planar coupling surface (e.g., a washer, one or more support magnets, etc.). The coupling member 3 and/or handpiece 3 can couple to the coupling surface, and the pressure wave generator 5 (e.g., a liquid jet device) can extend through the coupling surface such that a distal end portion 25 of the pressure wave generator 5 is disposed in the chamber 6 of the coupling member 3.
The tooth seal 26 can comprise any suitable sealant. For example, the tooth seal 26 can be a substantially semi-flexible material that can set or harden in less than about 30 seconds. The tooth seal 26 can be any suitable material that is able to seal the coupling member 3 to the tooth 10, but that also can easily be removed from the tooth 10. Examples of suitable sealing materials can include silicones, impression materials, bite registration materials, etc. In some embodiments, for example, the sealing materials can include 3M Imprint™ Bite, Jet Blue Bite by Colténe Whaledent®, LuxaBite bite registration material by DMG America, Alpha-Dam™ LC Gingival Dam Material or any other suitable sealant. In other embodiments, however, the tooth seal may not be used.
In some embodiments, the tooth seal 26 can comprise a permeable or semi-permeable material, such that waste fluid can flow from within the tooth 10 and/or chamber 6 thorugh the tooth seal 6 and outside the tooth 10. In various embodiments, the tooth seal 26 can comprise a peripheral boundary shaped to secure the chamber 6 and/or coupling member 3 to the tooth seal 26. For example, in some embodiments, the tooth seal 26 can comprise a locking wall extending upwardly relative to the tooth. The locking wall can be shaped to laterally restrain the coupling member 3 during treatment. In some embodiments, a mating tube can extending outwardly from the chamber 6 and can surround an access port of the chamber 6. The mating tube can be positioned within the access opening 18 of the tooth 10 to substantially align the coupling member 3 and pressure wave generator 5 with the treatment region of the tooth 10.
In various embodiments, the tooth seal 26 can be shaped to permit the user to rotate the coupling member 3 relative to the tooth 10 to position the pressure wave generator 5 and coupling member 3 at a desired orientation relative to the treatment region of the tooth 10. For example, the tooth seal 26 can comprise a concave surface, and the distal end portion 21 of the handpiece 20 can be pressed against and/or coupled to the concave surface. The curved distal end portion 21 of the handpiece 20 can have a shape complementary to that of the curved tooth seal 26.

III. Examples of Power Generated by Pressure wave generators
Figures 4A and 4B are graphs that schematically illustrate possible examples of power that can be generated by different embodiments of the pressure wave generator 5. These graphs schematically show acoustic power (in arbitrary units) on the vertical axis as a function of acoustic frequency (in kHz) on the horizontal axis. The acoustic power in the tooth may influence, cause, or increase the strength of effects including, e.g., acoustic cavitation (e.g., cavitation bubble formation and collapse, microjet formation), acoustic streaming, microerosion, fluid agitation, fluid circulation and/or rotational motion, sonoporation, sonochemistry, and so forth, which may act to dissociate organic material in or on the tooth and effectively clean the undesirable materials, e.g., undesirable organic and/or inorganic materials and deposits. In some embodiments, these effects can enhance or enable the obturation or filling of treated root canals or other treatment regions of the tooth, For example, the embodiments disclosed herein can advantageously obturate or fill substantially the entire canal(s) and/or branch structures therefrom, as explained in greater detail above. In various embodiments, the pressure wave generator can produce a pressure wave including acoustic power (at least) at frequencies above: about 1 Hz, about 0.5 kHz, about 1 kHz, about 10 kHz, about 20 kHz, about 50 kHz, about 100 kHz, or greater. The pressure wave can have acoustic power at other frequencies as well (e.g., at frequencies below the aforelisted frequencies).
The graph in Figure 4A represents a schematic example of acoustic power generated by a liquid jet impacting a surface disposed within a chamber on or around the tooth that is substantially filled with liquid and by the interaction of the liquid jet with fluid in the chamber. This schematic example shows a broadband spectrum 190 of acoustic power with significant power extending from about 1Hz to about 1000 kHz, including, e.g., significant power in a range of about 1 kHz to about 1000 kHz (e.g., the bandwidth can be about 1000 kHz). The bandwidth of the acoustic energy spectrum may, in some cases, be measured in terms of the 3-decibel (3-dB) bandwidth (e.g., the full-width at half-maximum or FWHM of the acoustic power spectrum). In various examples, a broadband acoustic power spectrum can include significant power in a bandwidth in a range from about 1 Hz to about 500 kHz, in a range from about 1 kHz to about 500 kHz, in a range from about 10 kHz to about 100 kHz, or some other range of frequencies. In some implementations, a broadband spectrum can include acoustic power above about 1 MHz. In some embodiments, the pressure wave generator can produce broadband acoustic power with peak power at about 10 kHz and a bandwidth of about 100 kHz. In various embodiments, the bandwidth of a broadband acoustic power spectrum is greater than about 10 kHz, greater than about 50 kHz, greater than about 100 kHz, greater than about 250 kHz, greater than about 500 kHz, greater than about 1 MHz, or some other value. In some cleaning methods, acoustic power between about 1 Hz and about 200 kHz, e.g., in a range of about 20 kHz to about 200 kHz may be particularly effective at cleaning teeth. The acoustic power can have substantial power at frequencies greater than about 1 kHz, greater than about 10 kHz, greater than about 100 kHz, or greater than about 500 kHz. Substantial power can include, for example, an amount of power that is greater than 10%, greater than 25%, greater than 35%, or greater than 50% of the total acoustic power (e.g., the acoustic power integrated over all frequencies). In some arrangements, the broadband spectrum 190 can include one or more peaks, e.g., peaks in the audible, ultrasonic, and/or megasonic frequency ranges.
The graph in Figure 4B represents a schematic example of acoustic power generated by an ultrasonic transducer disposed in a chamber on or around the tooth that is substantially filled with liquid. This schematic example shows a relatively narrowband spectrum 192 of acoustic power with a highest peak 192a near the fundamental frequency of about 30 kHz and also shows peaks 192b near the first few harmonic frequencies. The bandwidth of the acoustic power near the peak may be about 5 to 10 kHz, and can be seen to be much narrower than the bandwidth of the acoustic power schematically illustrated in Figure 4A. In other embodiments, the bandwidth of the acoustic power can be about 1 kHz, about 5 kHz, about 10 kHz, about 20 kHz, about 50 kHz, about 100 kHz, or some other value. The acoustic power of the example spectrum 192 has most of its power at the fundamental frequency and first few harmonics, and therefore the ultrasonic transducer of this example may provide acoustic power at a relatively narrow range of frequencies (e.g., near the fundamental and harmonic frequencies). The acoustic power of the example spectrum 190 exhibits relatively broadband power (with a relatively high bandwidth compared to the spectrum 192), and the example liquid jet can provide acoustic power at significantly more frequencies than the example ultrasonic transducer. For example, the relatively broadband power of the example spectrum 190 illustrates that the example jet device provides acoustic power at these multiple frequencies with energy sufficient to break the bonds between the decayed and healthy material so as to substantially remove the decayed material from the carious region.
It is believed, although not required, that pressure waves having broadband acoustic power (see, e.g., the example shown in Figure 4A) can generate acoustic cavitation or other means of cleaning and disinfection that is more effective at cleaning teeth (including cleaning, e.g., unhealthy materials in or on the tooth) than cavitation generated by pressure waves having a narrowband acoustic power spectrum (see, e.g., the example shown in Figure 4B). Further, broadband acoustic power can also generate sufficient energy at frequencies capable of obturating or filling a root canal or other treatment region (such as a treated carious region on an exterior surface of the tooth). For example, a broadband spectrum of acoustic power can produce a relatively broad range of bubble sizes in the cavitation cloud and on the surfaces on the tooth, and the implosion of these bubbles may be more effective at disrupting tissue than bubbles having a narrow size range. Relatively broadband acoustic power may also allow acoustic energy to work on a range of length scales, e.g., from the cellular scale up to the tissue scale. Accordingly, pressure wave generators that produce a broadband acoustic power spectrum (e.g., some embodiments of a liquid jet) can be more effective at tooth cleaning for some treatments than pressure wave generators that produce a narrowband acoustic power spectrum. In some embodiments, multiple narrowband pressure wave generators can be used to produce a relatively broad range of acoustic power. For example, multiple ultrasonic tips, each tuned to produce acoustic power at a different peak frequency, can be used. As used herein, broadband frequencies and broadband frequency spectrum is defined regardless of secondary effects such as harmonics of the main frequencies and regardless of any noise introduced by measurement or data processing (e.g., FFT); that is, these terms should be understood when only considering all main frequencies activated by the pressure wave generator.
Figure 4C is a graph of an acoustic power spectrum 1445 generated at multiple frequencies by the pressure wave generators disclosed herein. For example, the spectrum 1445 in Figure 4C is an example of acoustic power generated by a liquid jet impacting a surface disposed within a chamber on, in, or around the tooth that is substantially filled with liquid and by the interaction of the liquid jet with fluid in the chamber. The spectrum 1445 of Figure 4C represents acoustic power detected by a sensor spaced apart from the source of the acoustic energy, e.g., the pressure wave generator. The data was acquired inside an insulated water tank data when the distance between the power wave generator and the hydrophone (e.g., sensor) being about 8 inches. The vertical axis of the plot represents a measure of acoustic power: Log (P_{acoustic}^2), referred to herein as "power units". The units of P_{acoustic} in the measurement were µPa (micro Pascal). Thus, it should be appreciated that the actual power at the source may be of a different magnitude because the sensor is spaced from the acoustic power generator. However, the general profile of the power spectrum at the source should be the same as the spectrum 1445 detected at the sensor and plotted in Figure 4C. It should also be understood that, although the plot shows frequencies only up to 100 KHz, the power above 100 KHz was greater than zero - the data just was not plotted. It should further be noted that, as would be appreciated by one skilled in the art, the plot and the values would also depend on other parameters, such as, for example, the size and shape of the tank in which data was acquired, the insulation of the inner surface of the tank, the relative distance between the source (e.g., power wave generator), and the free water surface of the tank.
As shown in Figure 4C, the spectrum 1445 can include acoustic power at multiple frequencies 1447, e.g., multiple discrete frequencies. In particular, the spectrum 1445 illustrated in Figure 4C includes acoustic power at frequencies in a range of about 1 Hz to about 100 KHz. The acoustic power can be in a range of about 10 power units to about 80 power units at these frequencies. In some arrangements, the acoustic power can be in a range of about 30 power units to about 75 power units at frequencies in a range of about 1 Hz to about 10 kHz. In some arrangements, the acoustic power can be in a range of about 10 power units to about 30 power units at frequencies in a range of about 1 KHz to about 100 kHz. In some embodiments, for example, the broadband frequency range of the pressure waves generated by the pressure wave generators disclosed herein can comprise a substantially white noise distribution of frequencies (see, e.g., Figure 11B and associated disclosure).
Pressure wave generators that generate acoustic power associated with the spectrum 1445 of Figure 4C can advantageously and surprisingly clean undesirable materials from teeth. As explained above, the generation of power at multiple frequencies can help to remove various types of organic and/or inorganic materials that have different material or physical characteristics, and/or different bonding strengths at various frequencies. For example, some undesirable materials may be removed from the teeth and/or gums at relatively low acoustic frequencies, while other materials may be removed from the teeth at relatively high acoustic frequencies, while still other materials may be removed at intermediate frequencies between the relatively low and relatively high frequencies. As shown in Figure 4C, lower frequency cleaning phases can be activated at higher powers, and higher frequency cleaning phases can be activated at lower powers. In other embodiments, low frequency cleaning phases may be activated at relatively low powers, and high frequency cleaning phases may be activated at relatively high powers. Pressure wave generators that generate acoustic power at multiple frequencies (e.g., multiple discrete frequencies) are capable of cleaning undesirable materials and decayed matter from interior and/or exterior portions of teeth.
In the embodiments disclosed herein, treatment procedures can be activated to generate acoustic power at various frequency ranges. For example, some treatment phases may be activated at lower frequencies, and other treatment phases may be activated at higher frequencies. The pressure wave generators disclosed herein can be adapted to controllably generate acoustic power at any suitable frequencies 1447 of the spectrum 1445. For example, the pressure wave generators disclosed herein can be adapted to generate power at multiple frequencies 1447 simultaneously, e.g., such that the delivered acoustic power in a particular treatment procedure can include a desired combination of individual frequencies. For example, in some procedures, power may be generated across the entire frequency spectrum 1445. In some treatment phases, the pressure wave generator can deliver acoustic power at only relatively low frequencies, and in other treatment phases, the pressure wave generator can deliver power at only relatively high frequencies, as explained herein. Further, depending on the desired treatment procedure, the pressure wave generator can automatically or manually transition between frequencies 1447 according to a desired pattern, or can transition between frequencies 1447 randomly. In some arrangements, relatively low frequencies can be associated with large-scale bulk fluid movement, and relatively high frequencies can be associated with small-scale, high-energy oscillations.
In some embodiments, the treatment procedure may include one or more treatment phases. In each treatment phase, energy can be applied at a different frequency or band of frequencies. For example, in one phase, energy (e.g., pressure or acoustic waves) propagating at a relatively low frequency (or band of frequencies) may be generated. The low frequency pressure waves can interact with the treatment fluid in the chamber and can induce removal of large-scale dental deposits or materials. Without being limited by theory, the low frequency pressure waves can remove a substantial portion of the unhealthy materials in the tooth. For example, the low frequency waves may have a sufficiently high energy at suitably low frequencies to remove large deposits or materials from the tooth. The acoustic power at the relatively low frequencies can include acoustic power at any suitable low-frequency band of the power spectrum of the pressure wave generator (see, e.g., Figure 4A). For example, in some embodiments, the acoustic power in the first, low-frequency range can include one or more frequencies in a range of about 0.1 Hz to about 100 Hz, for example in a range of about 1 Hz to about 50 Hz in some arrangements.
In another phase, acoustic energy may be generated at relatively high frequencies. At higher frequencies, the pressure wave generator can be configured to remove smaller deposits and debris. For example, at higher frequencies, the pressure waves can propagate through the treatment fluid. The higher frequency waves can remove smaller portions from relatively small locations, such as crevices, cracks, spaces, and irregular surfaces of the tooth. In some embodiments, degassed liquid can be used to enhance the removal of matter from these small spaces. When the higher frequency cleaning is performed after the lower frequency cleaning, in some embodiments, the high frequency waves (and/or intermediate frequency waves) can clean the remainder of the unhealthy material left behind from the low frequency cleaning. In the relatively high frequency phases, acoustic energy can be generated in a range of about 10 kHz to about 1000 kHz, e.g., in a range of about 100 kHz to about 500 kHz.
In some embodiments, the treatment procedure can progress from the relatively low frequencies (or bands of frequencies) toward higher frequencies (or bands of frequencies). For example, the procedure can move from the relatively low frequency phase(s), through intermediate frequency phase(s), until the high frequency phase(s) are reached. Thus, in some embodiments, the treatment procedure can provide a gradual and/or substantially continuous transition between relatively low and relatively high frequencies. As the treatment progresses through the frequencies, unhealthy dental deposits or materials of varying size and type can be removed by the pressure wave generator. In other embodiments, however, the treatment procedure can transition or switch between frequencies (or bands of frequencies) or phases (e.g., between high, low and/or intermediate frequencies or bands of frequencies) at discrete levels. At various intermediate frequency ranges, acoustic energy can be generated in a range of about 100 Hz to about 10 kHz. For example, in some embodiments, the various phases of the treatment procedures described above may be activated by the user or clinician, or the pressure wave generator can be configured to automatically transition between the phases. In some embodiments, for example, the pressure wave generator can randomly switch between high, low, and intermediate frequencies.
Various treatment procedures may include any suitable number of treatment phases at various different frequencies. Furthermore, although various low- and high-frequency phases may be described above as occurring in a particular order, in other embodiments, the order of activating the low- and high-frequency phases, and/or any intermediate frequency phases, may be any suitable order. Furthermore, the treatment procedures and phases described herein can also be used to fill or obturate treatment regions of a tooth after cleaning. In obturation procedures, the embodiments disclosed herein can advantageously obturate or fill substantially the entire canal(s) and/or branch structures therefrom, as explained in greater detail herein.

IV. Examples of Coupling Members
Figure 5 is a schematic cross-sectional side view of a coupling member 3 having a fluid inlet 61 passing therethrough. In Figure 5, the coupling member 3 comprises a distal portion 21 of a handpiece 20. A pressure wave generator 5 can be coupled to or integrally formed with the coupling member 3. As shown in Figure 5, the pressure wave generator 5 can be disposed inside a chamber 6 of the coupling member 3 and outside the tooth 10. The coupling member 3 can be applied over an access opening 18 of the tooth 10. For example, a tooth seal 26 can be applied in flowable form over a top (e.g., occlusal) surface of the tooth 10 to provide a stable coupling surface to which the coupling member 3 can be secured. In some embodiments, the tooth seal 26 can be hardened to form a substantially solid material.
Once the coupling member 3 is secured to the tooth 10, the chamber 6 of the coupling member 3 can be at least partially, and in some arrangements substantially, filled with a suitable fluid 22. For example, as explained above, a treatment fluid can be used in cleaning treatments. An obturation material can be used in filling or obturation procedures. The fluid inlet 61 can comprise a hole or port in fluid communication with a fluid inlet line passing through or along the handpiece 20. Fluid 22 can be supplied actively (e.g., by way of a pump) or passively (e.g., by way of gravity or other potential flow) from the console 2 through the inlet line of the handpiece 20 and into the chamber 6. The pulp cavity 11 and/or chamber 6 of the coupling member 3 can be substantially filled with the fluid 22. For example, a controller in the console 2 can controllably direct the fluid 22 into the chamber 6 through the fluid inlet 61.
During a treatment procedure, the pressure wave generator 6 can be activated to generate sufficient fluid motion 24 and/or pressure waves 23 to clean unhealthy materials from the tooth 10, e.g., from the pulp cavity 11 and root canal 13. The fluid motion 24 can act to detach or break up the undesirable materials in the tooth 10, and can remove the materials from the tooth 10. For example, the fluid motion 24 can remove large particles or deposits of diseased tissue in some arrangements. The fluid motion 24 can also act to replenish chemical reactants supplied with the fluid 22. The pressure waves 23 can propagate through the fluid 22 and tooth to enhance the reactivity of the fluid 22 with the unhealthy materials in the tooth 10. For example, the pressure waves 23 can induce acoustic cavitation and other fluidic effects described herein that can enable the removal of unhealthy or undesirable materials from small spaces in the tooth 10, such as tubules, cracks, crevices, etc. The pressure wave generator 5 of Figure 5 can be any suitable pressure wave generator disclosed herein, such as, a liquid jet device. In other embodiments, as explained above, the pressure wave generator 5 can also be used to fill or obturate the root canal 13. In such arrangements, the fluid 22 can comprise a flowable obturation material. The embodiments disclosed herein can advantageously obturate or fill substantially the entire canal(s) and/or branch structures therefrom, as explained in greater detail herein.
The tooth seal 26 can comprise a fluid-permeable material in the embodiment of Figure 5. For example, the tooth seal 26 can include pores or other spaces through which waste fluid can flow. Accordingly, during a treatment procedure, fluid 22 can enter the tooth 10 and chamber 6 by way of the fluid inlet 61, and waste fluid can exit the tooth 10 and/or chamber 6 by way of the permeable tooth seal 26.
Figure 6 is a schematic cross-sectional side view of a coupling member 3 having a fluid inlet 61 and a fluid outlet 62 passing therethrough. As with Figure 5, a pressure wave generator 5 can be coupled to or integrally formed with the coupling member 3, and can be disposed in the chamber 6 of the coupling member 3. As explained herein, the pressure wave generator 5 can be used to clean and/or fill a tooth 10. Furthermore, as with the embodiment of Figure 5, the fluid inlet 61 can be formed through the handpiece 20 and coupling member 3 to supply fluid 22 to the chamber 6 and the tooth 10. As above, the pressure wave generator 5 can be activated to induce pressure waves 23 and fluid motion 24 to clean unhealthy materials from the tooth 10. The pressure wave generator 5 of Figure 6 can be any suitable pressure wave generator disclosed herein, such as, a liquid jet device.
In addition, a fluid outlet 62 can be disposed through the handpiece 20 to convey fluid out of the tooth 10 and chamber 6. For example, the fluid outlet 62 can act as a waste line, in which waste fluid can be expelled from the chamber 6 and tooth 10. The fluid outlet 62 can be incorporated to allow waste liquid to exit the chamber 6 into a hose which can be connected to a collection canister or a drain. The fluid outlet 62 can be an active or passive outlet. For a passive fluid outlet 62, in some cases the waste treatment liquid moves through a conduit due to capillary forces, gravity, or because of a slight overpressure created in the enclosed volume. For an actively pumped fluid outlet 62, the waste liquid can be transferred using a pump, suction, or other device that draws liquid out through an outflow conduit. In some arrangements, for example, the fluid outlet 62 can be connected to the suction system and/or vacuum lines in the clinician's office. In the embodiment of Figure 6, the tooth seal 26 may or may not be permeable to fluid.
Accordingly, the embodiment disclosed in Figure 6 can include both the inlet port 61 and the outlet port 62, which can balance the amount of fluid 22 in the tooth 10 at a given time. For example, the console 2 can be programmed such that the amount of fluid entering the tooth 10 and/or chamber 6 through the inlet port 61 is substantially the same as the amount of fluid exiting the tooth 10 and/or chamber 6 through the outlet port 62.
Figure 7A is a schematic cross-sectional side view of a coupling member 3 having a fluid inlet 61, a fluid outlet 62, and a vent 63 configured to regulate a pressure inside the chamber 6 and/or tooth 10. As with the embodiments of Figures 6A and 6B, the coupling member 3 can be coupled to or formed with a pressure wave generator 5 adapted to clean and/or fill a tooth 10. The coupling member 3 can be part of the distal end portion 21 of the handpiece 20. The coupling member 3 can couple to the tooth by way of the tooth seal 26.
The pressure wave generator 5 can be disposed inside the chamber 6 outside the tooth 10. The pressure wave generator 5 of Figure 7A can be any suitable pressure wave generator disclosed herein, such as, a liquid jet device. Fluid 22 can be supplied to the tooth 10 and chamber 6 by way of the fluid inlet 61. For example, the fluid 22 can substantially fill the chamber 6. The pressure wave generator 5 can be activated to clean unhealthy material from the tooth 10. For example, as explained herein, the pressure wave generator 5 can generate pressure waves 23 and fluid motion 24 sufficient to clean and/or fill the tooth 10.
As shown in Figure 7A, one or more vents 63 can be provided or formed in the coupling member 3 and/or the distal end portion 21 of the handpiece 20. The vent(s) 63 can act to at least partially regulate pressure of the fluid 22 inside the chamber 6 of the coupling member 3. For example, the vent(s) 63 can be disposed along the fluid outlet 62 (e.g., waste line). The vent 63 can fluidly communicate with the exterior environs, and air from the exterior environs can be entrained with the fluid outlet line 62.
In some vented arrangements, the inlet and outlet flow rates can be driven by independent driving forces. For example, in some implementations, the fluid inlet 61 can be in fluid communication with and driven by a pressure pump, while the fluid outlet 62 can be in fluid communication with and controlled via an evacuation system (e.g., a suction or vacuum pump). In other implementations, the fluid inlet 61 or outlet 62 can be controlled with a syringe pump. The pressures of the fluid inlet 61 and the fluid outlet 62 can be such that a negative net pressure is maintained in the chamber 6. Such a net negative pressure can assist delivering the treatment fluid into the chamber 6 from the fluid inlet 61.
In various embodiments described herein, the vents 63 can take the form of a permeable or semi-permeable material (e.g., a sponge), openings, pores, or holes, etc. The use of vents in a controlled fluid system can lead to one or more desirable advantages. For example, the evacuation system can collect waste fluid from the chamber 6, as long as there is any available. If there is a pause in treatment (e.g. the time between treatment cycles), waste fluid flow may stop, and the evacuation system may start drawing air through the one or more vents 63 to at least partially compensate for the lack of fluid supplied to the evacuation system, rather than depressurizing the chamber 6. If the evacuation system stops working for any reason, the waste fluid may flow out through the one or more vents 63 into the patient's mouth or onto a rubber dam (if used), where it can be collected by an external evacuation line. Therefore, the use of vent(s) can tend to dampen the effects of the applied pressure differential, and therefore can inhibit or prevent negative or positive pressure buildup. Also note that positive or negative pressure inside the chamber 6 can exert some amount of force on the sealing material(s), and as such a stronger seal may be required to withstand such force in some cases. Possible advantages of some vented systems include that the vent(s) help relieve pressure increases (or decreases) inside the chamber 6, reduce or eliminate the forces acting on the tooth seal 26, and therefore render the sealing more feasible and effective.
Figure 7B is a schematic cross-sectional side view of a plurality of pressure wave generators 5A, 5B, 5C coupled with a coupling member 3. As with the embodiments of Figures 5-7A, the pressure wave generators 5A, 5B, 5C can be disposed in the chamber 6 of the coupling member 3 outside the tooth 10. For example, the pressure wave generators 5A, 5B, 5C can be coupled to walls of the coupling member 3. The pressure wave generators 5A, 5B, 5C of Figure 7B can be any suitable pressure wave generator disclosed herein, such as a liquid jet device. In some embodiments, at least one of the pressure wave generators 5A, 5B, 5C can comprise an acoustic energy source. The pressure wave generators 5A, 5B, 5C can be the same type of pressure wave generator, or they can be different types of pressure wave generators. Although three pressure wave generators 5A, 5B, 5C are shown in Figure 7B, it should be appreciated that there could be any suitable number of pressure wave generators, such as one, two, four, five, or more.
As above, the coupling member 3 can be coupled to the tooth 10 by way of the tooth seal 26. Fluid 22 can be supplied to the chamber 6 by way of the fluid inlet 61. For example, the fluid 22 can substantially fill the chamber 6. The fluid outlet 62 can convey waste fluid out of the tooth 10 and the chamber 6. Although not illustrated in Figure 7B, one or more vents can also be provided to regulate the pressure in the chamber 6 and tooth 10.
During a treatment procedure, the pressure wave generators 5A, 5B, 5C can be activated sequentially or simultaneously. Advantageously, in some embodiments, the pressure wave generators 5A, 5B, 5C can be configured to generate corresponding pressure waves 23A, 23B, and 23C having different frequencies and/or powers. For example, the pressure wave generator 5A can generate a corresponding pressure wave 23A having a first frequency or a first range of frequencies. The pressure wave generator 5B can generate a corresponding pressure wave 23B having a second frequency or a second range of frequencies different form the first frequency or first range. The pressure wave generator 5C can generate a corresponding pressure wave 23C having a third frequency or a third range of frequencies that are different from the first and second frequencies/ranges. In some embodiments, the frequency ranges may overlap. In still other embodiments, the frequencies and ranges of frequencies can be about the same. For example, in some embodiments, each pressure wave generator 5A, 5B, 5C can generate pressure waves 23A, 23B, 23C across the full spectrum illustrated in Figures 4A or 4C.
As explained herein, different frequencies of pressure waves may be effective at detaching or disrupting different types of tissue. For example, some frequencies may be more effective at detaching relatively large portions of unhealthy material from the tooth 10, and other frequencies may be more effective at detaching relatively small portions of unhealthy material from the tooth 10. Still other frequencies may be particularly effective at detaching intermediate sized portions from the tooth 10. In some embodiments, the acoustic frequencies that are effective at detaching material from the tooth 10 may be related to the composition of unhealthy material to be removed. For example, some frequencies may be more effective at removing diseased pulp tissue, while other frequencies may be more effective at removing calcified deposits. Still other frequencies may be effective at removing bacteria, biofilms, caries, plaque, calculus, etc.
To completely clean the tooth 10, it can be desirable to remove all types of unhealthy or undesirable materials from the tooth 10. For example, it can be desirable to remove organic and inorganic tissue from the root canal 13, in addition to bacteria, biofilms, and portions of the smear layer (if applicable). For exterior surfaces or portions of the tooth 10, it can be desirable to remove carious regions, in addition to dental deposits such as plaque, calculus, etc. Accordingly, during a treatment procedure, it can be desirable to propagate pressure waves 23A, 23B, 23C across the full range of frequencies that correspond to effective detachment of all types of unhealthy materials. In some embodiments, the full range of frequencies can be applied substantially simultaneously. For example, an acoustic signal comprising a random or noisy distribution of frequencies can be applied to the tooth 10 to clean all the unhealthy portions from the tooth 10.
In other embodiments, pressure wave generators 5A, 5B, 5C corresponding to a particular range of frequencies may be applied sequentially to sequentially remove the various types and/or sizes of unhealthy material from the tooth 10. For example, during a first treatment phase, the pressure wave generator 5A may be activated first to propagate pressure waves 23A corresponding to the first frequency or range of frequencies. During a second treatment phase, the pressure wave generator 5B may be activated next to propagate pressure waves 23B corresponding to the second frequency or range of frequencies. During a third treatment phase, the pressure wave generator 5C may be activated to propagate pressure waves 23C corresponding to the third frequency or range of frequencies. In some embodiments, the clinician can select the treatment phase as desired, e.g., to target a specific type or size of unhealthy material. In other embodiments, the system can be configured such that the treatment phases are automatically cycled in order to activate each of the plurality of pressure wave generators. In some arrangements, the system can be configured such that the treatment phases are randomly cycled.
Furthermore, the pressure wave generators 5A, 5B, 5C can act to induce bulk fluid movement, e.g., fluid motion 24 in the chamber 6, as described herein. In addition, in some embodiments, the pressure wave generators 5A, 5B, 5C can act to obturate or fill a treated tooth or treatment region. Accordingly, in the embodiment of Figure 7B, multiple pressure wave generators 5A, 5B, 5C can be used sequentially and/or simultaneously to propagate acoustic waves in multiple frequency bands to substantially clean and/or fill the tooth 10 or a treatment region thereof.

V. Examples of Tooth Seals and Alignment Features
Figure 8A is a schematic side cross-sectional view of a coupling member 3 attached or coupled to a tooth 10 by way of a locking tooth seal 26. It can be important to provide a stable coupling surface upon which to couple the coupling member 3. For example, if the coupling member 3 and pressure wave generator 5 are permitted to move significantly relative to the tooth 10, then the results of the procedure may be inconsistent and unsuitable.
Accordingly, the clinician can form an access opening 18 in the tooth 10. The tooth seal 26 can be applied around a perimeter of the access opening 18 such that the tooth seal 26 comprises a peripheral boundary. The chamber 6 and positioning member 3 can be positioned within the peripheral boundary of the tooth seal 26 to secure the chamber 6 and positioning member 3 to the tooth seal 26. Furthermore, it can be important to prevent or reduce lateral movement of the positioning member 3 relative to the tooth 10, e.g., movement transverse to a central axis Z of the root canal 13. For example, a locking wall 64 can be defined along the periphery of the tooth seal 26. The locking wall 64 can extend upwardly relative to the tooth 10, such that the wall 64 prevents lateral movement of the positioning member 3 and to help secure the coupling member 3 to the tooth 10. The lateral wall 64 can be defined to have a width or diameter slightly larger than a corresponding width or diameter of the coupling member 3. The lateral wall 64 can be defined to have tolerances such that a snug fit is formed between the seal 26 and the coupling member 3.
In some embodiments, the clinician can form the tooth seal 26 and locking wall 64 using a mold. The mold can be shaped to correspond to the ultimate profile of the seal 26 and locking wall 64. For example, the clinician can apply the mold about the tooth 10 and can flow the sealing material inside the mold in a flowable state. The sealing material can be cured (e.g., heated, exposed to ultraviolet light, etc.) such that the sealing material hardens into a solid or semi-solid state. In other embodiments, the clinician can manually shape the tooth seal 26 and locking wall 64 to have the desired dimensions and shape.
The clinician can apply the coupling member 3 to the seal 26 between and/or within the boundary defined by the locking wall 64. The seal 26 can comprise a substantially planar surface upon which the distal end of the coupling member 3 rests. As explained above, the locking walls 64 can prevent lateral movement of the coupling member 3. In some embodiments, the coupling member 3 can be attached to the seal 26, while in other embodiments, the clinician can press the coupling member 3 against the seal 26.
Fluid 22 can be supplied to the chamber 6 by way of the fluid inlet 61 such that the chamber 6 is at least partially or substantially filled with the fluid 22. The pressure wave generator 5 can be activated to substantially clean and/or fill the tooth 10. For example, as explained herein, the pressure wave generator 5 can induce pressure waves 23 and fluid motion 24 in the chamber 6 and/or tooth 10 that are sufficient to clean and/or fill the tooth 10. As above, the pressure wave generator 5 of Figure 8A can be any suitable pressure wave generator, such as a liquid jet device. Waste fluid can flow out of the tooth 10 and chamber 6 by way of the fluid outlet 62 along the handpiece 20. A vent 63 can be provided to regulate the pressure in the tooth 10 and/or chamber 6. As shown in Figure 8A, for example, the vent 63 can be formed through a wall of the coupling member 3 to provide fluid communication with the exterior environs, e.g., air.
Figure 8B is a schematic side cross-sectional view of a coupling member 3 having a curved distal end portion 65 shaped to mate with a curved surface 66 of a tooth seal 26. As shown in Figure 8B, the coupling member 3 can be ball-shaped in some embodiments. In some procedures, it may be desirable for the clinician to rotate the coupling member 3 and pressure wave generator 5 to a desired orientation relative to the tooth 10. For example, the clinician may desire to position the pressure wave generator 5 at a particular location and/or orientation relative to the access opening 18 of the tooth 10. As explained herein, it can be advantageous in some arrangements to direct or pass fluid across the access opening 18 transverse to a central axis Z of the root canal 13.
In some embodiments, the tooth seal 26 can be applied to the tooth 10 about the access opening 18 such that the tooth seal 26 comprises a curved surface 66, e.g., a surface defining a concave portion facing the coupling member 3 and an opposing convex portion facing the tooth 10. As above, the seal 26 can be formed using a mold in some embodiments. In other embodiments, the clinician can manually shape the curved surface 66 of the tooth seal 26. The curved surface 66 of the tooth seal 26 can be defined to have a curvature (e.g., a radius of curvature) that is approximately the same as a curved distal portion 65 of the coupling member 3.
After forming the tooth seal 26, the clinician can apply the curved distal portion 65 of the coupling member 3 to the corresponding curved surface 66 of the tooth seal 26 such that the curved distal portion 65 mates with the complementary curved surface 66 of the seal 26. In some embodiments, the tooth seal 26 is fixed relative to the tooth 10 and the curved distal portion 65 is rotationally free to move relative to the seal 26. In other embodiments, the curved surface 66 of the tooth seal 26 and the curved distal portion 65 are coupled together and free to rotate relative to the tooth 10 and access opening 18.
As explained above, fluid 22 is supplied to the chamber 6 and the tooth 10 by way of the fluid inlet 61. For example, the chamber 6 can be substantially filled with the fluid 22. The pressure wave generator 5 can be activated to substantially clean the tooth 10, e.g., to remove unhealthy materials from the tooth. The pressure wave generator 5 can generate pressure waves 23 and fluid motion 24 sufficient to clean the tooth 10. Waste fluid can be removed from the tooth 10 and chamber 6 by way of the fluid outlet 62. The vent 63 can be provided in the coupling member 3 to regulate the pressure in the tooth 10 and/or chamber 6.
During the treatment procedure, the clinician may want to manipulate the coupling member 3 and/or pressure wave generator 5 to orient the pressure wave generator 5 at a desired orientation and/or position. In the embodiment of Figure 8B, for example, the clinician can manually rotate the handpiece 20, which in turn rotates the coupling member 3 and the curved distal portion 65 of the coupling member 3. The curved distal portion 65 can rotate relative to the curved surface 66 of the tooth seal 26 until the coupling member 3 and pressure wave generator 5 are oriented relative to the tooth 10 at a desired orientation. Accordingly, the tooth seal 26 and curved coupling member 3 can advantageously be used by a clinician to rotate the coupling member 3 relative to the tooth 10.
Figure 8C is a schematic side cross-sectional view of a coupling member 3 having an alignment feature comprising a mating tube 67 sized and shaped to fit through an access opening 18 formed in the tooth 10. As shown in Figure 8C, the coupling member 3 can comprise an access aperture 70 that defines an opening configured to provide fluid communication between the chamber 6 and the tooth 10. The mating tube 67 can surround and extend from the access aperture 70 of the coupling member 3.
In some embodiments, such as treatment procedures applied to a premolar tooth, it can be challenging to align the coupling member 3 to the access opening 18 of the tooth 10. Accordingly, in some embodiments, the clinician can form the access opening 18 and can apply the tooth seal 26 about the access opening 18 of the tooth 10. The clinician can apply the coupling member 3 to the tooth seal 26 such that the mating tube 67 is inserted through the access opening 18 and into a portion of the tooth 10. As shown in Figure 8C, the mating tube 67 can help the clinician find the access opening 18 during treatment. Furthermore, the mating tube 67 can help laterally secure the coupling member 3 relative to the tooth 10. For example, the mating tube 67 can prevent the coupling member 3 from translating in a direction transverse to a central axis Z of the root canal 13 during treatment. The coupling member 3 can be attached to the seal 26, or the clinician can press the coupling member 3 against the tooth seal 26.
As above, the chamber 6 can be substantially filled with fluid 22 supplied by the fluid inlet 61. The pressure wave generator 5 can be activated to generate pressure waves 23 and fluid motion 24 in the chamber 6 and/or tooth 10. The pressure wave generator 5 can act to substantially clean and/or fill the tooth 10. Waste fluid can be removed by the fluid outlet 62. A vent 63 can be provided to regulate the pressure in the tooth 10 and/or chamber 6. Accordingly, the embodiment disclosed in Figure 8C can advantageously align the coupling member 3 with the access opening 18 of the tooth 10 and can help to secure the coupling member 3 relative to the tooth 10.

VI. Examples of Pressure wave generators
Figure 9A is a schematic side cross-sectional view of a coupling member 3 and a pressure wave generator 5 comprising a liquid jet device. As with the embodiments of Figure 5-8C, the coupling member 3 can couple to the tooth 10 by way of a tooth seal 26. The pressure wave generator 5 can be disposed in the chamber 6 of the coupling member 3 outside the tooth 10. The fluid inlet 61 can supply fluid 22 to the tooth 10, and the pressure wave generator 5 can be activated to clean the tooth 10.
As shown in Figure 9A, the pressure wave generator 5 comprises a liquid jet device. The liquid jet device can include a guide tube 60 and an impingement member 69 disposed at a distal end of the guide tube 60. A liquid jet 60 can be formed by a nozzle or orifice disposed in the distal end portion 21 of the handpiece. The jet 60 can propagate through a channel of the guide tube 27. One or more openings in the guide tube 27 can permit the jet 60 to interact with the fluid 22 filling the chamber 6. The jet 60 can impinge upon the impingement member 69, and can form a spray 68 of fluid that disperses through the fluid 22 in the chamber 6. Additional details of the liquid jet device disclosed in Figure 9A can be found at least in [0045]-[0050], [0054]-[0077] and various other portions of U.S. Patent Publication No. US 2011/0117517, published May 19, 2011, and in [0136]-[0142] and various other portions of U.S. Patent Publication No. US 2012/0237893, published September 20, 2012, each of which is incorporated by reference herein in its entirety and for all purposes.
A fluid inlet 61 can supply fluid 22 to the tooth 10. In the embodiment of Figure 9A, the liquid jet device can comprise the fluid inlet 61. As explained herein, the interaction of the liquid jet 60 with the fluid 22 and the impingement member 69 can create pressure waves 23 and fluid motion 24 that are sufficient to clean the tooth 10 (or fill or obturate the tooth in obturation treatments). As above, waste fluid can be removed from the chamber 6 and tooth 10 by way of the fluid outlet 62. One or more vents 63 can be provided to regulate the pressure in the tooth 10 and/or chamber 6.
Figure 9B is a schematic side cross-sectional view of a coupling member 3 and a pressure wave generator 5 comprising a light emitting element 71. Unless otherwise noted, the components illustrated in Figure 9B are similar to or the same as similarly numbered components in Figure 9A. The light emitting element 71 can be disposed in the chamber 6 of the coupling member 3. A laser beam or other suitable light source can propagate electromagnetic energy into the chamber 6, and the electromagnetic energy can be transformed into pressure waves 23 as it enters the fluid 22. In some embodiments, the laser beam can be directed into the chamber 6 as a collimated and coherent beam of light. The collimated laser beam can be sufficient to generate pressure waves 23 as the light delivers energy to the fluid 22. The concentrated energy can be transformed into pressure waves 23 sufficient to clean the undesirable dental matter. In some embodiments, the wavelength of the laser beam or electromagnetic source can be selected to be highly absorbable by the treatment fluid in the chamber or mouth (e.g., water) and/or by the additives in the treatment fluid (e.g., nanoparticles, etc.). For example, at least some of the electromagnetic energy may be absorbed by the fluid (e.g., water) in the chamber, which can generate localized heating and pressure waves 23 that propagate in the fluid. The acoustic waves generated by the electromagnetic beam can generate photo-induced or photo-acoustic cavitation effects in the fluid. In some embodiments, the localized heating can induce rotational fluid flow 24 in the chamber 6 and/or tooth 10 that further enhances cleaning of the tooth 10. In obturation procedures, the pressure wave generator 5 of Figure 9B can be used to substantially fill the treated root canal 13.
Figure 9C is a schematic side cross-sectional view of a coupling member 3 and a pressure wave generator 5 comprising a vibrating mechanical element 72. Unless otherwise noted, the components illustrated in Figure 9C are similar to or the same as similarly numbered components in Figures 9A-9B. The vibrating mechanical element 72 can comprise a piezoelectric element that vibrates in response to an applied electrical signal. As with the pressure wave generators 5 disclosed herein, the vibrating mechanical element 72 can be disposed in the chamber 6. When activated, the vibrating mechanical element 72 can propagate pressure waves 23 through the fluid 22 and tooth 10 and can induce fluid motion 24 in the chamber 6. The pressure wave generator 5 of Figure 9C can therefor act to clean and/or fill the tooth 10, as explained herein.
Figure 9D is a schematic side cross-sectional view of a coupling member 3 and a pressure wave generator 5 comprising a stirring element 73. Unless otherwise noted, the components illustrated in Figure 9D are similar to or the same as similarly numbered components in Figures 9A-9C. The stirring element 73 can comprise a rotational drive axis and a propeller coupled to the drive axis. When rotated, the drive axis can rotate the propeller of the stirring element 73 to generate pressure waves 23 and/or fluid motion 24 in the chamber 6 and/or tooth 10 to clean and/or fill the tooth 10.
Figure 10A is a side cross-sectional view of a coupling member 3 having a pressure wave generator 5 configured to generate a fluid motion 24 in a chamber 6 of the coupling member 3 and/or pressure waves 23 in the fluid 22. As above, the coupling member 3 can be formed with or coupled to a distal end portion 21 of a handpiece 20. In the embodiment of Figure 10A, the coupling member 3 is coupled to the tooth 10 by way of a tooth seal 26. A mating tube 67 can be used to align and/or secure the positioning member 3 to the tooth 10. The mating tube 67 can extend about and define an access aperture or port 70 of the coupling member 3 that provides fluid communication between the chamber 6 and the tooth 10. As shown in Figure 10A, the root canal 13 can have a central axis Z extending along a major length or dimension of the root canal 13. The mating tube 67 can prevent the coupling member 3 from translating in a direction X transverse to the central axis Z.
In the embodiment of Figure 10A, the pressure wave generator 5 can be disposed in the chamber 6, which can be outside the tooth 10. The pressure wave generator 5 can be positioned offset from a central region of the coupling member 3, e.g., positioned along a wall of the coupling member 3. As shown in Figure 10A, the pressure wave generator 5 can comprise a fluid inlet 61 configured to supply a fluid 22 to the chamber 6 of the coupling member 3. For example, in some embodiments, the fluid inlet 61 can be configured to supply a treatment fluid. In embodiments using a treatment fluid, the pressure wave generator 5 can be configured to clean the tooth. As explained herein, the pressure wave generator 5 can enhance the effects of the treatment fluid to clean both larger canal spaces and smaller cracks and crevices of the tooth. The pressure wave generator 5 can be activated to generate a broad spectrum of acoustic frequencies to clean different types of material from differently-sized spaces of the tooth 10.
In other embodiments, the fluid inlet 61 can be configured to supply a flowable obturation material. As explained above, in these embodiments, the pressure wave generator can supply the flowable obturation material in a flowable state and can propagate the flowable obturation material throughout the root canal, e.g., through both the larger root canal space and smaller cracks, spaces, crevices, tubules, etc. of the tooth. By filling substantially the entire root canal system, the pressure wave generator 5 can prevent infection or other negative patient outcomes by preventing the growth of bacteria in unfilled or unobturated spaces.
The fluid inlet 61 can be in fluid communication with the console 2, and a controller can control the flow of flowable material 22 through the inlet 61. As explained herein, the controller can supply the fluid 22 (e.g., the treatment fluid or a flowable obturation material) through the inlet 61 at various frequencies during a treatment phase of the procedure. In some embodiments, the chamber 6 can be filled or substantially filled with a flowable material 22, such as a treatment fluid or an obturation material, and the pressure wave generator 5 can be activated once the chamber 6 is filled with the flowable material 22 at a desired level and/or can be activated to substantially fill the chamber 6.
As shown in Figure 10A, the fluid inlet 61 can supply the fluid 22 into the chamber 6 to introduce fluid motion 24 in the chamber. As shown in Figure 10A, for example, the fluid motion 24 comprises a rotational flow of fluid in the chamber 6. The fluid motion 24 can define a rotational flow path or field substantially about an axis transverse to the central axis Z of the root canal 13 (e.g. the fluid flows in a direction ω about axes transverse to the central axis Z).
For example, one way to induce the fluid motion 24 illustrated in Figure 10A is to position a distal end portion 25 of the pressure wave generator 5 adjacent to the access port 70 of the coupling member 3. As explained herein, the pressure wave generator 5 can act as a fluid motion generator to generate fluid motion 24 in the chamber 6. The distal end portion 25 of the fluid inlet 61 can direct a stream or beam of fluid across the access opening 18 of the tooth 10 (and/or across the access port 70 of the coupling member 3 and chamber 6) along an X direction transverse to the central axis Z of the root canal 13. For example, in some embodiments, the fluid inlet 61 can direct a stream of fluid 22 along a direction that is substantially perpendicular to the central axis Z of the root canal 13, e.g., in a direction that is more or less orthogonal to a major axis of the canal 13. Furthermore, the fluid (e.g., the momentum of the fluid stream) can be directed along and/or substantially parallel to a plane near the proximal-most end of the access port 70 to induce the fluid motion 24 shown in Figure 10A. The fluid flow 24 across the access port 70 can be varied to control a desired apical pressure near the apex of the tooth 10. For example, the momentum of the fluid motion 24 can be controllably adjusted by way of the system controller 51. Further, the angle relative to the central axis Z can also be adjusted to control apical pressure. Indeed, the parameters of the pressure wave generator 5 can be adjusted to increase, decrease, and/or maintain the apical pressure to improve patient outcomes.
The motion 24 of the fluid 22 in the chamber 6 across the port 70 (which may induce flow in the rotational direction ω shown in Figure 10A) can induce vortices 75 throughout the root canal 13. For example, shear forces in the fluid 22 induced by the rotational flow 24 can generate vortices 75 that rotate or circulate in opposite directions (e.g., clockwise and counterclockwise as shown in Figure 10A). For example, in some arrangements, stronger vortices 75 may be created near the access port 70, and weaker vortices 75 may be created nearer the apical opening 15. In some embodiments, the vortices 75 may gradually weaken along the length of the canal from a point near the access port 70 to the apical opening 15. The weaker vortices 75 nearer the apical opening 15 may help to prevent or reduce the risk of extrusion of material through the apex of the tooth, which can lead to safer treatment procedures. The vortices 75 can be adjusted by controlling the parameters of the pressure wave generator 5 and the fluid motion 24 generated by the pressure wave generator 5. In some embodiments, the vortices 75 can be steady in size, shape, and/or direction. In other embodiments, the vortices 75 can be unsteady or chaotic.
Furthermore, the alternating directions of the vortices along the root canal 13 can advantageously create a negative pressure (or low positive pressure) near the apical opening 15 of the tooth 10. For example, the vortices 75, which also rotate about axes transverse to the central axis Z of the root canal 13, may cause micro-flows upwards towards the access opening 18 such that fluid 22 tends to experience a slightly negative pressure (e.g., a slight tendency to flow upwards through the canal 13 towards the access opening 18) near the apical opening 15. As explained below with respect to Figures 14A-14C, the negative pressure near the apical opening 15 can prevent material in the tooth 10 from extruding out through the apical opening 15. In other treatments, for example, the pressure near the apical opening 15 can be positive such that material is pushed out, or extruded, through the apical opening 15 and into the jaw of the patient. Such extrusion can lead to undesirable patient outcomes such as infection, high levels of pain, etc.
In some embodiments, it can be advantageous to dispose the pressure wave generator 5 within the chamber 6 and to use a coupling member 3 with an access port 70 as large as possible. By increasing the diameter or major dimension of the access port 70, more energy can be directed into the tooth 10, which can enhance the tooth cleaning procedure. Increasing the diameter or major dimension can also enhance the obturation procedure when used in such embodiments. In some embodiments, for example, the mating tube 67 may not be used so as to increase the size of the access port 70 by about twice a thickness of the walls of the mating tube 67. Accordingly, in various embodiments, the access port 70 of the coupling member 3 can be at least as large as a diameter or major dimension of the access opening 18 formed in the tooth 10. In some embodiments, for example, the access port 70 can be about the same size as the access opening 18 formed in the tooth 10.
As above, the pressure wave generator 5 can also be configured to generate pressure waves 23 through the fluid 22 and the tooth 10. As explained herein, in cleaning treatments, a combination of the pressure waves 23, fluid motion 24, and chemistry of the treatment fluid can act to substantially remove unhealthy materials from the tooth 10, including in small spaces, cracks, and crevices of the tooth 10. Waste fluid and detached materials can be removed from the tooth 10 and/or the chamber 6 by way of a fluid outlet 62. As explained above, one or more vents 63 can be provided through the coupling member 3 to regulate the pressure in the chamber 6. In filling or obturation procedures, the pressure waves 23, fluid motion 24, and chemistry of the obturation material can act to substantially fill the entire root canal system.
Figure 10B is a side cross-sectional view of a coupling member 3 having a pressure wave generator 5 comprising a liquid jet device configured to generate a fluid motion 24 in a chamber 6 of the coupling member 3. Unless otherwise noted, the components illustrated in Figure 10B are similar to or the same as similarly numbered components in Figures 9A and 10A. As with the pressure wave generator 5 of Figure 10A, the liquid jet device can be disposed along a wall of the coupling member 3. The liquid jet device can include a guide tube 27 along which the jet 60 propagates. The guide tube 27 can include one or more openings that permit fluid communication between the jet 60 and the fluid 22 in the chamber 6. In some embodiments, the fluid 22 may be supplied by an inlet other than the jet 60. In other embodiments, the jet 60 can comprise the fluid 22 and can supply the fluid 22 to the chamber 6. In some embodiments, the chamber 6 can be filled or substantially filled with the fluid 22.
The pressure wave generator 5 can be activated, and the jet 60 can impact the impingement member 69, which can deflect the jet 60 into a spray 69. For example, the spray 69 can generate fluid motion 24 across the access port 70, as explained above with respect to Figure 10A. The liquid jet device can induce fluid motion 24 in the chamber, e.g., in a rotational direction ω about an axis transverse to a central axis Z of the root canal. For example, the spray 68 can induce a stream of fluid passing across an access aperture 70 of the coupling member 3, e.g., along a direction X transverse to (e.g., substantially perpendicular to) the central axis Z of the root canal 13 and/or a central axis of the chamber. The spray 69 can induce fluid flow 24 in a direction parallel to a plane of the access port 70, e.g., a proximal-most plane of the access port that defines an opening between the chamber 6 and the tooth. The fluid flow 24 can induce opposing vortices 75 throughout the root canal 13. The fluid motion 24 induced in the tooth 10 (possibly in combination with pressure waves 23) can act to remove unhealthy materials from the tooth 10. Furthermore, as explained above with respect to Figure 10A, the induced vortices 75 can create a negative pressure at or near the apical opening 15, which can advantageously prevent the extrusion of material through the apical opening 15. In addition, as with Figure 10A, the diameter of the access port 70 of the coupling member 3 can be at least as large as the access opening 18 formed in the tooth 10, e.g., about the same size as the access opening 18. Furthermore, in obturation treatments, the pressure wave generator 5 of Figure 10B can act to substantially fill the entire root canal system.
Figure 10C is a side cross-sectional view of a coupling member 3 having a pressure wave generator 5 comprising a light emitting element 72 configured to generate a fluid motion 24 in a chamber 6 of the coupling member 3. Unless otherwise noted, the components illustrated in Figure 10C are similar to or the same as similarly numbered components in Figures 9B and 10A-10B. As with the embodiment of Figure 9B, the pressure wave generator 5 can comprise a laser or other light source. The light emitting element 72 can propagate high intensity light onto a localized reservoir 78 of fluid 22, such as a treatment fluid, an obturation material, etc. For example, a gate 77 can selectively permit fluid 22 to flow from the chamber 6 into the localized reservoir 78. The light propagating from the light emitting element 72 can impinge upon the fluid 22 in the reservoir 78 and can locally heat the fluid 22 in the reservoir 78. Heating the fluid 22 in the reservoir 78 to a sufficient degree may cause the fluid 22 to move out of the reservoir along a direction X transverse to a central axis Z of the root canal 13 of the tooth 10. For example the fluid 22 can move out of the reservoir 78 substantially perpendicular to the central axis Z of the root canal and/or in a direction substantially parallel to a proximal-most plane of the access port 70.
As with the embodiments disclosed above with respect to Figures 10A-10B, the flow of flowable material 22 from the reservoir 78 can induce a rotational fluid flow 24 about a rotational direction ω. The rotational flow 24 can induce vortices 75 throughout the root canal 13 that can induce negative pressures at or near the apical opening 15 of the tooth 10. Furthermore, a diameter of the access port 70 can be at least as large as the access opening 18 in some embodiments. As above, in cleaning procedures, the fluid motion 24 and the pressure waves 23 can act to substantially clean the tooth 10. In obturation procedures, the pressure wave generator 5 can act to substantially fill the entire root canal system.
Figure 10D is a side cross-sectional view of a coupling member 3 having a pressure wave generator 5 substantially aligned with a central axis Z of the root canal 13. The pressure wave generator 5 of Figure 10D can be a nozzle configured to output a fluid 22 into the chamber 6, or any of the other pressure wave generators disclosed herein. Unless otherwise noted, the components illustrated in Figure 10D are similar to or the same as similarly numbered components in Figures 10A-10C. The pressure wave generator 5 can be any suitable pressure wave generator disclosed herein, such as a liquid jet device, a fluid inlet, a light emitting element, etc. Unlike the embodiments of Figures 10A-10C, which may be offset from the Z-axis, the pressure wave generator 5 of Figure 10D is generally aligned with the Z-axis.
Furthermore, unlike the embodiments of Figures 10A-10C, the pressure wave generator 5 of Figure 10D can be configured to generate a fluid motion 24 of flowable material 22 about the Z-axis. The fluid motion 24 substantially around the Z-axis can generate a swirl 76 of fluid, which can propagate through the root canal 23. Similar to the embodiments above, the rotational power of the fluid motion 24 can be adjusted to control the amount of swirl 76 to assist with the treatment procedure. As above, in cleaning treatments, the pressure wave generator 5 can clean substantially the entire root canal 13. In obturation treatments, the pressure wave generator 5 can fill or obturate substantially the entire root canal 13, including branch structures, as explained in more detail herein.
Figure 10E is a side cross-sectional view of a coupling member 3 having a first pressure wave generator 5a and a second pressure wave generator 5b. Unless otherwise noted, the components illustrated in Figure 10E are similar to or the same as similarly numbered components in Figure 10D. However, unlike the embodiment of Figure 10D, the two pressure wave generators 5a, 5b can be disposed offset from the central axis Z. In the illustrated embodiment, the pressure wave generators 5a, 5b can be disposed eccentrically with respect to the Z-axis (e.g., a central axis of the root canal and/or a central axis of the chamber 6), e.g., the pressure wave generators 5a, 5b can be at about the same distance from the Z-axis. Like the embodiment of Figure 10D, each pressure wave generator can generate a corresponding fluid motion 24 about the direction of the Z-axis, but the rotation is offset from the Z-axis, as shown in Figure 10E. Furthermore, in the illustrated embodiment, the pressure wave generator 5a can generate fluid motion 24a about the Z-axis in one direction, and the pressure wave generator 5b can generate fluid motion 24b about the Z-axis direction in an opposite direction. The counter-flows induced by the two pressure wave generators 24a, 24b can cooperate to induce swirl 76 that propagate through the root canal 13. As explained above, the induced swirl 76 and pressure waves 23 can clean substantially the entire root canal 13 in cleaning treatments. In obturation treatments, the induced vortices and pressure waves 23 can fill or obturate substantially the entire root canal system.
Figure 10F is a schematic top view of fluid motion generator 5 at least partially disposed in a chamber 6 and configured to generate swirl 76 in the chamber 6. The fluid motion generator 5 of Figure 10F can comprise a nozzle or outlet configured to supply fluid 23 into the chamber 6. In the embodiment of Figure 10F, the central Z-axis of the root canal is coming out of the page. As shown in Figure 10F, the fluid motion generator 5 can direct fluid motion 24 in a direction transverse (e.g., substantially perpendicular to) the major axis of the root canal, e.g., across the access port 70. The fluid motion 24 can impact walls of the chamber 6 and can shear inwardly to create the swirl motion 76. As explained above, the swirl 76 can propagate through the root canal 13 to clean and/or fill the root canal 13. The fluid motion generator 5 can be disposed anywhere along the height of the chamber 6. Furthermore, as explained herein, the fluid motion generator 5 may also comprise a liquid jet, fluid inlet, etc.
Figure 10G is a schematic top view of multiple fluid motion generators 5a, 5b at least partially disposed in a chamber 6 and configured to generate counter-swirl fluid motion 76a, 76b in the chamber 6. As shown in Figure 10G, for example, the fluid motion generators can be disposed eccentrically relative to the central axis Z of the root canal and/or the central axis of the chamber 6 (e.g., out of the page). Each fluid motion generator 5a, 5b can propagate fluid motion 24 across the access port 70 in a direction transverse to (e.g., substantially perpendicular to) the central axis Z. Each counter-swirl 76a, 76b can rotate in opposing directions about the Z-axis of the root canal and can interact with one another to generate swirl 76 throughout the root canal to clean and/or fill the canals.

VII. Additional Details Regarding Enhanced Cleaning of Teeth
It is believed, although not required, that some or all of the effects described herein may be at least in part responsible for advantageous effects, benefits, or results provided by various implementations of the treatment methods and systems described herein. Accordingly, various embodiments of the systems disclosed herein can be configured to provide some or all of these effects.
In the following description, unless a different meaning is indicated, the following terms have their ordinary and customary meaning. For example, a chemical reaction front may generally refer to an interface between the tissue and the solution which contains a chemical such as a tissue dissolving agent. Tissue may refer to all types of cells existing in the tooth as well as bacteria and viruses. Calcified tissue may refer to calcified pulp, pulp stones, and tertiary dentin. Bubbles includes but is not limited to bubbles created due to a chemical reaction, dissolved gas remaining in the fluid after degassing (if used) and released as bubbles in the fluid, and any bubbles which are introduced into the tooth due to imperfect sealing.
Tissue cleaning treatments may utilize one or more of the physicochemical effects described herein to clean and remove tissue and/or calcified tissue from a tooth chamber. In some cleaning treatments, the combination of (1) acoustic or pressure waves (e.g., generation of acoustic cavitation), (2) circulation of fluid in the chamber (e.g., macroscopic eddies and flows), and (3) chemistry (e.g., use of a tissue dissolving agent, use of degassed fluids) can provide highly effective cleaning. Accordingly, certain embodiments of the systems disclosed herein utilize a pressure wave generator to generate the acoustic waves, a fluid platform (e.g., fluid retainer) to retain treatment fluid in the tooth chamber and to enable circulation of the treatment fluid, and a treatment fluid that is degassed or includes a chemical agent such as a tissue dissolving agent.

A. Pressure Waves
A pressure wave generator can be used to generate pressure waves that propagate through the fluid in the chamber 6 (and the tooth). Upon irradiation of a fluid with high intensity pressure waves (e.g., broadband frequencies), acoustic cavitation may occur. As has been described herein, the implosive collapse of the cavitation bubbles can produce intense local heating and high pressures with short lifetimes. Therefore, in some treatment methods, acoustic cavitation may be responsible for or involved in enhancing chemical reactions, sonochemistry, sonoporation, tissue dissociation, tissue delamination, as well as removing the bacteria and/or the smear layer from the root canals and tubules. The effects of enhancing chemical reaction via vibrations or sonochemistry will be described below in the section on chemistry.
Sonoporation is the process of using an acoustic field to modify the permeability of the cell plasma membrane. This process may greatly expedite the chemical reaction. It may be advantageous if the acoustic field has a relatively broad bandwidth (e.g., from hundreds to thousands of kHz). Some frequencies (e.g., low frequency ultrasound) may also result in cellular rupture and death (e.g., lysis). This phenomenon may kill bacteria which might otherwise reinfect the tooth. Acoustic waves and/or acoustic cavitation may loosen the bond between cells and/or may dissociate the cells. Acoustic waves and/or acoustic cavitation may loosen the bond between cells and dentin and/or delaminate the tissue from the dentin.
For removing calcified tissue, acoustic waves may induce sonochemistry and microscopic removal of calcified structures due to shock waves and/or microjets created as a result of cavitation bubble implosion. Pressure or acoustic waves may break microscopic calcified structures through structural vibrations. If a chemical (e.g., a chelating agent such as, e.g., EDTA) is used for this procedure, the acoustic waves may enhance the chemical reaction.
Certain properties of the system can be adjusted to enhance the effects of the acoustic waves. For example, properties of the fluid including, e.g., surface tension, boiling or vapor temperature, or saturation pressure can be adjusted. A degassed fluid with a reduced dissolved gas content can be used, which may reduce the energy loss of acoustic waves that may be generated by hydrodynamic cavitation or any other sources. The fluid can be degassed, which may help preserve the energy of the acoustic waves and may increase the efficiency of the system.

B. Fluid Circulation
Some treatment systems and methods use diffusion and/or acoustically enhanced diffusion of reactants and byproducts to and away from the chemical reaction front. However, due to the relatively short time scale of the reaction process, a faster mechanism of reactant delivery such as "macroscopic" fluid motion, circulation, convection, vorticity, or turbulence may be advantageous in some of the embodiments disclosed herein. For example, fluid inflow into the tooth chamber may induce a macroscopic circulation in the pulp cavity (see, e.g., Figures 1A and 10A-10C). A liquid jet device not only may create acoustic waves but may also induce circulation as the jet and/or spray enter the chamber 6. Other pressure wave generators can produce fluid circulation via their interaction with ambient fluid (e.g., via localized heating of the fluid, which may induce convection currents and circulation).
Fluid circulation with a time scale comparable to (and preferably faster than) that of chemical reaction may help replenish the reactants at a chemical reaction front and/or may help to remove reaction byproducts from the reaction site. The convective time scale, which may relate to effectiveness of the convection or circulation process, can be adjusted depending on, e.g., the location and characteristics of the source of circulation. The convective time scale is approximately the physical size of the chamber divided by the fluid speed in the chamber. Introduction of circulation generally does not eliminate the diffusion process, which may still remain effective within a thin microscopic layer at the chemical reaction front. Fluid circulation may create flow-induced pressure oscillations inside the root canal which may assist in delaminating, loosening, and/or removing larger pieces tissue from the root canal.
For removing calcified tissue, fluid circulation may create flow-induced pressure oscillations inside the root canal which may assist in removing larger pieces of calcified structures from the root canal.
Certain properties of the system can be adjusted to enhance the effects of the circulation in the tooth. For example, the location of the source of circulation inside the tooth, the source flow characteristics such as shape (e.g. planar vs. circular jets) or velocity and/or direction of a fluid stream, and the fluid kinematic viscosity may be adjusted. The circulation may also be effected by the anatomy of the tooth or the canal orifice or root canal size. For example, a narrow root canal with constrictions may have a lower solution replenishment rate than a wide canal with no constrictions. If the source of convection/circulation is placed near the pulp chamber floor, a tooth with a smaller pulp chamber may have stronger circulation than one with a larger pulp chamber. Convection-induced pressure exerted at the periapical region of the tooth may be controlled to reduce or avoid extrusion of the treatment fluid into the periapical tissues. Large magnitude vacuum or low pressure in the tooth may cause discomfort in some patients. Thus, the properties of the coupling member 3 (e.g., vents, sponges, flow restrictors, etc.) can be adjusted to provide a desired operating pressure range in the chamber 6 and/or tooth 10.

C. Chemistry
As explained herein, various reaction chemistries can be adjusted or designed to improve the cleaning process. For example, to enhance the dissolution of organic tissue, a tissue dissolving agent (e.g., a mineralization therapy agent, EDTA, sodium hypochlorite - NaOCl) can be added to the treatment liquid. The agent may react with various components at the treatment site. In some cases, tissue dissolution may be a multi-step process. The agent may dissolve, weaken, delaminate or dissociate organic and/or inorganic matter, which may result in better patient outcomes. The chemical reaction can modify the physical characteristics of the treatment solution locally (e.g., reducing the local surface tension via saponification), which may assist in the penetration of the treatment liquid into gaps and small spaces in the treatment sites or to remove bubbles formed during the chemical reaction. A tissue dissolving agent (e.g., sodium hypochlorite or bleach) may be added to the treatment fluid to react with tissue. Tissue dissolution may be a multi-step and complex process. Dissolution of sodium hypochlorite in water can include a number of reactions such as, e.g., the sodium hypochlorite (bleach) reaction, a saponification reaction with triglycerides, an amino acid neutralization reaction, and/or a chloramination reaction to produce chloramine. Sodium hypochlorite and its by-products may act as dissolving agents (e.g. solvents) of organics, fats, and proteins; thereby, degrading organic tissue in some treatments.
Sodium hypochlorite may exhibit a reversible chemical equilibrium based on the bleach reaction. Chemical reactions may occur between organic tissue and sodium hypochlorite. For example, sodium hydroxide can be generated from the sodium hypochlorite reaction and can react with organic and fat (triglycerides) molecules to produce soap (fatty acid salts) and glycerol (alcohol) in the saponification reaction. This may reduce the surface tension of the remaining solution. Sodium hydroxide can neutralize amino acids forming amino acid salts and water in the amino acid neutralization reaction. Consumption of sodium hydroxide can reduce the pH of the remaining solution. Hypochlorous acid, a substance that can be present in sodium hypochlorite solution, can release chlorine that can react with amino groups of proteins and amino acids to produce various chloramines derivatives. For example, hypochlorous acid can react with free amino acids in tissue to form N-chloro amino acids which can act as strong oxidizing agents that may have higher antiseptic activity than hypochlorite.
Chemical(s) in the fluid, depending on their type, may affect the surface tension of the solution, which in turn may modify the cavitation phenomenon. For example, solution of an inorganic chemical such as, e.g., sodium hypochlorite in water, may increase the ion concentration in the solution which may increase the surface tension of the solution, which may result in stronger cavitation. In some cases, the magnitude of a cavitation inception threshold may increase with increasing surface tension, and the cavitation inducing mechanism (e.g., a pressure wave generator) may be sufficiently intense to pass the threshold in order to provide inception of cavitation bubbles. It is believed, but not required, that once the cavitation threshold is passed, increased surface tension may result in stronger cavitation. Reducing the dissolved gas content of a fluid (e.g., via degassing) can increase the surface tension of the fluid and also may result in stronger cavitation. Addition of chemicals, agents, or substances (e.g., hydroxyl functional groups, nanoparticles, etc.) to the treatment may increase the efficiency of conversion of a pressure wave into cavitation, and such chemoacoustic effects may be desirable in some treatment procedures.
In some methods, a chemical, such as sodium hypochlorite, may cause saponification. The removal of bubbles created or trapped inside the root canals (or tubules) may be accelerated due to local reduction of surface tension at the chemical reaction front as a result of saponification. Although in some methods it may be desirable to have a relatively high surface tension at the pressure wave source (e.g. inside the pulp chamber), inside the canals it may be beneficial to have locally reduced surface tension to accelerate bubble removal. This phenomenon may happen as tissue dissolving agent(s) react with the tissue. For example, sodium hypochlorite can act as a solvent degrading fatty acids, transforming them into fatty acid salts (soap) and glycerol (alcohol) that can reduce the surface tension of the remaining solution at the chemical reaction front.
A number of variables or factors may be adjusted to provide effective cleaning. For example, each chemical reaction has a reaction rate determining the speed of reaction. The reaction rate may be dependent on several parameters including temperature. The concentration of reactants can be a factor and may affect the time for the reaction to complete. For instance, a 5% sodium hypochlorite solution generally may be more aggressive than a 0.5% sodium hypochlorite solution and may tend to dissolve tissue faster.
The refreshment rate of reactants may be affected by some or all of the following. Bubbles may form and stay at the chemical reaction front (e.g., due to surface tension forces) and may act as barriers at the chemical reaction front impeding or preventing fresh reactants from reaching the reaction front. Accordingly, circulation of the treatment fluid can help remove the bubbles and the reaction byproducts, and may replace them with fresh treatment fluid and fresh reactants. Thus, use of an embodiment of the fluid platform that can provide fluid circulation in the tooth chamber advantageously may improve the cleaning process.
Heat may increase the chemical reaction rate and may be introduced through a variety of sources. For example, the treatment solution may be preheated before delivery to the tooth chamber. Cavitation, exothermic chemical reactions, or other internal or external dissipative sources may produce heat in the fluid, which may enhance, sustain, or increase reaction rates.
Sonication of the fluid may increase chemical reaction rates or effectiveness. For example, upon irradiation of a fluid (e.g., water) with high intensity pressure waves (including, e.g., sonic or ultrasonic waves, or broad spectrum acoustic power produced by a liquid jet) acoustic cavitation may occur. The implosive collapse of the cavitation bubbles can produce intense local heating and high pressures with short lifetimes. Experimental results have shown that at the site of the bubble collapse, the temperature and pressure may reach around 5000 K and 1000 atm, respectively. This phenomenon, known as sonochemistry, can create extreme physical and chemical conditions in otherwise cold liquids. Sonochemistry, in some cases, has been reported to enhance chemical reactivity by as much as a million fold. In cases where acoustic cavitation does not occur (or occurs at a relatively low amplitude), the vibration of reactants, due to the pressure waves, may enhance the chemical reaction as it assists in replacing the byproducts by fresh reactants.
For removing calcified tissue, a decalcifying agent (e.g., an acid such as, e.g., EDTA or citric acid) may be added to the treatment fluid. The decalcifying agent may remove calcium or calcium compounds from the tooth dentin. The substances remaining after treatment with the decalcifying agent may be relatively softer (e.g., gummy) than prior to treatment and more easily removable by the fluid circulation and acoustic waves.

VIII. Degassed Treatment Fluids
As will be described below, the treatment fluid (and/or any of solutions added to the treatment fluid) can be degassed compared to normal liquids used in dental offices. For example, degassed distilled water can be used (with or without the addition of chemical agents or solutes).

A. Examples of Possible Effects of Dissolved Gases in the Treatment Fluid
In some procedures, the treatment fluid can include dissolved gases (e.g., air). For example, the fluids used in dental offices generally have a normal dissolved gas content (e.g., determined from the temperature and pressure of the fluid based on Henry's law). During cleaning procedures using a pressure wave generator, the acoustic field of the pressure wave generator and/or the flow or circulation of fluids in the chamber can cause some of the dissolved gas to come out of solution and form bubbles.
The bubbles can block small passageways or cracks or surface irregularities in the tooth, and such blockages can act as if there were a "vapor lock" in the small passageways. In some such procedures, the presence of bubbles may at least partially block, impede, or redirect propagation of acoustic waves past the bubbles and may at least partially inhibit or prevent cleaning action from reaching, for example, unhealthy dental materials in tubules and small spaces of the tooth 10. The bubbles may block fluid flow or circulation from reaching these difficult-to-reach, or otherwise small, regions, which may prevent or inhibit a treatment solution from reaching these areas of the tooth.
In certain procedures, cavitation is believed to play a role in cleaning the tooth. Without wishing to be bound by any particular theory, the physical process of cavitation inception may be, in some ways, similar to boiling. One possible difference between cavitation and boiling is the thermodynamic paths that precede the formation of the vapor in the fluid. Boiling can occur when the local vapor pressure of the liquid rises above the local ambient pressure in the liquid, and sufficient energy is present to cause the phase change from liquid to a gas. It is believed that cavitation inception can occur when the local ambient pressure in the liquid decreases sufficiently below the saturated vapor pressure, which has a value given in part by the tensile strength of the liquid at the local temperature. Therefore, it is believed, although not required, that cavitation inception is not determined by the vapor pressure, but instead by the pressure of the largest nuclei, or by the difference between the vapor pressure and the pressure of the largest nuclei. As such, it is believed that subjecting a fluid to a pressure slightly lower than the vapor pressure generally does not cause cavitation inception. However, the solubility of a gas in a liquid is proportional to pressure; therefore lowering the pressure may tend to cause some of the dissolved gas inside the fluid to be released in the form of gas bubbles that are relatively large compared to the size of bubbles formed at cavitation inception. These relatively large gas bubbles may be misinterpreted as being vapor cavitation bubbles, and their presence in a fluid may have been mistakenly described in certain reports in the literature as being caused by cavitation, when cavitation may not have been present.
In the last stage of collapse of vapor cavitation bubbles, the velocity of the bubble wall may even exceed the speed of sound and create strong shock waves inside the fluid. The vapor cavitation bubble may also contain some amount of gas, which may act as a buffer and slow down the rate of collapse and reduce the intensity of the shockwaves. Therefore, in certain procedures that utilize cavitation bubbles for tooth cleaning, it may be advantageous to reduce the amount of the dissolved air in the fluid to prevent such losses.
The presence of bubbles that have come out of solution from the treatment fluid may lead to other disadvantages during certain procedures. For example, if the pressure wave generator produces cavitation, the agitation (e.g. pressure drop) used to induce the cavitation may cause the release of the dissolved air content before the water molecules have a chance to form a cavitation bubble. The already-formed gas bubble may act as a nucleation site for the water molecules during the phase change (which was intended to form a cavitation bubble). When the agitation is over, the cavitation bubble is expected to collapse and create pressure waves. However, cavitation bubble collapse might happen with reduced efficiency, because the gas-filled bubble may not collapse and may instead remain as a bubble. Thus, the presence of gas in the treatment fluid may reduce the effectiveness of the cavitation process as many of the cavitation bubbles may be wasted by merging with gas-filled bubbles. Additionally, bubbles in the fluid may act as a cushion to damp pressure waves propagating in the region of the fluid comprising the bubbles, which may disrupt effective propagation of the pressure waves past the bubbles. Some bubbles may either form on or between tooth surfaces, or be transferred there by the flow or circulation of fluid in the tooth. The bubbles may be hard to remove due to relatively high surface tension forces. This may result in blocking the transfer of chemicals and/or pressure waves into the irregular surfaces and small spaces in and between teeth, and therefore may disrupt or reduce the efficacy of the treatment.

B. Examples of Degassed Treatment Fluids
Accordingly, it may be advantageous in some systems and methods to use a degassed fluid, which can inhibit, reduce, or prevent bubbles from coming out of solution during treatments as compared to systems and methods that use normal (e.g., non-degassed) fluids. In dental procedures in which the treatment fluid has a reduced gas content (compared with the normal fluids) tooth surfaces or tiny spaces in the tooth may be free of bubbles that have come out of solution. Acoustic waves generated by the pressure wave generator can propagate through the degassed fluid to reach and clean the surfaces, cracks, and tooth spaces and cavities. In some procedures, the degassed fluid can be able to penetrate spaces as small as about 500 microns, 200 microns, 100 microns, 10 microns, 5 microns, 1 micron, or smaller, because the degassed fluid is sufficiently gas-free that bubbles are inhibited from coming out of solution and blocking these spaces (as compared to use of fluids with normal dissolved gas content).
For example, in some systems and methods, the degassed fluid can have a dissolved gas content that is reduced when compared to the "normal" gas content of water. For example, according to Henry's law, the "normal" amount of dissolved air in water (at 25 C and 1 atmosphere) is about 23 mg/L, which includes about 9 mg/L of dissolved oxygen and about 14 mg/L of dissolved nitrogen. In some embodiments, the degassed fluid has a dissolved gas content that is reduced to approximately 10%-40% of its "normal" amount as delivered from a source of fluid (e.g., before degassing). In other embodiments, the dissolved gas content of the degassed fluid can be reduced to approximately 5%-50% or 1%-70% of the normal gas content of the fluid. In some treatments, the dissolved gas content can be less than about 70%, less than about 50%, less than about 40%, less than about 30%, less than about 20%, less than about 10%, less than about 5%, or less than about 1% of the normal gas amount.
In some embodiments, the amount of dissolved gas in the degassed fluid can be measured in terms of the amount of dissolved oxygen (rather than the amount of dissolved air), because the amount of dissolved oxygen can be more readily measured (e.g., via titration or optical or electrochemical sensors) than the amount of dissolved air in the fluid. Thus, a measurement of dissolved oxygen in the fluid can serve as a proxy for the amount of dissolved air in the fluid. In some such embodiments, the amount of dissolved oxygen in the degassed fluid can be in a range from about 1 mg/L to about 3 mg/L, in a range from about 0.5 mg/L to about 7 mg/L, or some other range. The amount of dissolved oxygen in the degassed fluid can be less than about 7 mg/L, less than about 6 mg/L, less than about 5 mg/L, less than about 4 mg/L, less than about 3 mg/L, less than about 2 mg/L, or less than about 1 mg/L.
In some embodiments, the amount of dissolved gas in the degassed fluid can be in a range from about 2 mg/L to about 20 mg/L, in a range from about 1 mg/L to about 12 mg/L, or some other range. The amount of dissolved gas in the degassed fluid can be less than about 20 mg/L, less than about 18 mg/L, less than about 15 mg/L, less than about 12 mg/L, less than about 10 mg/L, less than about 8 mg/L, less than about 6 mg/L, less than about 4 mg/L, or less than about 2 mg/L.
In other embodiments, the amount of dissolved gas can be measured in terms of air or oxygen percentage per unit volume. For example, the amount of dissolved oxygen (or dissolved air) can be less than about 5% by volume, less than about 1% by volume, less than about 0.5% by volume, or less than about 0.1% by volume.
The amount of dissolved gas in a liquid can be measured in terms of a physical property such as, e.g., fluid viscosity or surface tension. For example, degassing water tends to increase its surface tension. The surface tension of non-degassed water is about 72 mN/m at 20 °C. In some embodiments, the surface tension of degassed water can be about 1%, 5%, or 10% greater than non-degassed water.
In some treatment methods, one or more secondary fluids can be added to a primary degassed fluid (e.g., an antiseptic solution can be added to degassed distilled water). In some such methods, the secondary solution(s) can be degassed before being added to the primary degassed fluid. In other applications, the primary degassed fluid can be sufficiently degassed such that inclusion of the secondary fluids (which can have normal dissolved gas content) does not increase the gas content of the combined fluids above what is desired for a particular dental treatment.
In various implementations, the treatment fluid can be provided as degassed liquid inside sealed bags or containers. The fluid can be degassed in a separate setup in the operatory before being added to a fluid reservoir. In an example of an "in-line" implementation, the fluid can be degassed as it flows through the system, for example, by passing the fluid through a degassing unit attached along a fluid line (e.g., the fluid inlet). Examples of degassing units that can be used in various embodiments include: a Liqui-Cel® MiniModule® Membrane Contactor (e.g., models 1.7 x 5.5 or 1.7 x 8.75) available from Membrana-Charlotte (Charlotte, North Carolina); a PermSelect® silicone membrane module (e.g., model PDMSXA-2500) available from MedArray, Inc. (Ann Arbor, Michigan); and a FiberFlo® hollow fiber cartridge filter (0.03 micron absolute) available from Mar Cor Purification (Skippack, Pennsylvania). The degassing can be done using any of the following degassing techniques or combinations of thereof: heating, helium sparging, vacuum degassing, filtering, freeze-pump-thawing, and sonication.
In some embodiments, degassing the fluid can include de-bubbling the fluid to remove any small gas bubbles that form or may be present in the fluid. De-bubbling can be provided by filtering the fluid. In some embodiments, the fluid may not be degassed (e.g., removing gas dissolved at the molecular level), but can be passed through a de-bubbler to remove the small gas bubbles from the fluid.
In some embodiments, a degassing system can include a dissolved gas sensor to determine whether the treatment fluid is sufficiently degassed for a particular treatment. A dissolved gas sensor can be disposed downstream of a mixing system and used to determine whether mixing of solutes has increased the dissolved gas content of the treatment fluid after addition of solutes, if any. A solute source can include a dissolved gas sensor. For example, a dissolved gas sensor can measure the amount of dissolved oxygen in the fluid as a proxy for the total amount of dissolved gas in the fluid, since dissolved oxygen can be measured more readily than dissolved gas (e.g., nitrogen or helium). Dissolved gas content can be inferred from dissolved oxygen content based at least partly on the ratio of oxygen to total gas in air (e.g., oxygen is about 21% of air by volume). Dissolved gas sensors can include electrochemical sensors, optical sensors, or sensors that perform a dissolved gas analysis. Examples of dissolved gas sensors that can be used with embodiments of various systems disclosed herein include a Pro-Oceanus GTD-Pro or HGTD dissolved gas sensor available from Pro-Oceanus Systems Inc. (Nova Scotia, Canada) and a D-Opto dissolved oxygen sensor available from Zebra-Tech Ltd. (Nelson, New Zealand). In some implementations, a sample of the treatment can be obtained and gases in the sample can be extracted using a vacuum unit. The extracted gases can be analyzed using a gas chromatograph to determine dissolved gas content of the fluid (and composition of the gases in some cases).
Accordingly, fluid delivered to the tooth from a fluid inlet and/or the fluid used to generate the jet in a liquid jet device can comprise a degassed fluid that has a dissolved gas content less than normal fluid. The degassed fluid can be used, for example, to generate the high-velocity liquid beam for generating acoustic waves, to substantially fill or irrigate a chamber, to provide a propagation medium for acoustic waves, to inhibit formation of air (or gas) bubbles in the chamber, and/or to provide flow of the degassed fluid into small spaces in the tooth (e.g., cracks, irregular surfaces, tubules, etc.). In embodiments utilizing a liquid jet, use of a degassed fluid can inhibit bubbles from forming in the jet due to the pressure drop at a nozzle orifice where the liquid jet is formed.
Thus, examples of methods for dental and/or endodontic treatment comprise flowing a degassed fluid onto a tooth or tooth surface or into a chamber. The degassed fluid can comprise a tissue dissolving agent and/or a decalcifying agent. The degassed fluid can have a dissolved oxygen content less than about 9 mg/L, less than about 7 mg/L, less than about 5 mg/L, less than about 3 mg/L, less than about 1 mg/L, or some other value. A fluid for treatment can comprise a degassed fluid with a dissolved oxygen content less than about 9 mg/L, less than about 7 mg/L, less than about 5 mg/L, less than about 3 mg/L, less than about 1 mg/L, or some other value. The fluid can comprise a tissue dissolving agent and/or a decalcifying agent. For example, the degassed fluid can comprise an aqueous solution of less than about 6% by volume of a tissue dissolving agent and/or less than about 20% by volume of a decalcifying agent.

IX. Various Performance Characteristics of the Disclosed Systems and Methods
The disclosed methods, compositions, and systems (e.g., the disclosed pressure wave generators, treatment fluids, etc.) may clean outer and inner surfaces of teeth better than other systems, and may do so more safely than the other systems.
Figure 11A is a schematic diagram of an experimental setup designed to measure the power output of various tooth cleaning devices. As shown in Figure 11A, a tank was filled with a liquid (e.g., water), and a tip of the device to be tested was placed underneath the surface of the liquid. A hydrophone was placed in the tank to measure the output of each device under operating conditions. A voltage amplifier, circuit board, a DC power supply, and a workstation were used to measure the voltage output from the hydrophone for each measurement.
Figure 11B is a plot of the voltage (in volts) output by the hydrophone over time (in seconds) for each device. Measurements for four experiments are shown in Figure 11B. In particular, the plot in the upper left corner is a measure of voltage output over time for systems disclosed in this Application that are adapted to clean a molar tooth (referred to herein as "Applicant's Molar Cleaning Apparatus"). In particular, Applicant's Molar Cleaning Apparatus used in the experimental setup of Figure 11A is generally similar to the handpiece 50 described in relation to Figures 15A-15C of U.S. Patent Publication No. 2012/0237893, which is incorporated by reference herein. An impingement member having a concave impingement surface similar to the impingement members 110 described in relation to Figures 12A-12C of U.S. Patent Publication No. 2011/0117517, which is also incorporated by reference herein, can be disposed at a distal portion of the guide tube. Furthermore, Applicant's Molar Cleaning Apparatus can include a jet device configured to form a liquid jet beam at a pressure of about 9000 psi, +/- about 1000 psi. The jet can be formed by passing pressurized liquid through a nozzle having a diameter of about 63 microns, +/- about 5 microns. In general, the parameters for the nozzle and guide tube can be similar to those described in U.S. Patent Publication No. 2012/0237893 and U.S. Patent Publication No. 2011/0117517 such that a coherent, collimated jet with a length of at least about 1 mm is produced. The plot in the upper right corner is a measure of voltage output over time for systems disclosed in this Application that are adapted to clean a pre-molar tooth (referred to herein as "Applicant's Pre-Molar Cleaning Apparatus"). In Applicant's Pre-Molar Cleaning Apparatus, a jet similar to the one described for the Molar Cleaning Apparatus can be used. The jet device for the Pre-Molar Cleaning Apparatus can be used in conjunction with a pre-molar handpiece such as the one illustrated in Figure 10B. The plot in the lower left corner is a measure of voltage output over time for a Fotona photon induced photoacoustic streaming (PIPS®) device. The plot in the lower right corner is a measure of voltage output over time for a Piezon® Master ultrasonic device.
As shown in Figure 11B, Applicant's Molar and Pre-Molar Cleaning Apparatuses generate a voltage output (representative of power) over time that includes multiple frequencies. Indeed, as shown in Figure 11B, Applicant's Molar and Pre-Molar Cleaning Apparatuses can generate a signal including a significant amount of noise. For example, the frequencies in the signal may include multiple, substantially random frequencies (e.g., approximating white noise in some arrangements). By contrast, the signal produced by the PIPS device includes pulses generated at substantially regular intervals, and the signal produced by the ultrasonic device can include a substantially periodic signal, e.g., one frequency, or only a few frequencies. As explained herein, the broadband signals generated by Applicant's Molar and Pre-Molar Apparatuses can advantageously clean different types of materials from the tooth and can do so quickly and effectively. For example, different frequencies may clean different types and/or sizes of materials effectively.
Figure 12A illustrates images of root canals that compare the use of non-degassed liquid and degassed liquid in the disclosed pressure wave generators. As shown in image 1201 on the left side of Figure 12A, the use of non-degassed liquid may cause bubbles to form in the canals, which may inhibit the propagation of energy in some arrangements. As shown in image 1202 on the right side of Figure 12A, the use of degassed liquid may substantially prevent the formation of bubbles in the root canals when exposed to broadband acoustic or pressure waves. Figure 12B is a plot comparing the power output for techniques using non-degassed and degassed liquids. The power outputs plotted in Figure 12B are measured based on the liquid jet device described above with respect to Applicant's Molar Cleaning Apparatus. As shown in Figure 12B, at higher acoustic frequencies, the use of degassed liquid in the disclosed systems can generate significantly more power than in techniques using non-degassed liquid. As illustrated in Figure 12B, for example, at high acoustic frequencies, the difference between power generated by degassed and non-degassed liquids can be given by ΔP, which can be in a range of about 5 dB to about 25 dB for frequencies in a range of about 20 kHz to about 200 kHz. For example, for frequencies in a range of about 70 kHz to about 200 kHz, ΔP can be in a range of about 10 dB to about 25 dB. At lower frequencies, the differences in power generated by degassed and non-degassed techniques may not be noticeable. At lower frequencies, relatively high powers may be generated even with non-degassed liquid because low frequency, large-scale fluid motion may produce substantial momentum that contributes to the cleaning of the tooth.
Figure 13 is a plot comparing the rates of tissue dissolution (in units of % per second) for Applicant's device versus other devices, for different treatment fluids and compositions. As used herein, the data labeled "Applicant's system" was obtained from a system similar to that described above in relation to Applicant's Molar Cleaning Apparatus. In Figure 13, the plot compares tissue dissolution rates for pure water, 0.5% NaOCl, 3% NaOCl, and 6% NaOCl. For example, Figure 13 compares tissue dissolution rates at room temperature for Applicant's device, a 27G irrigation needle supplying irrigation fluid at a rate of 10 mL/min, an activated Piezon Master device, an activated Piezon Master Agitation in addition to some fluid irrigation, and an activated PIPS device. As shown in Figure 13, for each treatment fluid and concentration, Applicant's system cleans at substantially higher rates than the other tested devices. For example, tissue dissolution rates for each treatment solution using Applicant's system may be at least 8-10 times the dissolution rates for the other tested devices.
Figures 14A-14B are plots relating to the pressure measured at or near the apical opening of the root canal during treatment. As used herein, the data labeled "Applicant's system" was obtained from a system similar to that described above in relation to Applicant's Molar Cleaning Apparatus. As explained herein, it should be appreciated that high apical pressures can harm the patient. For example, high apical pressures can cause fluid or other material to extrude through the apex and into the patient's jaw. Extrusion through the apex can cause the patient substantial pain and can cause various health problems. Accordingly, it can be desirable for endodontic treatments to have low or negative apical pressures. Figure 14A is a plot of mean apical pressure versus the hand file size used to enlarge the apex. As shown in Figure 14A, Applicant's system generates negative pressures for each file size. Such negative pressures can advantageously prevent extrusion through the apex. For example, as explained above, the induced vortices can cause the pressures at or near the apical opening to be slightly negative. For example, the mean apical pressures can be in a range of about -5 mmHG to about -15 mmHg.
Figure 14B is a plot comparing the apical pressures during treatments using Applicant's system and various other devices, such as various sizes of and flow rates dispensed from open-vented needles. The plot of Figure 14B includes data for a distobuccal canal, and the plot compares the pressures for different amounts of canal shaping (e.g., no shaping, minimal shaping, traditional shaping, apical enlargement). As shown in Figure 14B, Applicant's techniques and systems produce negative apical pressures, as compared to the high, positive apical pressures generated by the other plotted devices.
The negative apical pressures generated by Applicant's systems can advantageously improve patient outcomes by preventing and/or reducing extrusion of materials through the apex. Figure 14C is a plot of the mass of material extruded through the apex for various simulated peri-apical pressures for Applicant's system and for various needles. As used herein, the data labeled "Applicant's system" was obtained from simulations of a system similar to that described above in relation to Applicant's Molar Cleaning Apparatus. As shown in Figure 14C, the mass of material extruded when Applicant's system and methods are used to clean canals is less than that of other devices. Indeed, the disclosed systems and methods can clean root canals with minimal or no material extruded through the apex.
Although the tooth schematically depicted in some of the figures is a pre-molar, the procedures can be performed on any type of tooth such as an incisor, a canine, a bicuspid, a pre-molar, or a molar. Further, although the tooth may be depicted as a lower (mandibular) tooth in the figures, this is for purposes of illustration, and is not limiting. The systems, methods, and compositions can be applied to lower (mandibular) teeth or upper (maxillary) teeth. Also, the disclosed apparatus and methods are capable of any portions of a tooth, including interior spaces such as root canals, pulp cavity, etc., and/or exterior surfaces of the tooth. Moreover, the disclosed apparatus, methods, and compositions can be applied to to human teeth (including juvenile teeth) and/or to animal teeth.
Reference throughout this specification to "some embodiments" or "an embodiment" means that a particular feature, structure, element, act, or characteristic described in connection with the embodiment is included in at least one embodiment. Thus, appearances of the phrases "in some embodiments" or "in an embodiment" in various places throughout this specification are not necessarily all referring to the same embodiment and may refer to one or more of the same or different embodiments. Furthermore, the particular features, structures, elements, acts, or characteristics may be combined in any suitable manner (including differently than shown or described) in other embodiments. Further, in various embodiments, features, structures, elements, acts, or characteristics can be combined, merged, rearranged, reordered, or left out altogether. Thus, no single feature, structure, element, act, or characteristic or group of features, structures, elements, acts, or characteristics is necessary or required for each embodiment. All possible combinations and subcombinations are intended to fall within the scope of this disclosure.
As used in this application, the terms "comprising," "including," "having," and the like are synonymous and are used inclusively, in an open-ended fashion, and do not exclude additional elements, features, acts, operations, and so forth. Also, the term "or" is used in its inclusive sense (and not in its exclusive sense) so that when used, for example, to connect a list of elements, the term "or" means one, some, or all of the elements in the list.
Similarly, it should be appreciated that in the above description of embodiments, various features are sometimes grouped together in a single embodiment, figure, or description thereof for the purpose of streamlining the disclosure and aiding in the understanding of one or more of the various inventive aspects. This method of disclosure, however, is not to be interpreted as reflecting an intention that any claim require more features than are expressly recited in that claim. Rather, inventive aspects lie in a combination of fewer than all features of any single foregoing disclosed embodiment.
The foregoing description sets forth various example embodiments and other illustrative, but non-limiting, embodiments of the inventions disclosed herein. The description provides details regarding combinations, modes, and uses of the disclosed inventions. Other variations, combinations, modifications, equivalents, modes, uses, implementations, and/or applications of the disclosed features and aspects of the embodiments are also within the scope of this disclosure, including those that become apparent to those of skill in the art upon reading this specification. Additionally, certain objects and advantages of the inventions are described herein. It is to be understood that not necessarily all such objects or advantages may be achieved in any particular embodiment. Thus, for example, those skilled in the art will recognize that the inventions may be embodied or carried out in a manner that achieves or optimizes one advantage or group of advantages as taught herein without necessarily achieving other objects or advantages as may be taught or suggested herein. Also, in any method or process disclosed herein, the acts or operations making up the method or process may be performed in any suitable sequence and are not necessarily limited to any particular disclosed sequence.
Embodiments, not forming part of the invention, will now be summarized in the following numbered paragraphs. The invention is defined by the claims.
1. 1. An apparatus for treating a tooth, the apparatus comprising:
  - a chamber having an access port which places the chamber in fluid communication with a treatment region of the tooth when the chamber is coupled to tooth;
  - a fluid motion generator coupled to the chamber, the fluid motion generator configured to direct fluid across the access port to generate fluid motion in the chamber.
2. 2. The apparatus of paragraph 1, wherein the apparatus is configured to clean a root canal of the tooth when the chamber is in fluid communication with a chamber of the root canal, the root canal having a central axis, and wherein the fluid motion generator is configured to direct fluid across the access port in a direction substantially perpendicular to the central axis of the root canal.
3. 3. The apparatus of any one of paragraphs 1 to 2, wherein the apparatus is configured to clean a root canal of the tooth when the chamber is in fluid communication with a chamber of the root canal, the root canal having a central axis, and wherein the fluid motion generator is configured to rotate the fluid about an axis transverse to the central axis of the root canal.
4. 4. The apparatus of paragraph 1, wherein the apparatus is configured to clean a root canal of the tooth when the chamber is in fluid communication with the root canal, the root canal having a central axis, and wherein the fluid motion generator is configured to rotate the fluid about the central axis of the root canal.
5. 5. The apparatus of any one of paragraphs 1 to 4, wherein the access port has a diameter that is at least as large as a diameter of an access opening of the tooth.
6. 6. The apparatus of paragraph 5, wherein the access port has a diameter that is about the same size as the access opening.
7. 7. The apparatus of any one of paragraphs 1 to 5, wherein the fluid motion generator is configured to generate a chaotic fluid flow in the chamber.
8. 8. The apparatus of any one of paragraphs 1 to 7, wherein the fluid motion generator is configured to generate a planar flow in the chamber.
9. 9. The apparatus of any one of paragraphs 1 to 8, wherein the apparatus is configured to clean a root canal of the tooth when the chamber is in fluid communication with the root canal, and wherein the fluid motion generator is configured to generate a swirling flow in the chamber with an axis of rotation of the swirl substantially aligned with a central axis of the root canal.
10. 10. The apparatus of paragraphs 9, wherein the fluid motion generator is configured to generate a plurality of swirling flows in the chamber with the axis of rotation of the swirl substantially parallel to the axis of the root canal.
11. 11. The apparatus of any one of paragraphs 1 to 10, wherein the apparatus is configured to clean a treatment region at or near an exterior surface of the tooth, and wherein the chamber is configured to couple to the tooth over the treatment region.
12. 12. The apparatus of any one of paragraphs 1 to 11, wherein the fluid comprises a flowable obturation material, and wherein, when activated, the fluid motion generator is configured to fill a treatment region of the tooth with the flowable obturation material.
13. 13. The apparatus of paragraph 12, wherein the fluid motion generator is configured to fill substantially an entire root canal system of the tooth using the fluid motion.
14. 14. The apparatus of any one of paragraphs 1 to 13, wherein the access port defines a proximal-most plane, and wherein the fluid motion generator is configured to direct the fluid substantially parallel to the proximal-most plane.
15. 15. The apparatus of paragraph 14, wherein the fluid motion generator is configured such that the momentum of the fluid is in a direction substantially parallel to the proximal-most plane.
16. 16. The apparatus of any one of paragraphs 1 to 15, wherein the fluid motion generator is configured to direct fluid in a direction substantially perpendicular to a central axis of the access port.
17. 17. The apparatus of any one of paragraphs 1 to 16, wherein the fluid motion generator is further configured to generate pressure waves through the fluid having energy sufficient to substantially clean the tooth.
18. 18. The apparatus of any one of paragraphs 1 to 17, wherein the fluid motion generator is configured to generate rotational motion having energy sufficient to generate rotational flow inside a root canal to substantially clean the root canal.
19. 19. The apparatus of any one of paragraphs 1 to 18, wherein the fluid motion generator comprises a liquid jet device.
20. 20. The apparatus of paragraph 19, wherein the liquid jet device is configured to substantially clean the tooth using liquid that is substantially free of dissolved gases.
21. 21. The apparatus of any one of paragraphs 1 to 20, wherein the fluid motion generator is configured to generate acoustic power having multiple frequencies.
22. 22. The apparatus of paragraph 21, wherein the fluid motion generator is configured to generate acoustic power having a substantially white noise distribution of frequencies.
23. 23. The apparatus of any one of paragraph 1 to 22, wherein the fluid motion generator is disposed along a wall of the chamber between the wall and the access port.
24. 24. The apparatus of any one of paragraph 1 to 23, further comprising an obturation material configured to fill a root canal of the tooth.
25. 25. The apparatus of any one of paragraph 1 to 25, further comprising a plurality of fluid motion generators eccentrically positioned relative to a central axis of the access port, the plurality of fluid motion generators configured to generate a swirl motion in the chamber.
26. 26. The apparatus of any one of paragraph 25, wherein a first fluid motion generator is configured to generate swirl in a first direction, and wherein a second fluid motion generator is configured to generate swirl in a second direction opposite the first direction.
27. 27. An apparatus for treating a tooth, the apparatus comprising:
  - a chamber configured to couple to a tooth; and
  - a fluid motion generator disposed in the chamber and configured to generate a rotational motion of fluid in the chamber,
  - wherein when the chamber is coupled to the tooth, the fluid motion generator is positioned outside the tooth.
28. 28. The apparatus of paragraph 27, wherein the apparatus is configured to clean a root canal of the tooth, the root canal having a central axis, and wherein the fluid motion generator is configured to generate the rotational motion about an axis transverse to the central axis of the root canal.
29. 29. The apparatus of paragraph 27, wherein the apparatus is configured to clean a root canal of the tooth, the root canal having a central axis, and wherein the fluid motion generator is configured to generate the rotational motion about the central axis.
30. 30. The apparatus of any one of paragraphs 27 to 29, wherein the apparatus is configured to clean a treatment region at or near an exterior surface of the tooth, and wherein the chamber is configured to couple to the tooth over the treatment region.
31. 31. The apparatus of any one of paragraphs 27 to 30, wherein the fluid comprises a flowable obturation material, and wherein, when activated, the fluid motion generator is configured to fill a treatment region of the tooth with the flowable obturation material.
32. 32. The apparatus of paragraph 31, wherein the fluid motion generator is configured to fill substantially an entire root canal system of the tooth using the rotational motion of the fluid.
33. 33. The apparatus of any one of paragraphs 27 to 32, wherein the chamber comprises an access port configured to provide fluid communication with the tooth, and wherein the fluid motion generator is configured to direct fluid in a direction substantially perpendicular to a central axis of the access port.
34. 34. The apparatus of any one of paragraphs 27 to 33, wherein the chamber includes an access port such that, when the chamber is coupled to the tooth, the access port is proximate an access opening of the tooth.
35. 35. The apparatus of paragraph 34, wherein the access port has a diameter that is at least as large as a diameter of the access opening.
36. 36. The apparatus of any one of paragraphs 27 to 35, wherein the fluid motion generator is configured to pass a stream of the fluid across an access port of the chamber.
37. 37. The apparatus of paragraphs 36, wherein the access port defines a proximal-most plane, and wherein the fluid motion generator is configured to pass the stream of fluid substantially parallel to the proximal-most plane.
38. 38. The apparatus of paragraphs 37, wherein the fluid motion generator is configured such that the momentum of the stream is in a direction substantially parallel to the proximal-most plane.
39. 39. The apparatus of any one of paragraphs 27 to 38, wherein the fluid motion generator is further configured to generate acoustic waves through the fluid having energy sufficient to substantially clean the tooth.
40. 40. The apparatus of any one of paragraphs 27 to 39, wherein the fluid motion generator comprises a liquid jet device.
41. 41. The apparatus of paragraph 40, wherein the liquid jet device is configured to substantially clean the tooth using liquid that is substantially free of dissolved gases.
42. 42. The apparatus of any one of paragraphs 27 to 41, wherein the fluid motion generator is configured to generate acoustic power having multiple frequencies.
43. 43. The apparatus of paragraph 42, wherein the fluid motion generator is configured to generate acoustic power having a substantially white noise distribution of frequencies.
44. 44. The apparatus of any one of paragraphs 27 to 43, wherein the fluid motion generator is disposed near a wall of the chamber between the wall and an access port of the chamber.
45. 45. The apparatus of any one of paragraphs 27 to 44, further comprising an obturation material configured to fill a root canal of the tooth.
46. 46. The apparatus of any one of paragraphs 26 to 45, wherein the fluid motion generator is configured to generate a chaotic fluid flow in the chamber.
47. 47. The apparatus of any one of paragraphs 27 to 46, wherein the fluid motion generator is configured to generate a planar flow in the chamber.
48. 48. The apparatus of paragraph 27, wherein the apparatus is configured to clean a root canal of the tooth when the chamber is in fluid communication with the root canal, and wherein the fluid motion generator is configured to generate a swirling flow in the chamber with an axis of rotation of the swirl substantially aligned with a central axis of the root canal.
49. 49. The apparatus of paragraph 48, wherein the fluid motion generator is configured to generate a plurality of swirling flows in the chamber with the axis of rotation of the swirl substantially parallel to the axis of the root canal.
50. 50. The apparatus of paragraph 27, further comprising a plurality of fluid motion generators eccentrically positioned relative to a central axis of the access port, the plurality of fluid motion generators configured to generate a swirl motion in the chamber.
51. 51. The apparatus of paragraph 50, wherein a first fluid motion generator is configured to generate swirl in a first direction, and wherein a second fluid motion generator is configured to generate swirl in a second direction opposite the first direction.
52. 52. A method of treating a tooth, the method comprising:
  - positioning a fluid motion generator near an access opening of the tooth;
  - activating the fluid motion generator to pass a stream of fluid across the access opening of the tooth; and
  - generating fluid motion at a treatment region of the tooth.
53. 53. The method of paragraph 52, wherein generating fluid motion comprises generating fluid motion in a root canal of the tooth.
54. 54. The method of paragraph 52, wherein generating fluid motion comprises generating fluid motion at or near a carious region of the tooth.
55. 55. The method of paragraph 52, wherein positioning the fluid motion generator comprises positioning the fluid motion generator outside the tooth.
56. 56. The method of paragraph 55, wherein the fluid motion generator is disposed in a chamber, and wherein positioning the fluid motion generator comprises coupling the chamber to the tooth.
57. 57. The method of paragraph 56, wherein activating the fluid motion generator comprises generating rotational motion of the fluid in the chamber.
58. 58. The method of paragraph 57, wherein activating the fluid motion generator comprises generating the rotational motion about an axis transverse to a central axis of a root canal of the tooth.
59. 59. The method of paragraph 52, wherein the access opening of the tooth is in communication with an access port of the chamber, and wherein activating the fluid motion generator comprises passing the stream of fluid along a direction substantially parallel to a proximal-most plane of the access port.
60. 60. The method of paragraph 52, wherein the access opening of the tooth is in communication with an access port of the chamber, and wherein activating the fluid motion generator comprises passing the stream of fluid along a direction substantially perpendicular to a central axis of the access port.
61. 61. The method of paragraph 52, wherein the fluid comprises a flowable obturation material, the method further comprising activating the fluid motion generator to substantially fill the treatment region.
62. 62. The method of paragraph 61, further comprising activating the fluid motion generator to substantially fill a root canal of the tooth.
63. 63. The method of paragraph 52, wherein the fluid comprises a treatment fluid, the method further comprising activating the fluid motion generator to substantially clean the treatment region.
64. 64. The method of paragraph 52, wherein generating fluid motion at the treatment region comprises generating vortices in a root canal.
65. 65. The method of paragraph 64, wherein generating vortices comprises generating vortices substantially through the entire root canal.
66. 66. The method of paragraph 52, wherein generating fluid motion at the treatment region comprises generating a swirl motion in a root canal.
67. 67. The method of paragraph 66, further comprising generating two opposing counter-swirl motions in the chamber.
68. 68. A method of treating a tooth, the method comprising:
  - coupling a chamber to the tooth, the chamber having a fluid motion generator disposed therein, the fluid motion generator disposed outside the tooth; and
  - activating the fluid motion generator to generate a rotational motion of fluid in the chamber.
69. 69. The method of paragraph 68, wherein activating the fluid motion generator comprises generating the rotational motion about an axis transverse to a central axis of a root canal of the tooth.
70. 70. The method of paragraph 68, wherein activating the fluid motion generator comprises generating the rotational motion about a central axis of a root canal of the tooth.
71. 71. The method of paragraph 68, further comprising:
  - coupling the chamber to an exterior surface of the tooth over a treatment region on or near an exterior surface of the tooth; and
  - activating the fluid motion generator to clean the treatment region on or near the exterior surface of the tooth.
72. 72. The method of paragraph 68, wherein the fluid comprises a flowable obturation material, the method further comprising activating the fluid motion generator to substantially fill a treatment region of the tooth.
73. 73. The method of paragraph 68, wherein activating the fluid motion generator comprises passing a stream of the fluid across an access opening formed in the tooth.
74. 74. The method of paragraph 73, wherein the access opening comprises a proximal-most plane, and wherein passing the stream of the fluid comprises passing the stream of fluid substantially parallel to the proximal-most plane.
75. 75. The method of paragraph 68, wherein activating the fluid motion generator comprises activating a liquid jet device.
76. 76. The method of paragraph 75, wherein activating the liquid jet device comprises forming a liquid jet beam comprising liquid that is substantially free of dissolved gases.
77. 77. The method of paragraph 68, wherein activating the fluid motion generator comprises generating acoustic power having multiple frequencies.
78. 78. The method of paragraph 77, wherein generating acoustic power having multiple frequencies comprises generating acoustic power having a substantially white noise distribution of frequencies.
79. 79. The method of paragraph 68, further comprising filling a root canal of the tooth with an obturation material.
80. 80. An apparatus for treating a tooth, the apparatus comprising:
  - a chamber configured to couple to a tooth; and
  - a fluid motion generator disposed in the chamber and configured to generate a rotational motion of fluid in the chamber.
81. 81. The apparatus of paragraph 80, wherein when the chamber is coupled to the tooth, the fluid motion generator is positioned outside the tooth.
82. 82. The apparatus of any one of paragraphs 80 to 81, wherein the apparatus is configured to clean a root canal of the tooth, the root canal having a central axis, and wherein the fluid motion generator is configured to generate the rotational motion about an axis transverse to the central axis of the root canal.
83. 83. The apparatus of any one of paragraphs 80 to 82, wherein the chamber includes an access port such that, when the chamber is coupled to the tooth, the access port is proximate an access opening of the tooth.
84. 84. The apparatus of paragraph 83, wherein the access port has a diameter that is at least as large as a diameter of the access opening.
85. 85. The apparatus of any one of paragraphs 83 to 84, wherein the fluid motion generator is configured to pass a stream of the fluid across the access port of the chamber.
86. 86. The apparatus of paragraph 85, wherein the access port is disposed along a major axis, and wherein the fluid motion generator is configured to pass the stream of fluid substantially parallel to the major axis.
87. 87. The apparatus of paragraph 86, wherein the fluid motion generator is configured such that the momentum of the stream is in a direction substantially parallel to the major axis.
88. 88. The apparatus of any one of paragraphs 80 to 87, wherein the fluid motion generator is further configured to generate acoustic waves through the fluid having energy sufficient to substantially clean the tooth.
89. 89. The apparatus of any one of paragraphs 80 to 88, wherein the fluid motion generator comprises a liquid jet device.
90. 90. The apparatus of paragraph 89, wherein the liquid jet device is configured to substantially clean the tooth using liquid that is substantially free of dissolved gases.
91. 91. The apparatus of any one of paragraphs 80 to 90, wherein the fluid motion generator is configured to generate acoustic power having multiple frequencies.
92. 92. The apparatus of paragraph 91, wherein the fluid motion generator is configured to generate acoustic power having a substantially white noise distribution of frequencies.
93. 93. The apparatus of any one of paragraphs 80 to 92, wherein the fluid motion generator is disposed along a wall of the chamber between the wall and an access port of the chamber.
94. 94. The apparatus of any one of paragraphs 80 to 93, further comprising an obturation material configured to fill a root canal of the tooth.
95. 95. An apparatus for treating a tooth, the apparatus comprising:
  - a chamber configured to couple to the tooth; and
  - a plurality of fluid motion generators disposed in the chamber.
96. 96. The apparatus of paragraph 95, wherein each fluid motion generator of the plurality of fluid motion generators is configured to propagate acoustic waves through the chamber at a different frequency.
97. 97. The apparatus of any one of paragraphs 95 to 96, wherein the plurality of fluid motion generators are coupled to a wall of the chamber.
98. 98. The apparatus of any one of paragraphs 95 to 97, further comprising a first fluid motion generator disposed along a top wall of the chamber and a second fluid motion generator disposed along a side wall of the chamber.
99. 99. The apparatus of any one of paragraphs 95 to 98, further comprising a plurality of fluid motion generators disposed along a top wall of the chamber.
100. 100. The apparatus of any one of paragraphs 95 to 99, further comprising a fluid outlet configured to supply fluid into the chamber.
101. 101. The apparatus of any one of paragraphs 95 to 100, further comprising a fluid outlet configured to transport fluid out of the chamber.
102. 102. The apparatus of any one of paragraphs 95 to 101, wherein the plurality of fluid motion generators comprises at least one of a liquid jet device, a laser, a piezoelectric transducer, and a stirring element.
103. 103. The apparatus of any one of paragraphs 95 to 102, further comprising a controller in electronic communication with the plurality of fluid motion generators, the controller configured to:
  - select a fluid motion generator based at least in part on a treatment phase of a cleaning procedure; and
  - activate the selected fluid motion generator at a frequency associated with the treatment phase of the cleaning procedure.
104. 104. A method for treating a tooth, the method comprising:
  - coupling a chamber to the tooth, the chamber including a plurality of fluid motion generators disposed therein; and
  - activating the plurality of fluid motion generators to clean the tooth.
105. 105. The method of Claim 104, further comprising selecting a fluid motion generator based at least in part on a treatment phase of a cleaning procedure.
106. 106. The method of Claim 105, further comprising activating the selected fluid motion generator at a frequency associated with the treatment phase of the cleaning procedure.
107. 107. The method of any one of paragraphs 104 to 105, further comprising filling a root canal of the tooth with an obturation material.
108. 108. A method for treating a tooth, the method comprising:
  - forming an access opening in the tooth;
  - applying a tooth seal around a perimeter of the access opening, the tooth seal having a peripheral boundary; and
  - positioning a chamber within the peripheral boundary of the tooth seal to secure the chamber to the tooth seal.
109. 109. The method of Claim 108, further comprising defining a locking wall along the periphery of the tooth seal, the locking wall extending upwardly relative to the tooth.
110. 110. The method of Claim 109, further comprising positioning the chamber within an area formed by the locking wall to secure the chamber to the tooth seal.
111. 111. The method of any one of paragraphs 108 to 110, wherein the chamber comprises a mating tube extending outwardly from the chamber and surrounding an access port of the chamber, the method further comprising positioning the mating tube within the access opening of the tooth.
112. 112. The method of any one of paragraphs 108 to 111, wherein applying the tooth seal comprises applying the tooth seal along a concave surface, and wherein positioning the chamber comprises coupling a curved distal end portion of the chamber to the concave surface.
113. 113. The method of paragraphs 112, further comprising rotating the curved distal end portion along the concave surface to position the chamber at a desired orientation.
114. 114. The method of any one of paragraphs 108 to 112, wherein a fluid motion generator is coupled to the chamber, the method further comprising activating the fluid motion generator to clean the tooth.
115. 115. The method of any one of paragraphs 108 to 114, further comprising filling a root canal of the tooth with an obturation material.
1. An apparatus for treating a tooth, the apparatus comprising:
a chamber (6) to be positioned against a tooth; and
a fluid motion generator coupled to the chamber (6) and configured to generate a rotational motion of fluid in the chamber (6),
wherein when the chamber is positioned against the tooth, the fluid motion generator is positioned outside the tooth.
2. The apparatus of Claim 1, wherein the apparatus is configured to clean a root canal of the tooth, the root canal having a central axis, and wherein the fluid motion generator is configured to generate the rotational motion about an axis transverse to the central axis of the root canal.
3. The apparatus of Claim 1, wherein the apparatus is configured to clean a root canal of the tooth, the root canal having a central axis, and wherein the fluid motion generator is configured to generate the rotational motion about the central axis.
4. The apparatus of any one of Claims 1 to 3, wherein the apparatus is configured to clean a treatment region at or near an exterior surface of the tooth, and wherein the chamber is configured to couple to the tooth over the treatment region.
5. The apparatus of any one of Claims 1 to 4, wherein the fluid comprises a flowable obturation material, and wherein, when activated, the fluid motion generator is configured to fill a treatment region of the tooth with the flowable obturation material.
6. The apparatus of any one of Claims 1 to 5, wherein the chamber comprises an access port configured to provide fluid communication with the tooth, and wherein the fluid motion generator is configured to direct fluid in a direction substantially perpendicular to a central axis of the access port.
7. The apparatus of any one of Claims 1 to 6, wherein the fluid motion generator is configured to pass a stream of the fluid across an access port of the chamber.
8. The apparatus of Claim 7, wherein the access port defines a proximal-most plane, and wherein the fluid motion generator is configured to pass the stream of fluid substantially parallel to the proximal-most plane.
9. The apparatus of Claim 8, wherein the fluid motion generator is configured such that the momentum of the stream is in a direction substantially parallel to the proximal-most plane.
10. The apparatus of any one of Claims 1 to 9, wherein the fluid motion generator is further configured to generate acoustic waves through the fluid having energy sufficient to substantially clean the tooth.
11. The apparatus of any one of Claims 1 to 10, wherein the fluid motion generator comprises a liquid jet device.
12. The apparatus of Claim 11, wherein the liquid jet device is configured to substantially clean the tooth using liquid that is substantially free of dissolved gases.
13. The apparatus of any one of Claims 1 to 12, wherein the fluid motion generator is configured to generate acoustic power having multiple frequencies.
14. The apparatus of Claim 13, wherein the fluid motion generator is configured to generate acoustic power having a substantially white noise distribution of frequencies.
15. The apparatus of any one of Claims 1 to 14, wherein the fluid motion generator is disposed near a wall of the chamber between the wall and an access port of the chamber.
16. The apparatus of any one of Claims 1 to 15, wherein the fluid motion generator is configured to generate a chaotic fluid flow in the chamber.
17. The apparatus of any one of Claims 1 to 16, wherein the apparatus is configured to clean a root canal of the tooth when the chamber is in fluid communication with the root canal, and wherein the fluid motion generator is configured to generate a swirling flow in the chamber with an axis of rotation of the swirl substantially aligned with a central axis of the root canal.
P1883EP02
EP
21175783.6
SONENDO, INC.
1a
MN
20211213
A61C
US
2012237893
A1
BERGHEIM BJARNE [US] ET AL
20120920
X
1-17
* figures 3a-5d *
* figures 7-10a *
* the whole document *
US
6245032
B1
SAUER MICHAEL [DE] ET AL
20010612
X
1-4,6-9,11,16,17
* the whole document *
US
2001055742
A1
HOOD LARRY L [US] ET AL
20011227
X
1-4,6-9,11,16,17
* figures 16-20 *
* the whole document *
Salvatore, Claudio
Munich
20211202
US
2012237893
A1
20120920
AU
2011316839
A1
20130502
BR
112013009708
A2
20160719
CA
2815219
A1
20120426
CN
103347462
A
20131009
CN
107115154
A
20170901
EP
2629693
A2
20130828
EP
3808306
A1
20210421
IL
225829
A
20180830
IL
261307
A
20200730
JP
6241997
B2
20171206
JP
2013544120
A
20131212
JP
2018038846
A
20180315
JP
2020006220
A
20200116
US
2012237893
A1
20120920
US
2018116761
A1
20180503
US
2020038140
A1
20200206
US
2021068921
A1
20210311
WO
2012054905
A2
20120426
US
6245032
B1
20010612
AT
213137
T
20020215
DE
19645644
A1
19980507
EP
0841038
A1
19980513
US
6245032
B1
20010612
US
2001055742
A1
20011227
NONE

REFERENCES CITED IN THE DESCRIPTION
This list of references cited by the applicant is for the reader's convenience only. It does not form part of the European patent document. Even though great care has been taken in compiling the references, errors or omissions cannot be excluded and the EPO disclaims all liability in this regard.

Patent documents cited in the description
- US
61740351
20121220
[0001]
- US
61907345
20131121
[0001]
- US
20110117517
A
20110519
[0066]
[0084]
[0141]
[0205]
[0205]
- US
20120237893
A
20120920
[0066]
[0079]
[0084]
[0085]
[0086]
[0087]
[0089]
[0141]
[0205]
[0205]