ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRIS..MTNORSMESMMAKHTNMD..........
J
BDM Ver 2.0.24 - 1100000/0
4250260
EUROPEAN PATENT APPLICATION
A1
20230927
EP
22460019.7
20220322
20230615
en
en
en
20230927
202339
20230927
202339
G07F 11/10 20060101AFI20220906BHEP
G07F 11/16 20060101ALI20220906BHEP
G07F 11/32 20060101ALI20220906BHEP
G07F 11/42 20060101ALI20220906BHEP
G07F 11/58 20060101ALI20220906BHEP
G07F 11/165 20130101 FI20220901BHEP
G07F 11/58 20130101 LI20220901BHEP
G07F 11/42 20130101 LI20220901BHEP
G07F 11/32 20130101 LI20220901BHEP
G07F 11/10 20130101 LI20220901BHEP
G07F 11/1653 20200501 LI20220901BHEP
de
VERKAUFSAUTOMAT
en
VENDING MACHINE
fr
DISTRIBUTEUR AUTOMATIQUE
3
Delfin Spolka z o.o. Spolka Komandytowa
101945113
0222/EP/03/22
Ul.Oswiecimska 52
32-651 Nowa Wies
PL
Piecha, Mariusz
32-651 NOWA WIES
PL
Karczmitowicz, Teresa Ewa
101843725
Kancelaria Prawa Wlasnosci Przemyslowej Ul. Wroclawska 33 lok. A4
30-011 Kraków
PL
AL
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HR
HU
IE
IS
IT
LI
LT
LU
LV
MC
MK
MT
NL
NO
PL
PT
RO
RS
SE
SI
SK
SM
TR
BA
ME
KH
MA
MD
TN
A vending machine comprises a store space (1), a confectioning zone (2), a shopping basket (3), an issuing chamber (4), and a control unit (5). At least the store space (1) and the confectioning zone (2) are enclosed in a thermostatic housing (6). The store space (1) may consist of first store space (1A) and second store space (1B) located on opposite sides of the confectioning zone (2). The store space (1) is divided into compartments (10) each having essentially vertical side walls (11). At least one compartment (10) has an essentially horizontal belt conveyor (12) consisting of a driving roller (13) ended with a slave gear (14), an idle roller (15), an endless belt (16) and a belt tensioner (17). The confectioning zone (2) has a movable confectioning unit (20) comprising a frame (21) movable in horizontal direction X along the front side of the store space (1), and a platform (22) movable on the frame (21) in vertical direction Z in front of the store space (1). The platform (22) is equipped with at least one actuator (23) fitted with a master gear (24) capable of meshing with the slave gear (14). The actuator (23) is coupled with the master gear (24) through an endless toothed belt (29) and is controlled by the control unit (5). The platform (22) is movable in horizontal direction Y perpendicular to direction X towards the front side of the store space (1) to mesh the master gear (24) with the slave gear (14) and back to release the meshing. The basket (3) for collecting items supplied from the store space (1) is fixed on the platform (22). The movements of the frame (21) in horizontal direction X, and of the platform (22) in directions Y and Z are executed by the X-actuator (25), Y-actuator (26), and Z-actuator (27) respectively, controlled by the control unit (5). Servo motors may be used for the actuators (23, 25, 26, 27). The master gear (24) and the slave gear (14) may be double helical gears. At least one compartment (10) is equipped with an auger conveyor (18). The basket (3) has an openable bottom (31) to release the collected items into the issuing chamber (4). The issuing chamber (4) may have an openable bottom (41) to release the collected items into the repository in case of cancelled confectioning.
The present invention relates to a vending machine which can be used indoors and outdoors for self-service shopping of packaged commodities, in particular ready-made food products packaged in bags, boxes, cans, bottles, etc. Unpackaged items may also be sold as long as their shape or size does not block the device.
Most of commonly used vending machines are based on auger and/or belt conveyors operating in a step-wise manner where one step means delivery of a single item if the payment was internally confirmed in a checking module. In more sophisticated apparatuses a buyer can select several products from a menu displayed on a touch screen while paying once. When the list of selected items is ended and a transaction of payment completed, the products are delivered one by one to a dispensing compartment or a drawer which then may be opened only after completing the entire operation.
In the known vending appliances each auger or belt conveyor is set in motion by its own motor being a part of the conveyor. The conveyors are often tiled side by side, several in one cassette thus making the standardized modules easy to arrange in the vending device. The cassettes may be stacked in larger modules. Whether separate or arranged in the module every conveyor has its own motor. In consequence, each motor must be separately driven and controlled from the control unit. The proposed invention offers different approach to the paradigm of driving individual conveyors.
The technical problem of transporting the purchased commodity from the conveyor into a dispensing chamber is solved in various ways. In smaller machines the item is dropped and directed into the dispensing chamber or drawer by gravity, directly or on a chute. In bigger vending appliances this may require additional driving of the item by specialized units.
Chinese utility model application CN210377657 U (Henan Huiquhuina Intelligent Tech. Co. Ltd., CN; publ. 2020-04-21) discloses a cassette comprising a number of the belt conveyors to be applied in a vending machine. The cassette has a base body with sliding rails fixedly connected to its two sides, and is connected to first motor which is arranged on rear side of the base body. An output shaft of first motor is in transmission connection with a screw rod which penetrates through a fixed block mounted to the underside of the cassette, and is in threaded connection with the fixed block. Plurality of baffles are fixed to the base body at intervals which divide the interior of the base body into a plurality of material conveying units. In each unit a conveying frame is fixed to the base body, conveying belts are arranged on the conveying frames, and driving mechanisms comprising second motors are correspondingly driving the conveying belts. A push plate is mounted on each conveying belt.
According to another Chinese utility model application CN209842769 U (Ningbo Jiayin Intelligent Tech. Co. Ltd., CN; publ. 2019-12-24) numerous conveyors are arranged in rows, side by side, on a number of levels in a thermally insulated store space. The conveyors are fitted with plates pushing the selected item into a cargo basket which is movable in vertical direction along a vertical column. The latter is movable horizontally on rails and is arranged in front of the conveyors. The basket carries an item from the belt conveyor to the pick-up window where it can be taken out by the buyer. The store space is separated from the pick-up window by a thermo-insulating wall preventing leakage of chilled air.
A pre-orderable vending machine that includes main cabinet, storage compartment, a push frame, a lift push table, and a storage tray is proposed in Chinese utility model application CN206460556 U (Yan Fuying, CN; publ. 2017-09-01). The board of the machine is divided into upper and lower layers, each layer of the main cabinet is provided with brackets. The bracket is provided with a number of slide rails, a rotating shaft, a receiving plate, and a motor on one side of the bracket. The main cabinet is provided with a number of glass doors. Its right side is connected with the auxiliary cabinet which is provided with a number of speakers and a pick-up port, and is also provided with a number of lifting and pushing platforms.
Still another Chinese utility model application CN210466543 U (Yibao International Tech Beijing Co. Ltd., CN; publ. 2020-05-05) discloses a vending machine which comprises a main machine frame and a thermo-insulated goods storage cabinet. This cabinet comprises a plurality of goods channels extending from the rear to the front of the cabinet. Pushing devices are arranged in the goods channels. Each pushing device comprises a screw which is rotatably arranged on the partition plate along the channel, and a power device which drives the screw. A pushing element cooperating with the screw and slidably mounted on the partition plate is used for pushing the goods to the place of receipt of goods.
Japanese patent document JPH02163896 A (Fuji Elecric Co. Ltd., JP; publ. 1990-06-25) describes a vending appliance which is equipped with the endless belt conveyors. Tension is applied to the belt with horizontal rollers. A driving device is connected to at least one of the rollers. Plural locking parts are formed on the surface of the belt on which the commodities are to be placed. Alternatively, the auger conveyors are installed in the machine. The selected product is carried down from the conveyor to the pick-up place either on a chute or on a transporting basket.
If shopping procedure is realized according to a pre-set shopping list the selected items may be stacked one by one in the basked which is moved from one conveyor to another and finally delivered into the dispensing chamber or drawer. Such a solution has been adopted in the proposed invention but the basket has been modified to enable shopping of large quantities whose total volume may overpass that of the basket itself. The invented basket is suitable for both small requests of one or a few items, and large shopping of dozens of commodities.
To the best knowledge of the inventors, to date there have not been proposed any solution where dispensing of requested items according to previously compiled shopping list could be invalidated by the buyer during delivering of subsequent products into the shopping basket if the payment was confirmed. The only reported solutions describe annulation of single-item purchases.
For example according to British patent GB695867 A (Communication Engineering PTY Ltd., AU; publ. 1953-08-19) a deposit must be inserted in a vending machine before articles for purchase may be selected. The selected articles are delivered only when further money is inserted to bring the total amount inserted up to the total price of the articles. An order is cancelled and the money inserted, less the deposit, returned when a refund button is pressed. The deposit is also returned if the total price of any articles selected does not exceed it, or if the means for collecting the deposit has been made ineffective by a control preset by the proprietor. Should the customer wish to cancel his order he presses a button connected mechanically to return the inserted coins less the deposit if it has already been discharged.
In a vending machine described in another British patent GB1086127 A (Omron Tateisi Electronics Co., JP; publ. 1967-10-04) pressing of a "cancel" push-button after insertion of money but before pressing any other button causes refund.
The proposed vending machine significantly changes this state of play through enabling the purchaser to cancel buying even if all selected items have been all delivered into the dispensing drawer but still not withdrawn from there. The proposed solution makes buying in the vending machine more alike making shopping in a regular store where the customer may change his decision before, during, and even after payment. Thus the proposed device is more customer-friendly.
A vending machine according to the invention comprises a store space, a confectioning zone, a shopping basket, an issuing chamber, and a control unit. At least the store space and the confectioning zone are situated in a housing which is preferably maid of thermo-insulating composite panels. Other components may be located outside the thermostatic housing.
The store space may be divided into two sectors: first store space and second store space located on opposite sides of the confectioning zone. In exemplary embodiment first store space is equipped with the belt conveyors while second store space is equipped with the auger conveyors. The term "auger" shall be understood here as a helix made of rigid metal or plastic. The helix pitch and diameter are adjusted to dimensions of the items to be conveyed.
The store space is divided into compartments each having essentially vertical side walls (baffles). At least one compartment has an essentially horizontal belt conveyor consisting of a driving roller ended on one side with a slave gear, an idle roller, an endless belt, and a belt tensioner. Several belt conveyors can be fixed side by side in a common standardized cassette.
According to the invention the belt conveyor is not fitted with its own motor but is set in motion with an external actuator which is mounted on the basket platform described below. This actuator is provided with a master gear meshing with the slave gear of the belt conveyor.
The idea of motorless belt conveyors leads to elimination of dozens or hundreds of motors and their wiring. As a result total cost of the conveyors is significantly reduced, as well as the maintenance costs. Also a risk of failure and total weight of the conveyors are decreased.
The confectioning zone has a movable confectioning unit comprising a frame movable in horizontal direction X along the front side of the store space, and a platform movable on the frame in vertical direction Z in front of the store space.
In a simplified version of the invented vending machine, applicable mainly for large items, the store space may consist of a vertical stack of individual conveyors, one for each level. In this case the frame of the confectioning unit does not move in horizontal direction X and is permanently attached to the machine housing. Only the platform is movable on the frame in vertical direction Z.
As was mentioned above, the platform is equipped with at least one actuator fitted with a master gear capable of meshing with the slave gear mounted on the driving roller of the belt conveyor. This actuator drives the conveyor and is controlled by the control unit. To avoid axial force exerted on the driving roller the double helical gears are recommended for the tandem of the master gear and the slave gear. However, regular toothing of both wheels may be applied too. It is recommended the gears are printed in a 3D printer by additive manufacturing.
The actuator mounted on the platform to drive the conveyor is coupled with the master gear through an endless toothed belt.
Apart from Z-movement, the platform is also movable in horizontal direction Y perpendicular to direction X. The Y-movement towards the front side of the store space enables meshing the master gear with the slave gear to make the belt moving. Reverse Y-movement of the platform releases the meshing which makes the belt still.
The basket for collecting items supplied from the store space is fixed to the platform. The basket may have an openable bottom to release the collected items into an issuing chamber or an issuing drawer.
Also the issuing chamber/drawer may have an openable bottom to release the collected items into the repository in case of cancelled confectioning. Cancellation of confectioning may be requested by the buyer who decided to give up shopping, or may result from unexpected system failure or blocking of goods in the machine.
The movements of the frame in horizontal direction X, and of the platform in directions Y and Z are executed by the X-actuator, Y-actuator, and Z-actuator respectively, which are controlled by the control unit.
In preferred embodiment all actuators are servo motors. Alternatively, the actuators are stepper motors. A combination of servo motors and stepper motors can be used taken specific design of particular components. The X-, Y- and Z-actuators may be fitted with pinions cooperating with racks.
In one variant of the vending machine at least one compartment of the store space is equipped with the auger conveyor. The augers can differ in pitch and diameter as the dimensions of transported items may differ considerably.
According to one embodiment, the auger conveyor is rotated by a built-in motor which is controlled by the control unit, and is wired directly to this unit.
In a recommended embodiment the built-in motor is controlled by the control unit through a connector mounted on the platform. In that case the motor is wired to the connector instead of being wired to the control unit. Only the connector is wired directly to the control unit. This reduces wiring of the machine and makes maintenance cheaper and easier.
The connector is activated when the basket platform gets close to the auger conveyor by its horizontal displacement in direction Y, the same as in the described above turning on/off of the belt conveyor. When the connector is activated the control unit turns on/off the motor of the auger conveyor.
In alternative solution the auger conveyor is motorless. Instead, it is fitted with the slave gear connected to a simple transmission mechanism transmitting torque to the auger. The transmission mechanism may have an endless toothed belt extending from the front to the rear of the auger conveyor. The slave gear is rotated by the actuator mounted on the platform through the master gear in the same manner as described above for the belt conveyor. This may be the same actuator to drive the belt conveyor or the auger conveyor, or the latter may be driven by second actuator mounted on the platform and fitted with its own master gear.
Alike in the case of the motorless belt conveyors, the total price and weight, maintenance time and risk of failure are reduced.
The recommended embodiments of the invention are illustrated on the drawings where:
- Fig. 1 shows schematic top view of the vending machine having two separate store spaces;
- Fig. 2 shows schematic top view of the machine having one combined store space;
- Fig. 3 shows the embodiment from Fig. 1 in more detail;
- Fig. 4 shows the confectioning unit comprising vertical frame movable horizontally along top and bottom rails fixed to the housing in the confectioning zone;
- Fig. 5 shows a cassette comprising the belt conveyors;
- Fig. 6 shows the basket having openable bottom and the mechanism driving the conveyor;
- Fig. 7 shows the basket from Fig. 6 in another view;
- Fig. 8 shows the issuing chamber with opened pick-up door;
- Fig. 9 shows the side view of the issuing chamber fitted with openable bottom;
- Fig. 10 shows the basket on the platform in front of the store space consisting of the auger conveyors and a row of the belt conveyors at the bottom;
- Fig. 11 shows the platform with the basket and the connector pushed against the auger conveyor;
- Fig. 12 shows the platform with the basket and the meshing mechanism pushed against the belt conveyor;
- Fig. 13 shows details of the belt conveyor and its belt tensioner;
- Fig. 14 shows details of the torque transmission mechanism from the actuator to the belt driving roller.; and
- Fig. 15 shows details of the torque transmission mechanism from the actuator to the auger conveyor.
According to the preferred embodiment a vending machine comprises a store space (1), a confectioning zone (2), a shopping basket (3), an issuing chamber (4), and a control unit (5). The store space (1) is divided into compartments (10) each having essentially vertical side walls (11), wherein at least one compartment (10) has an essentially horizontal belt conveyor (12) consisting of a driving roller (13) ended with a slave gear (14), an idle roller (15), an endless belt (16) and a belt tensioner (17).
The store space (1) and the confectioning zone (2) are enclosed in a thermo-insulating and thermostatic housing (6). In one realization of the vending machine the store space (1) consists of first store space (1A) and second store space (1B) located on opposite sides of the confectioning zone (2). Fig. 3 illustrates the embodiment where both first and second store spaces have the belt conveyors and the auger conveyors. However, first store space (1A) may be equipped with the belt conveyors (12) only while second store space (1B) may be equipped entirely with the auger conveyors (18).
The confectioning zone (2) has a movable confectioning unit (20) comprising a frame (21) movable in horizontal direction X along the front side of the store space (1), and a platform (22) movable on the frame (21) in vertical direction Z in front of the store space (1). The frame (21) may have two vertical rails as shown in Fig. 4. In case of bigger vending machines dedicated for selling large numbers of items, especially heavy commodities, the frame may have four or more pillars moving on two or more horizontal rails. Such a solution reduces the moment of power exerted by the basket platform upon vertical rails.
The platform (22) is equipped with at least one actuator (23) fitted with a master gear (24) capable of meshing with the slave gear (14). The actuator (23) is controlled by the control unit (5). The platform (22) is movable in horizontal direction Y perpendicular to direction X towards the front side of the store space (1) to mesh the master gear (24) with the slave gear (14) and back to release the meshing. The basket (3) for collecting items supplied from the store space (1) is fixed on the platform (22).
The movements of the frame (21) in horizontal direction X, and of the platform (22) in directions Y and Z are executed by the X-actuator (25), Y-actuator (26), and Z-actuator (27) respectively, controlled by the control unit (5).
The actuator (23) is coupled with the master gear (24) through an endless toothed belt (29). The master gear (24) and the slave gear (14) are double helical gears.
The actuators (23, 25, 26, 27) are servo motors. In alternative embodiment, the actuators (23, 25, 26, 27) are stepper motors. The actuators (25, 26, 27) may be fitted with pinions cooperating with racks.
At least one compartment (10) is equipped with an auger conveyor (18) which is rotated by a built-in motor (19) controlled by and wired directly to the control unit (5).
In the improved embodiment the auger conveyor (18) is rotated by the built-in motor (19) controlled by the control unit (5) through a connector (28) mounted on the platform (22). The motor (19) is wired directly to said connector (28).
In another embodiment the auger conveyor (18) is rotated by the actuator (23) mounted on the platform (22) through the master gear (24) and the slave gear (14) connected to a transmission mechanism of the auger conveyor (18). The transmission mechanism has an endless toothed belt (29) extending along the auger and driving its rear end through additional gears.
The basket (3) has an openable bottom (31) to release the collected items into the issuing chamber (4). The issuing chamber (4) may have an openable bottom (41) to release the collected items into the repository in case of cancelled confectioning.

List of references
1
store space
1A
first store space
1B
second store space
10
compartment
11
side wall of the compartment / baffle between compartments
12
belt conveyor
13
driving roller
14
slave gear
15
idle roller
16
endless belt
17
belt tensioner
18
auger conveyor
19
motor of the auger conveyor
2
confectioning zone
20
confectioning unit
21
frame
22
platform
23
actuator for the belt/auger conveyor
24
master gear
25
X-actuator
26
Y-actuator
27
Z-actuator
28
connector
29
toothed belt
3
basket
31
openable bottom of the basket
4
issuing chamber
41
openable bottom of the issuing chamber
5
control unit
6
housing
1. A vending machine comprising a store space (1), a confectioning zone (2), a shopping basket (3), an issuing chamber (4), and a control unit (5), characterized in that the store space (1) is divided into compartments (10) each having essentially vertical side walls (11), wherein at least one compartment (10) has an essentially horizontal belt conveyor (12) consisting of a driving roller (13) ended with a slave gear (14), an idle roller (15), an endless belt (16) and a belt tensioner (17), and in that the confectioning zone (2) has a movable confectioning unit (20) comprising a frame (21) movable in horizontal direction X along the front side of the store space (1), and a platform (22) movable on the frame (21) in vertical direction Z in front of the store space (1), wherein the platform (22) is equipped with at least one actuator (23) fitted with a master gear (24) capable of meshing with the slave gear (14), the actuator (23) being controlled by the control unit (5), and in that the platform (22) is movable in horizontal direction Y perpendicular to direction X towards the front side of the store space (1) to mesh the master gear (24) with the slave gear (14) and back to release the meshing, and in that the basket (3) for collecting items supplied from the store space (1) is fixed on the platform (22), and in that the movements of the frame (21) in horizontal direction X, and of the platform (22) in directions Y and Z are executed by the X-actuator (25), Y-actuator (26), and Z-actuator (27) respectively, controlled by the control unit (5).
2. The vending machine according to claim 1, characterized in that the master gear (24) and the slave gear (14) are double helical gears.
3. The vending machine according to claim 1 or 2, characterized in that the actuator (23) is coupled with the master gear (24) through an endless toothed belt (29).
4. The vending machine according to any of claims 1 to 3, characterized in that the actuators (23, 25, 26, 27) are servo motors.
5. The vending machine according to any of claims 1 to 3, characterized in that the actuators (23, 25, 26, 27) are stepper motors.
6. The vending machine according to any of preceding claims, characterized in that the actuators (25, 26, 27) are fitted with pinions cooperating with racks.
7. The vending machine according to any of preceding claims, characterized in that at least one compartment (10) is equipped with an auger conveyor (18).
8. The vending machine according to claim 7, characterized in that the auger conveyor (18) is rotated by a built-in motor (19) controlled by and wired directly to the control unit (5).
9. The vending machine according to claim 7, characterized in that the auger conveyor (18) is rotated by a built-in motor (19) controlled by the control unit (5) through a connector (28) mounted on the platform (22), and in that the motor (19) is wired to the connector (28).
10. The vending machine according to claim 7, characterized in that the auger conveyor (18) is rotated by the actuator (23) mounted on the platform (22) through the master gear (24) and the slave gear (14) connected to a transmission mechanism of the auger conveyor (18), preferably comprising an endless toothed belt (29).
11. The vending machine according to any of preceding claims, characterized in that the basket (3) has an openable bottom (31) to release the collected items into the issuing chamber (4).
12. The vending machine according to any of preceding claims, characterized in that the issuing chamber (4) has an openable bottom (41) to release the collected items into the repository in case of cancelled confectioning.
13. The vending machine according to any of preceding claims, characterized in that the store space (1) consists of first store space (1A) and second store space (1B) located on opposite sides of the confectioning zone (2).
14. The vending machine according to claim 13, characterized in that first store space (1A) is equipped with the belt conveyors (12) while second store space (1B) is equipped with the auger conveyors (18).
15. The vending machine according to any of preceding claims, characterized in that at least the store space (1) and the confectioning zone (2) are enclosed in a thermostatic housing (6).
0222/EP/03/22
EP
22460019.7
Delfin Spolka z o.o. Spolka Komandytowa
3
MN
20220912
G07F
US
2020334940
A1
LIU KAI [CN] ET AL
20201022
X
1-15
* the whole document *
US
2020043272
A1
VAZQUEZ DIEGO [US] ET AL
20200206
A
1-15
* paragraphs [0033] - [0036] *
Verhoef, Peter
Munich
20220901
US
2020334940
A1
20201022
CN
109993903
A
20190709
US
2020334940
A1
20201022
WO
2019128337
A1
20190704
US
2020043272
A1
20200206
US
2020043272
A1
20200206
WO
2020028876
A1
20200206

REFERENCES CITED IN THE DESCRIPTION
This list of references cited by the applicant is for the reader's convenience only. It does not form part of the European patent document. Even though great care has been taken in compiling the references, errors or omissions cannot be excluded and the EPO disclaims all liability in this regard.

Patent documents cited in the description
- CN
210377657
U
20200421
[0005]
- CN
209842769
U
20191224
[0006]
- CN
206460556
U
20170901
[0007]
- CN
210466543
U
20200505
[0008]
- JP
H02163896
A
19900625
[0009]
- GB
695867
A
19530819
[0012]
- GB
1086127
A
19671004
[0013]