ATBECHDEDKESFRGBGRITLILUNLSEMCPTIESILTLVFIROMKCYALTRBGCZEEHUPLSKBAHRISYU........
J
DIM360 (Ver 1.5 21 Nov 2005) - 1100000/0
1772388
EUROPEAN PATENT APPLICATION
A1
20070411
EP
06398007.2
20060424
en
en
en
1007705 U
20051007
PT
20070411
200715
20070411
200715
B65D 5/54 20060101AFI20070125BHEP
B65D 71/00 20060101ALI20070125BHEP
de
Bandähnliche Verpackung
en
Band-like package
fr
Emballage du type bande
2
Graphicsleader Packging S.A.
07417950
2006-0844.EP 04
Rua Dos Moleiros
4416-801 Grijo
PT
Peres, Carlos Besse
Cabeço de Montachique Lousa
2670-141 LOURES
PT
Pereira da Cruz, Joao
00071781
J. Pereira da Cruz, S.A. Rua Vitor Cordon, 14
1249-103 Lisboa
PT
AT
BE
BG
CH
CY
CZ
DE
DK
EE
ES
FI
FR
GB
GR
HU
IE
IS
IT
LI
LT
LU
LV
MC
NL
PL
PT
RO
SE
SI
SK
TR
AL
BA
HR
MK
YU
The present invention concerns a band-like package, in cardboard, planiform, the mounting of which is performed by means of predefined folding lines. It is characterised in that it may be formed by only two side walls 8, one bottom 7 and one upper part or lid formed by two parts 18 and 19 and a central strip 20 which may be torn off through punched lines 22 and 23.

Scope of the invention
The present invention concerns a band-like package, in cardboard, essentially designed for the food industry, more particularly for refrigerated milk products as, for instance, yogurts, and which is appropriate for use in sales points, such as those normally present in supermarket shelves. It is essentially characterised in that it does not fully wrap the products to be packed and in that it is provided with opening means by tearing off a strip provided in the centre of the package's upper portion.

Prior art
A number of packages for food products or else, among which should be mentioned those that are the object of patents EP 0997380 and EP 0780311, are well known.
Patent EP 0997380 concerns one box with four side walls. Two of these respective walls are provided with first closing flaps and the other two respective walls are provided with second closing flaps. The second flaps, which edges are to be joined, cover the first flaps and, over the joints, are to be applied some adhesive bands, which may be stripped off, in order to secure the package closure. The side walls including the first flaps are provided with some punched lines. These flaps do also display opening means formed by a cutting line.
Patent EP 0780311 concerns a container, particularly a box in corrugated cardboard proper to house packs of commercial items, having rigid walls provided with an enclosing portion that are kept closed by means of sticking tape applied to the container. At least one wall of the container is provided with a cutting bore or a tab that may be removed and which is defined by cutting lines and/or weakened lines on the wall, the said bore or the said tab being provided under a portion of the sticking tape edge.
None of the previously mentioned documents display the characteristics of the package defined in claim 1.
The band-like package that is the object of the invention presents at least two advantages when compared with the currently known packages in the field of the industry in question. Such advantages are the following:
- It has an innovative lid, easy to open by tearing it off.
- Its design employs a lower amount of cardboard, which allows for the interconnection of the card packages on the printing/production sheet. This characteristic affords less card waste and a greater number of card packages per card sheet during production. Therefore, the manufacture of this card package is cheaper than the packages produced according to the standards of the package production industry.

Brief description of the drawings
In the attached drawings, which should not be construed as having a limiting character, the following is depicted:
- Figure 1 displays a planiform package of one embodiment of the invention;
- Figure 2 displays the package of Figure 1 duly mounted and showing the strip being torn off;
- Figure 3 displays one package of a second embodiment, duly mounted and showing the strip being torn off; and
- Figure 4 displays a series of planiform packages.

Detailed description of the invention
As it may be observed in the figures, the package that is the object of the invention 1, 2, is planiform displayed with parts 3, 4 and 5, 6 forming, respectively, the bottom 7 of the package 1 and the side walls 8. Each of these parts is separated from the remaining ones by means of folding lines, respectively 9, 10, 11 and 12, formerly grooved during the manufacturing process of the said packages. Part 5 is further provided with a small flap 13, which is fixed to the flap on the opposite side 3 by means of glue or any other suitable process to form the bottom 7 of package 1. Between parts 3 and 4 and 5 and 6, substantially trapezoidal small tabs 14 and 15 are made during manufacture, with previously grooved folding lines 16 and 17, which, when pressed inwards, shall allow them to assume an extending position towards the inside of the package, as it may be observed in figures 3 and 4.
Package 1, which is the object of this invention, is further formed by parts 18, 19 and 20 which compose the package upper part and may be called lid because access to the packed products 21 is provided thereby. Part 20, which forms a strip along the length of package 1, is attached to parts 18 and 19 by means of punched lines 22 and 23, which punches facilitate the tearing off of part, or strip, 20.
As it is obvious, the mounting of the package is made by means of folding lines 9, 10, 11 and 12 and by gluing flap 13 to the opposite part 3. It is preferred that the products to be packed, more particularly yogurts, are previously positioned before the package is duly mounted. As soon as the package is mounted, folding lines 16 and 17 are pressed so that the trapezoidal tabs assume an extending position towards the inside of the package in order to serve as a brake to prevent the yogurts from sliding.
This kind of package is supplied planiform, the mounting of which being performed later on by the food products distributor after such products are placed in suitable position.
In order to provide full access to the package insides and enable the withdrawal of the yogurts, removal of strip 20 is performed, as already mentioned, by tearing it off. Therefor, it shall be enough to engage the end portion of strip 20 and raise it. Punched lines 22 and 23 shall give in and, as if they were a zip, they shall successively separate from parts 18 and 19 which compose the package lid.
The geometrical characteristics of this package, namely the curved edges of strip 20, shall make it easy for the user, when tearing off the said strip, to easily engage the strip's edge and, thereafter, proceed to the removal thereof. The remaining geometrical characteristics condition a parallelepiped form of the package after it is mounted.
As the experts in the art will find obvious, there is no limit regarding the package's dimensions. It may be redesigned to contain a set of 4 yogurt cups, a set of 8 yogurt cups or a set of 16 yogurt cups. These are the standard amounts for the sets of yogurt cups in the field of the yogurt production industry when these are displayed for sale conditioned in cardboard packages.
As it may be seen in Figure 4, the packages may be arranged in a single sheet and, then, be cut to provide individual items. Such a procedure yields less cardboard waste and more cardboard packages per cardboard sheet during common printing and production.
1. Band-like package, in cardboard, planiform, the mounting of which is performed through predefined folding lines, characterised in that it is formed by only two side walls 8, one bottom 7 and one upper part or lid formed by two parts 18 and 19 and a central strip 20, which is removable.
2. Band-like package, according to the preceding claim, characterised in that the said central strip 20 is attached to the said parts 18 and 19 by means of punched lines 22 and 23, which facilitate the tearing off of the part or strip 20, thereby providing full access to the packed products.
3. Band-like package, according to the preceding claims, characterised in that strip 20 is extended along the full length of package 1.
4. Band-like package, according to the preceding claims, characterised in that substantially trapezoidal small tabs 14 and 15 are provided, with folding lines 16 and 17 previously grooved in the area of folding lines 9 and 11 of the parts that shall form the bottom 7 and the side walls 8, which, when pressed inwards, shall allow them to assume an extending position towards the inside of the package.
5. Band-like package, according to the preceding claims, characterised in that it is provided planiform and the mounting of which is to be made after the products to be packed are suitably positioned. Then, the trapezoidal tabs 16 and 17 are pressed in so that they assume an inward extending position to serve as a brake to prevent the packed products from sliding.
6. Band-like package, according to the preceding claims, characterised in that it may be manufactured together with other packages in a single cardboard sheet.

REFERENCES CITED IN THE DESCRIPTION
This list of references cited by the applicant is for the reader's convenience only. It does not form part of the European patent document. Even though great care has been taken in compiling the references, errors or omissions cannot be excluded and the EPO disclaims all liability in this regard.

Patent documents cited in the description
- EP
0997380
A
[0002]
[0003]
- EP
0780311
A
[0002]
[0004]